<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.831" y2="0" width="0" layer="20"/>
<wire x1="17.831" y1="0" x2="17.831" y2="20.31" width="0" layer="20"/>
<wire x1="17.831" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>P0.01</text>
<text>P0.02</text>
<text>P0.03</text>
<text>P0.04</text>
<text>P0.09</text>
<text>P0.10</text>
<text>P0.13</text>
<text>DIO</text>
<text>DCLK</text>
<text>GND</text>
<text>nRF51822-04</text>
</plain>
<libraries>
<library name="djabi">
<packages>
<package name="H6-2.54">
<description>Mail Header 8p. &lt;br&gt;
Copy from speed-OPL-connector.lbr</description>
</package>
<package name="NRF51822-04AT">
<description>&lt;a href="http://www.wireless-tag.com/Public/upload/file/p19pme9j3f19lh375j7216b98m63.pdf"&gt;nRF51822-04AT&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="djabi" package="H6-2.54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="djabi" package="H6-2.54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="djabi" package="NRF51822-04AT" value="NRF51822"/>
</elements>
<signals>
<signal name="P1/VCC">
<contactref element="U$1" pad="P1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="P2/GND">
<contactref element="U$1" pad="P2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="P3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P7"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P8"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P9"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P10"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P11"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="P13/GND">
<contactref element="U$1" pad="P12"/>
<contactref element="J2" pad="6"/>
<contactref element="U$1" pad="P13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
