<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="3.92130625" y1="8.160971875" x2="19.36008125" y2="8.17578125" width="0" layer="20"/>
<wire x1="19.36008125" y1="8.17578125" x2="19.36008125" y2="32.465221875" width="0" layer="20"/>
<wire x1="19.36008125" y1="32.465221875" x2="3.92130625" y2="32.4504125" width="0" layer="20"/>
<wire x1="3.92130625" y1="32.4504125" x2="3.92130625" y2="8.160971875" width="0" layer="20"/>
<text>VCC
3V</text>
<text>GND</text>
<text>CS</text>
<text>RESET</text>
<text>DC/
RS</text>
<text>SDI/
MOSI</text>
<text>SCK</text>
<text>LED</text>
<text>SDO/
MISO</text>
<text>FUSEDCREATIONS.COM</text>
<text>ILI9341 INTERFACE BOARD</text>
<text>VCC
3V</text>
<text>GND</text>
<text>CS</text>
<text>RESET</text>
<text>DC/
RS</text>
<text>SDI/
MOSI</text>
<text>SCK</text>
<text>LED</text>
<text>SDO/
&lt;OSP</text>
<text>FUSEDCREATIONS.COM</text>
<text>TFT_GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="TFT18PIN">
<description>TFT ribbon connector with 18 pads
14 pads for the screen and 4 for the touch controller</description>
<packages>
<package name="TFT_18PIN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X09" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10">
<attribute name="PROD_ID" value="RES-12180"/>
</element>
<element name="U$4" library="TFT18PIN" package="TFT_18PIN" value="TFT_18PIN"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$4" pad="TFT_GND"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="TFT_RESET">
<contactref element="U$4" pad="TFT_RESET"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="TFT_SCK">
<contactref element="U$4" pad="TFT_SCK"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="TFT_RS">
<contactref element="U$4" pad="TFT_RS"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="TFT_CS">
<contactref element="U$4" pad="TFT_CS"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="TFT_SDI">
<contactref element="U$4" pad="TFT_SDI"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="TFT_SDO">
<contactref element="U$4" pad="TFT_SDO"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="VCC3V">
<contactref element="U$4" pad="VIN3V"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="TFT_LED">
<contactref element="J1" pad="8"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$4" pad="LED"/>
<contactref element="R1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
