<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<text>ThingySticks.com</text>
<text>FETs</text>
<wire x1="20.5" y1="33" x2="110" y2="33" width="0" layer="20"/>
<wire x1="110" y1="33" x2="114" y2="29" width="0" layer="20" curve="-90"/>
<wire x1="114" y1="29" x2="114" y2="-3" width="0" layer="20"/>
<wire x1="114" y1="-3" x2="110" y2="-7" width="0" layer="20" curve="-90"/>
<wire x1="110" y1="-7" x2="19" y2="-7" width="0" layer="20"/>
<wire x1="19" y1="-7" x2="15" y2="-3.5" width="0" layer="20" curve="-90"/>
<wire x1="15" y1="-3.5" x2="15" y2="28" width="0" layer="20"/>
<wire x1="15" y1="28" x2="20.5" y2="33" width="0" layer="20" curve="-90"/>
<text>V1.1</text>
<text>GND</text>
<text>24V DC
10A Max</text>
<text>4 N-Channel FETs</text>
<text>Low Voltage DC ONLY.</text>
<text>S.Harrison</text>
<text>2 Dec 2016</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>G</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-SMT-MALE">
</package>
<package name="SCREWTERMINAL-3.5MM-5">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="Tinamous">
<packages>
<package name="ELECTRON_SIMPLE_SILK_NAMES_DUAL">
<description>Electron socket for a dual-row header for easy prototyping, with the pins also duplicated to unpopulated through-holes for easy soldering.</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="DPAK">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206-BOTTOM">
</package>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CONN1" library="SparkFun-Connectors" package="USB-A-SMT-MALE" value="USBA-SMD-MALE"/>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-5" value="">
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="Combine 8288+8399"/>
</element>
<element name="H1" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="U2" library="Tinamous" package="ELECTRON_SIMPLE_SILK_NAMES_DUAL" value="ELECTRONDUALNAMED"/>
<element name="D6" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="DPAK" value="FDD8780 or FDD8451">
<attribute name="PROD_ID" value="TRANS-09984"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10R">
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="DPAK" value="FDD8780 or FDD8451">
<attribute name="PROD_ID" value="TRANS-09984"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10R">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-1206-BOTTOM" value=""/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="R13" library="SparkFun-Resistors" package="0805" value="1k5">
<attribute name="NAME"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1k5">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1k5">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ6" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ7" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ8" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="DPAK" value="FDD8780 or FDD8451">
<attribute name="PROD_ID" value="TRANS-09984"/>
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="10R">
<attribute name="NAME"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="1k5">
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="DPAK" value="FDD8780 or FDD8451">
<attribute name="PROD_ID" value="TRANS-09984"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="10R">
<attribute name="NAME"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1k5">
<attribute name="NAME"/>
</element>
<element name="H3" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H4" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
</elements>
<signals>
<signal name="GND">
<contactref element="CONN1" pad="GND1"/>
<contactref element="U2" pad="GND_1B"/>
<contactref element="U2" pad="GND@2"/>
<contactref element="U2" pad="GND_1"/>
<contactref element="U2" pad="GND"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="D5" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="R10" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="D4" pad="C"/>
<contactref element="R7" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="D3" pad="C"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$17">
</signal>
<signal name="N$9">
</signal>
<signal name="N$8">
</signal>
<signal name="N$10">
</signal>
<signal name="5V">
<contactref element="U2" pad="VIN"/>
<contactref element="U2" pad="VIN_1B"/>
<contactref element="C3" pad="2"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$32">
</signal>
<signal name="N$34">
</signal>
<signal name="3.3V">
<contactref element="U2" pad="3V3"/>
<contactref element="U2" pad="3V3_1"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$18">
</signal>
<signal name="N$6">
<contactref element="U2" pad="VBATT_1"/>
<contactref element="U2" pad="VBAT"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="RST"/>
<contactref element="U2" pad="RST_1"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="D6_1"/>
<contactref element="U2" pad="D6"/>
</signal>
<signal name="N$16">
<contactref element="U2" pad="D5"/>
<contactref element="U2" pad="D5_1"/>
</signal>
<signal name="N$20">
<contactref element="U2" pad="D4_1"/>
<contactref element="U2" pad="D4"/>
</signal>
<signal name="N$23">
<contactref element="U2" pad="C5_1"/>
<contactref element="U2" pad="C5"/>
</signal>
<signal name="N$24">
<contactref element="U2" pad="C4"/>
<contactref element="U2" pad="C4_1"/>
</signal>
<signal name="N$25">
<contactref element="U2" pad="C3"/>
<contactref element="U2" pad="C3_1"/>
</signal>
<signal name="N$26">
<contactref element="U2" pad="C2"/>
<contactref element="U2" pad="C2_1"/>
</signal>
<signal name="N$28">
<contactref element="U2" pad="C1"/>
<contactref element="U2" pad="C1_1"/>
</signal>
<signal name="N$29">
<contactref element="U2" pad="C0"/>
<contactref element="U2" pad="C0_1"/>
</signal>
<signal name="N$31">
<contactref element="U2" pad="B0"/>
<contactref element="U2" pad="B0_1"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="U2" pad="B1"/>
<contactref element="U2" pad="B1_1"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="U2" pad="B2_1"/>
<contactref element="U2" pad="B2"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="U2" pad="B3"/>
<contactref element="U2" pad="B3_1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="U2" pad="B4_1"/>
<contactref element="U2" pad="B4"/>
</signal>
<signal name="N$38">
<contactref element="U2" pad="B5_1"/>
<contactref element="U2" pad="B5"/>
</signal>
<signal name="N$39">
<contactref element="U2" pad="A0_1"/>
<contactref element="U2" pad="A0"/>
</signal>
<signal name="N$40">
<contactref element="U2" pad="A1"/>
<contactref element="U2" pad="A1_1"/>
</signal>
<signal name="N$41">
<contactref element="U2" pad="A2"/>
<contactref element="U2" pad="A2_1"/>
</signal>
<signal name="N$42">
<contactref element="U2" pad="A3"/>
<contactref element="U2" pad="A3_1"/>
<contactref element="SJ7" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="U2" pad="A5"/>
<contactref element="U2" pad="A5_1"/>
</signal>
<signal name="N$45">
<contactref element="U2" pad="DAC_1"/>
<contactref element="U2" pad="DAC"/>
</signal>
<signal name="N$46">
<contactref element="U2" pad="WKP"/>
<contactref element="U2" pad="WKP_1"/>
</signal>
<signal name="N$47">
<contactref element="U2" pad="RX_1"/>
<contactref element="U2" pad="RX"/>
</signal>
<signal name="N$48">
<contactref element="U2" pad="TX_1"/>
<contactref element="U2" pad="TX"/>
</signal>
<signal name="N$1">
<contactref element="CONN1" pad="VBUS1"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="SDA">
<contactref element="U2" pad="D0_1"/>
<contactref element="U2" pad="D0"/>
</signal>
<signal name="SCL">
<contactref element="U2" pad="D1_1"/>
<contactref element="U2" pad="D1"/>
</signal>
<signal name="BIG_FET_1">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="SJ5" pad="2"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$105">
<contactref element="R5" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="BIG_FET_1_RETURN">
<contactref element="Q1" pad="4"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="BIG_FET_2_RETURN">
<contactref element="Q2" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="BIG_FET_2">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="SJ8" pad="1"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="D7">
<contactref element="R13" pad="1"/>
<contactref element="U2" pad="D7_1"/>
<contactref element="U2" pad="D7"/>
</signal>
<signal name="N$19">
<contactref element="D5" pad="A"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="D1" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="D2" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q4" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="D4" pad="A"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="Q3" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="D3" pad="A"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="BIG_FET_3_RETURN">
<contactref element="Q3" pad="4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="BIG_FET_4_RETURN">
<contactref element="Q4" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="BIG_FET_4">
<contactref element="R12" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="SJ7" pad="1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="BIG_FET_3">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ6" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="SJ8" pad="2"/>
<contactref element="U2" pad="A4"/>
<contactref element="U2" pad="A4_1"/>
</signal>
<signal name="N$43">
<contactref element="SJ6" pad="1"/>
<contactref element="U2" pad="D3"/>
<contactref element="U2" pad="D3_1"/>
</signal>
<signal name="N$49">
<contactref element="U2" pad="D2"/>
<contactref element="U2" pad="D2_1"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="N$50">
</signal>
</signals>
</board>
</drawing>
</eagle>
