<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="50.8" width="0.1524" layer="20"/>
<wire x1="0" y1="50.8" x2="76.2" y2="50.8" width="0.1524" layer="20"/>
<wire x1="76.2" y1="50.8" x2="76.2" y2="0" width="0.1524" layer="20"/>
<wire x1="76.2" y1="0" x2="0" y2="0" width="0.1524" layer="20"/>
<text>PB0</text>
<text>GND</text>
<text>PB1</text>
<text>PB3</text>
<text>VCC</text>
<text>PB2</text>
<text>3 in</text>
<text>2 in</text>
<text>0.25"</text>
<text>0.25"</text>
<text>0.25"</text>
<text>0.25"</text>
<text>Pulse Generator Board Tester</text>
<text>Rev. 1</text>
<text>MISO</text>
<text>SCK</text>
<text>RST</text>
<text>5V</text>
<text>MOSI</text>
<text>GND</text>
<text>ATtiny10 Board</text>
<text>Programmer</text>
<text>MOSI</text>
<text>SCK</text>
<text>RESET</text>
<text>5V</text>
<text>Programmer Connected</text>
<text>Disconnected</text>
<text>VCC Select</text>
<text>Programmer</text>
<text>External</text>
<text>Direct</text>
<text>External Power Select</text>
<text>Through Ammeter</text>
<text>VEXT+</text>
<text>VEXT-</text>
<text>AMM+</text>
<text>AMM-</text>
<text>Start (PB0)</text>
<text>Reset (PB3)</text>
<text>PB0</text>
<text>GND</text>
<text>PB1</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>PB3</text>
<text>VCC</text>
<text>PB2</text>
<text>PB0</text>
<text>PB1</text>
<text>PB2</text>
<text>DIP Mount</text>
<text>ATtiny10
Board</text>
<wire x1="34.925" y1="23.495" x2="34.925" y2="17.145" width="0.1524" layer="20"/>
<wire x1="34.925" y1="17.145" x2="36.83" y2="17.145" width="0.1524" layer="20"/>
<wire x1="36.83" y1="17.145" x2="36.83" y2="11.43" width="0.1524" layer="20"/>
<wire x1="36.83" y1="11.43" x2="39.37" y2="11.43" width="0.1524" layer="20"/>
<wire x1="39.37" y1="11.43" x2="39.37" y2="17.145" width="0.1524" layer="20"/>
<wire x1="39.37" y1="17.145" x2="41.275" y2="17.145" width="0.1524" layer="20"/>
<wire x1="41.275" y1="17.145" x2="41.275" y2="23.495" width="0.1524" layer="20"/>
<wire x1="41.275" y1="23.495" x2="34.925" y2="23.495" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="special-drill">
<description>&lt;b&gt;Special drills&lt;/b&gt;&lt;p&gt;
For drills bigger as 0.51602 Inch you must draw a circle in Layer 20 Dimension.&lt;br&gt;
See also HELP HOLE,</description>
<packages>
<package name="DRILL_0.2500">
<description>&lt;b&gt;1/4" Marker&lt;/b&gt; 250 thousands of an inch</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH_SPDT_PTH_11.6X4.0MM">
<description>&lt;h3&gt;SPDT PTH Slide Switch&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/P040040c.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-04">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J7" library="SparkFun-Connectors" package="2X3-SHROUDED" value="ATtiny10">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-10681"/>
<attribute name="SF_ID" value="PRT_10877"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="U$6" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="U$7" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="U$8" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="J1" library="SparkFun-Connectors" package="2X3-SHROUDED" value="Programmer">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-10681"/>
<attribute name="SF_ID" value="PRT_10877"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="SWITCH_SPDT_PTH_11.6X4.0MM" value="VCC Select">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-08261"/>
<attribute name="SF_SKU" value="COM-00102"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="special" package="EDG-04" value="Programmer Connection">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun-Switches" package="SWITCH_SPDT_PTH_11.6X4.0MM" value="External Power Select">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-08261"/>
<attribute name="SF_SKU" value="COM-00102"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3" value="External Power">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="VALUE"/>
</element>
<element name="S4" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="ATtiny10 DIP Right">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06" value="ATtiny10 DIP Left">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="J7" pad="4"/>
<contactref element="S1" pad="2"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="GROUND">
<contactref element="J7" pad="3"/>
<contactref element="J1" pad="6"/>
<contactref element="S2" pad="2"/>
<contactref element="S3" pad="1"/>
<contactref element="S4" pad="1"/>
<contactref element="J4" pad="6"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="PB0/MOSI">
<contactref element="J7" pad="1"/>
<contactref element="SW1" pad="3"/>
<contactref element="S3" pad="3"/>
<contactref element="J4" pad="1"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="PB1/SCK">
<contactref element="J7" pad="5"/>
<contactref element="SW1" pad="2"/>
<contactref element="J4" pad="3"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="PB3/RESET">
<contactref element="J7" pad="2"/>
<contactref element="SW1" pad="4"/>
<contactref element="S4" pad="3"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="PB2">
<contactref element="J7" pad="6"/>
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="3"/>
<contactref element="SW1" pad="7"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="5"/>
<contactref element="SW1" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="4"/>
<contactref element="SW1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="SW1" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="VPROG">
<contactref element="J1" pad="2"/>
<contactref element="SW1" pad="8"/>
</signal>
<signal name="VEXT+">
<contactref element="J2" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="VEXT-">
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="5"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="AMM-">
<contactref element="J2" pad="6"/>
<contactref element="S2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
