<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="30.4699625" x2="2.54" y2="6.985" width="0" layer="20"/>
<wire x1="2.54" y1="6.985" x2="3.81" y2="5.715" width="0" layer="20"/>
<wire x1="3.81" y1="5.715" x2="36.83" y2="5.715" width="0" layer="20"/>
<wire x1="36.83" y1="5.715" x2="38.0875" y2="6.9725" width="0" layer="20"/>
<wire x1="38.0875" y1="6.9725" x2="38.0875" y2="30.4824625" width="0" layer="20"/>
<wire x1="38.0875" y1="30.4824625" x2="36.8299625" y2="31.74" width="0" layer="20"/>
<wire x1="36.8299625" y1="31.74" x2="3.8100375" y2="31.74" width="0" layer="20"/>
<wire x1="3.8100375" y1="31.74" x2="2.54" y2="30.4699625" width="0" layer="20"/>
<text>Radio Adapter v1.1</text>
<text>Raspberry Pi GPIO</text>
<text>nRF24L01+ Radio Module</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
</package>
<package name="2X13">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="NRF" library="SparkFun-Connectors" package="2X4" value="M04X2"/>
<element name="PI-GPIO" library="SparkFun-Connectors" package="2X13" value="M13X22X13"/>
</elements>
<signals>
<signal name="3V3">
<contactref element="NRF" pad="2"/>
<contactref element="PI-GPIO" pad="17"/>
</signal>
<signal name="MOSI">
<contactref element="NRF" pad="6"/>
<contactref element="PI-GPIO" pad="19"/>
</signal>
<signal name="MISO">
<contactref element="NRF" pad="7"/>
<contactref element="PI-GPIO" pad="21"/>
</signal>
<signal name="SCK">
<contactref element="NRF" pad="5"/>
<contactref element="PI-GPIO" pad="23"/>
</signal>
<signal name="PIN24">
<contactref element="NRF" pad="3"/>
<contactref element="PI-GPIO" pad="18"/>
</signal>
<signal name="GND">
<contactref element="NRF" pad="1"/>
<contactref element="PI-GPIO" pad="6"/>
<contactref element="PI-GPIO" pad="9"/>
<contactref element="PI-GPIO" pad="25"/>
<contactref element="PI-GPIO" pad="14"/>
<contactref element="PI-GPIO" pad="20"/>
</signal>
<signal name="PIN25">
<contactref element="NRF" pad="8"/>
<contactref element="PI-GPIO" pad="22"/>
</signal>
<signal name="CE0">
<contactref element="NRF" pad="4"/>
<contactref element="PI-GPIO" pad="24"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
