<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0.2032" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="17.78" width="0.2032" layer="20"/>
<wire x1="35.56" y1="17.78" x2="0" y2="17.78" width="0.2032" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="15.24" width="0.2032" layer="20"/>
<wire x1="0" y1="15.24" x2="1.27" y2="13.97" width="0.2032" layer="20" curve="90"/>
<wire x1="1.27" y1="13.97" x2="3.81" y2="13.97" width="0.2032" layer="20"/>
<wire x1="3.81" y1="13.97" x2="6.35" y2="11.43" width="0.2032" layer="20" curve="-90"/>
<wire x1="6.35" y1="11.43" x2="6.35" y2="6.35" width="0.2032" layer="20"/>
<wire x1="6.35" y1="6.35" x2="3.81" y2="3.81" width="0.2032" layer="20" curve="-90"/>
<wire x1="3.81" y1="3.81" x2="1.27" y2="3.81" width="0.2032" layer="20"/>
<wire x1="1.27" y1="3.81" x2="0" y2="2.54" width="0.2032" layer="20" curve="90"/>
<wire x1="0" y1="2.54" x2="0" y2="0" width="0.2032" layer="20"/>
<text>U1</text>
<text>OLED1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -14 Pin No Silk outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="TeensyViewDev">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find graphical displays
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.
</description>
<packages>
<package name="OLED-UG-2832TSWGG01-REAR">
<description>&lt;h3&gt;OLDE display&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 30&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.7mm&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13003"&gt;Microview breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Altimeter">
<packages>
<package name="S25FL256S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X14_NO_SILK" value="DNP"/>
<element name="J2" library="SparkFun-Connectors" package="1X14_NO_SILK" value="DNP"/>
<element name="OLED1" library="TeensyViewDev" package="OLED-UG-2832TSWGG01-REAR" value="32x128 OLED">
<attribute name="PROD_ID" value="LCD-13577"/>
<attribute name="VALUE" value="32x128 OLED"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11624"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-10300"/>
<attribute name="VALUE" value="4.7uF"/>
</element>
<element name="U1" library="Altimeter" package="S25FL256S" value="S25FL256S"/>
<element name="C7" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0402" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0402" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="OLED1" pad="6"/>
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="GND1"/>
<contactref element="U1" pad="GND2"/>
<contactref element="C7" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="OLED1" pad="4"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="OLED1" pad="3"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="OLED1" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="OLED1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="OLED1" pad="13"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="OLED1" pad="14"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="!CS">
<contactref element="OLED1" pad="8"/>
<contactref element="J2" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="!RESET">
<contactref element="OLED1" pad="9"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="D/!C">
<contactref element="OLED1" pad="10"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="SCLK">
<contactref element="OLED1" pad="11"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="SDIN">
<contactref element="OLED1" pad="12"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="OLED1" pad="5"/>
<contactref element="OLED1" pad="7"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="12"/>
<contactref element="U1" pad="VDD"/>
<contactref element="C7" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="13"/>
<contactref element="U1" pad="SI/IO0"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="14"/>
<contactref element="U1" pad="SO/IO1"/>
</signal>
<signal name="SCK">
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="SCK"/>
</signal>
<signal name="N$1">
<contactref element="OLED1" pad="15"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="NOR_CS">
<contactref element="J2" pad="3"/>
<contactref element="U1" pad="CS"/>
<contactref element="J2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
