<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<text>Bottom towards board</text>
<text>2513 Character Gen.
to 2716 EPROM Adapter</text>
<text>github.com/bbenchoff/2513CharGenAdapter</text>
<wire x1="2.286" y1="36.195" x2="29.21" y2="36.195" width="0.0762" layer="20"/>
<wire x1="29.21" y1="36.195" x2="29.21" y2="3.81" width="0.0762" layer="20"/>
<wire x1="29.21" y1="3.81" x2="2.286" y2="3.81" width="0.0762" layer="20"/>
<wire x1="2.286" y1="3.81" x2="2.286" y2="36.195" width="0.0762" layer="20"/>
<wire x1="2.286" y1="36.195" x2="29.21" y2="36.195" width="0.0762" layer="46"/>
<wire x1="29.21" y1="3.81" x2="2.286" y2="3.81" width="0.0762" layer="46"/>
<wire x1="2.286" y1="3.81" x2="2.286" y2="36.195" width="0.0762" layer="46"/>
</plain>
<libraries>
<library name="memory">
<description>&lt;b&gt;Generic Memories&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL24">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="memory">
<description>&lt;b&gt;Generic Memories&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL24">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="2716" library="memory" package="DIL24" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2513" library="memory" package="DIL24" value="2513-CHARACTER">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="2513" pad="24"/>
<contactref element="2716" pad="24"/>
</signal>
<signal name="GND">
<contactref element="2513" pad="10"/>
<contactref element="2716" pad="12"/>
<contactref element="2716" pad="22"/>
<contactref element="2716" pad="19"/>
</signal>
<signal name="A8">
<contactref element="2513" pad="22"/>
<contactref element="2716" pad="23"/>
</signal>
<signal name="A7">
<contactref element="2513" pad="21"/>
<contactref element="2716" pad="1"/>
</signal>
<signal name="A6">
<contactref element="2513" pad="20"/>
<contactref element="2716" pad="2"/>
</signal>
<signal name="A5">
<contactref element="2513" pad="19"/>
<contactref element="2716" pad="3"/>
</signal>
<signal name="A4">
<contactref element="2513" pad="18"/>
<contactref element="2716" pad="4"/>
</signal>
<signal name="A3">
<contactref element="2513" pad="17"/>
<contactref element="2716" pad="5"/>
</signal>
<signal name="A2">
<contactref element="2513" pad="16"/>
<contactref element="2716" pad="6"/>
</signal>
<signal name="A1">
<contactref element="2513" pad="15"/>
<contactref element="2716" pad="7"/>
</signal>
<signal name="A0">
<contactref element="2513" pad="14"/>
<contactref element="2716" pad="8"/>
</signal>
<signal name="D1">
<contactref element="2513" pad="4"/>
<contactref element="2716" pad="9"/>
</signal>
<signal name="D2">
<contactref element="2513" pad="5"/>
<contactref element="2716" pad="10"/>
</signal>
<signal name="D3">
<contactref element="2513" pad="6"/>
<contactref element="2716" pad="11"/>
</signal>
<signal name="D4">
<contactref element="2513" pad="7"/>
<contactref element="2716" pad="13"/>
</signal>
<signal name="D5">
<contactref element="2513" pad="8"/>
<contactref element="2716" pad="14"/>
</signal>
<signal name="!CE">
<contactref element="2716" pad="18"/>
<contactref element="2716" pad="20"/>
<contactref element="2513" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
