<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="7.9375" y1="3.81" x2="7.9375" y2="5.08" width="0" layer="20"/>
<wire x1="6.985" y1="6.0325" x2="1.5875" y2="6.0325" width="0" layer="20"/>
<wire x1="1.5875" y1="6.0325" x2="1.5875" y2="0.635" width="0" layer="20"/>
<text>SOT23
</text>
<wire x1="2.54" y1="-0.3175" x2="3.81" y2="-0.3175" width="0" layer="20"/>
<wire x1="2.54" y1="-0.3175" x2="1.5875" y2="0.635" width="0" layer="20"/>
<wire x1="7.9375" y1="5.08" x2="6.985" y2="6.0325" width="0" layer="20"/>
<wire x1="7.9375" y1="3.81" x2="3.81" y2="-0.3175" width="0" layer="20"/>
</plain>
<libraries>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="ROUND">
<description>&lt;b&gt;Round Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="3" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="2" library="gm-supply" package="ROUND" value=""/>
<element name="1" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="D">
<contactref element="1" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="G">
<contactref element="3" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="S">
<contactref element="Q1" pad="2"/>
<contactref element="2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
