<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.127" y1="-2.54" x2="17.831" y2="-2.54" width="0" layer="20"/>
<wire x1="17.831" y1="-2.54" x2="17.831" y2="41.9" width="0" layer="20"/>
<wire x1="17.831" y1="41.9" x2="-0.127" y2="41.9" width="0" layer="20"/>
<wire x1="-0.127" y1="41.9" x2="-0.127" y2="-2.54" width="0" layer="20"/>
<text>G</text>
<text>S</text>
<text>D</text>
<text>-</text>
<text>+</text>
<text>BURN</text>
<text>johnboiles</text>
<text>Burn
Baby
Burn</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MICRO">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
<library name="Johnboiles">
<description>Custom parts used by John Boiles</description>
<packages>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUINO" library="SparkFun-Boards" package="ARDUINO_PRO_MICRO" value="ARDUINO_PRO_MICRO"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="220"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="10k"/>
<element name="JP1" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value="BURN"/>
<element name="JP2" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value="BATT"/>
<element name="MOSFET" library="Johnboiles" package="TO220" value="IRFZ40HORIZONTAL"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="MOSFET" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="ARDUINO" pad="13"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="P$1"/>
<contactref element="ARDUINO" pad="4"/>
<contactref element="ARDUINO" pad="3"/>
<contactref element="ARDUINO" pad="23"/>
<contactref element="JP2" pad="1"/>
<contactref element="MOSFET" pad="3"/>
</signal>
<signal name="VBATT">
<contactref element="ARDUINO" pad="24"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="MOSFET" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
