<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="20.32" x2="53.01" y2="20.32" width="0" layer="20"/>
<wire x1="53.01" y1="20.32" x2="53.01" y2="80" width="0" layer="20"/>
<wire x1="53.01" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="20.32" width="0" layer="20"/>
<text>ECHO</text>
<text>TRIG</text>
<text>GND</text>
<text>V++</text>
<text>SUPM PUMP WATER LEVEL &amp;</text>
<text>WATER LEAK MONITORING SYS</text>
<text>(RFM69 or WiFi Selectable)</text>
<text>O 433MHz 165mm Ant
O 868MHz 82mm Ant</text>
<text>Arduino Uno Shield v1.0</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>March 2016</text>
<text>V+ SDA SCL GND</text>
<text>TX CHPD RST VCC</text>
<text>GND  GPIO2  GPIO0  RX</text>
<text>GND  OUT  IN</text>
</plain>
<libraries>
<library name="discrete">
<description>Discrete devices (Antenna, Arrrester, Thermistor)</description>
<packages>
<package name="PAD-01">
<description>&lt;b&gt;PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-4">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 4 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
<package name="1X03_LOCK">
</package>
<package name="2X4">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RFM69W-XXXS2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANT" library="discrete" package="PAD-01" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="capacitor-wima" package="C2.5-4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="EXT PWR+">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="HC-SR04 SENSOR">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="I2C-LCD">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X03_LOCK" value="PWR 5TO3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Boards" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="J6" library="SparkFun-Connectors" package="2X4" value="ESP8266-01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X02" value="RFM/ESP SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="LEAK SENSOR">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="R16" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="R17" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Retired" package="TACTILE-PTH" value="RESET">
<attribute name="NAME"/>
</element>
<element name="T1" library="transistor" package="TO92" value="2N3904">
<attribute name="NAME"/>
</element>
<element name="U1" library="SparkFun-RF" package="RFM69W-XXXS2" value="RFM69HW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="BUZZER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="11"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="U1" pad="9"/>
<contactref element="T1" pad="3"/>
<contactref element="R9" pad="P$1"/>
<contactref element="J5" pad="GND@0"/>
<contactref element="J1" pad="1"/>
<contactref element="R11" pad="P$1"/>
<contactref element="C2" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="J4" pad="3"/>
<contactref element="J3" pad="4"/>
<contactref element="J11" pad="2"/>
<contactref element="R16" pad="P$1"/>
<contactref element="J6" pad="7"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J5" pad="D12"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="J5" pad="D10"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="J5" pad="D2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="ANT" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="P$2"/>
<contactref element="T1" pad="1"/>
<contactref element="J5" pad="A2"/>
</signal>
<signal name="VCC">
<contactref element="R4" pad="P$1"/>
<contactref element="J9" pad="2"/>
<contactref element="J5" pad="5V"/>
<contactref element="R13" pad="P$1"/>
<contactref element="R14" pad="P$1"/>
<contactref element="J3" pad="1"/>
<contactref element="J10" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R8" pad="P$2"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="J5" pad="D3"/>
<contactref element="J11" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J5" pad="D11"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="P$1"/>
<contactref element="U1" pad="14"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="J5" pad="D13"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="P$1"/>
<contactref element="U1" pad="12"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="P$2"/>
<contactref element="U1" pad="15"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="J5" pad="A3"/>
<contactref element="R10" pad="P$2"/>
<contactref element="R11" pad="P$2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="J5" pad="D7"/>
<contactref element="R12" pad="P$2"/>
</signal>
<signal name="N$22">
<contactref element="R12" pad="P$1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="J5" pad="RES"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="J1" pad="2"/>
<contactref element="J5" pad="VIN"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="R8" pad="P$1"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="J5" pad="A4"/>
<contactref element="R13" pad="P$2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="J5" pad="A5"/>
<contactref element="R14" pad="P$2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="J5" pad="D4"/>
<contactref element="J10" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J4" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="J6" pad="6"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="J5" pad="D9"/>
<contactref element="R15" pad="P$1"/>
</signal>
<signal name="N$26">
<contactref element="R15" pad="P$2"/>
<contactref element="J6" pad="1"/>
<contactref element="R16" pad="P$2"/>
</signal>
<signal name="N$27">
<contactref element="J5" pad="D8"/>
<contactref element="J6" pad="8"/>
</signal>
<signal name="N$28">
<contactref element="J5" pad="D6"/>
<contactref element="R17" pad="P$1"/>
</signal>
<signal name="N$29">
<contactref element="R17" pad="P$2"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="J5" pad="D5"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="R9" pad="P$2"/>
<contactref element="LED1" pad="K"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
