<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>1.0.1</text>
<text>SYNCMAP</text>
<text>LSDJ MIDI OUT</text>
<text>GB</text>
<text>Developed by trash80 in California.
PCB by Poldet.</text>
<text> µArduinoboy</text>
</plain>
<libraries>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="arduino-micro">
<packages>
<package name="MICRO-EXTENDED">
</package>
</packages>
</library>
<library name="Catskulls_link_port">
<packages>
<package name="GBA-LINK-ALT">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="KB" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LEAD" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MGB" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NL" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SYNC" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STATUS" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="arduino-micro" package="MICRO-EXTENDED" value="ARDUINO_MICROEXTENDED">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Catskulls_link_port" package="GBA-LINK-ALT" value="GBA-LINKA">
<attribute name="SPICEPREFIX" value="X"/>
</element>
<element name="MODE" library="SparkFun-Retired" package="TACTILE-PTH" value="SWITCHMODE">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$2" pad="SD"/>
<contactref element="U$1" pad="5V"/>
<contactref element="U$2" pad="VCC"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="P$1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="MODE" pad="4"/>
<contactref element="MODE" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="MGB" pad="A"/>
<contactref element="U$1" pad="D8"/>
</signal>
<signal name="N$2">
<contactref element="NL" pad="A"/>
<contactref element="U$1" pad="D9"/>
</signal>
<signal name="N$3">
<contactref element="KB" pad="A"/>
<contactref element="U$1" pad="D10"/>
</signal>
<signal name="N$4">
<contactref element="LEAD" pad="A"/>
<contactref element="U$1" pad="D11"/>
</signal>
<signal name="N$5">
<contactref element="SYNC" pad="A"/>
<contactref element="U$1" pad="D12"/>
</signal>
<signal name="N$7">
<contactref element="STATUS" pad="A"/>
<contactref element="U$1" pad="D13"/>
</signal>
<signal name="N$9">
<contactref element="MGB" pad="K"/>
<contactref element="R1" pad="P$2"/>
<contactref element="NL" pad="K"/>
<contactref element="KB" pad="K"/>
<contactref element="LEAD" pad="K"/>
<contactref element="SYNC" pad="K"/>
<contactref element="STATUS" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="SI"/>
<contactref element="U$1" pad="A2"/>
</signal>
<signal name="N$16">
<contactref element="U$2" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
</signal>
<signal name="N$19">
<contactref element="U$2" pad="SO"/>
<contactref element="U$1" pad="A1"/>
</signal>
<signal name="N$20">
<contactref element="U$2" pad="SC"/>
<contactref element="U$1" pad="A0"/>
</signal>
<signal name="N$6">
<contactref element="MODE" pad="2"/>
<contactref element="MODE" pad="1"/>
<contactref element="U$1" pad="D2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
