<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<text>Indiana University</text>
<text>Avian Monitor</text>
<text>beta_r001_hw </text>
<wire x1="0" y1="0" x2="76.2" y2="0" width="0" layer="20"/>
<wire x1="76.2" y1="0" x2="76.2" y2="-49.53" width="0" layer="20"/>
<wire x1="76.2" y1="-49.53" x2="0" y2="-49.53" width="0" layer="20"/>
<wire x1="0" y1="-49.53" x2="0" y2="0" width="0" layer="20"/>
<text>VCHG</text>
<text>BATT+</text>
<text>IUSB</text>
<text>IRTC</text>
<text>STM32 BOOT JUMPER</text>
<text>RESET</text>
<text>STM32 LED</text>
<text>REG</text>
<text>+3V3</text>
<text>EXT_PWR</text>
<text>+2V to +5V</text>
<text>GND</text>
<text>FLASH POWER SW BYPASS</text>
<text>ISTM32</text>
<text>IACC</text>
<text>IPRESS</text>
<text>IFLASH</text>
<text>S_SCK</text>
<text>S_MISO</text>
<text>S_MOSI</text>
<text>F_CS</text>
<text>A_CS</text>
<text>P_CS</text>
<text>F_PWR</text>
<text>P_PWR</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>ACC_EXTI</text>
<text>RTC_EXTI</text>
<text>GND</text>
<text>V+</text>
<text>Regulator Bypass</text>
<text>IBATT</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>STM UART</text>
<text>GND</text>
<text>F_SCK</text>
<text>F_MISO</text>
<text>F_MOSI</text>
<text>USV_AV</text>
<text>STM_WK</text>
<text>GND</text>
</plain>
<libraries>
<library name="trans">
<packages>
<package name="TI-FEMTOFET-0402">
</package>
</packages>
</library>
<library name="rtc">
<packages>
<package name="AB-RTCM032.768-PACKAGE">
</package>
</packages>
</library>
<library name="stmf3">
<packages>
<package name="UFQFPN32">
</package>
</packages>
</library>
<library name="memory">
<packages>
<package name="WSON-8">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LGA-16-3X2.5">
<description>&lt;h3&gt;16-Pin LGA (3 x 3.25 mm) (1:1 footprint)&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/ADXL362.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Pin Count: 16&lt;/li&gt;
&lt;li&gt;Dimensions: 3.0 x 3.25 x 1.06 mm&lt;/li&gt;
&lt;li&gt;Pitch: 0.5 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;ADXL362&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="Kemet_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 28/03/2012 12:54:09</description>
<packages>
<package name="CAPC2013X110N">
</package>
</packages>
</library>
<library name="con-cortex">
<description>This library is for the ARM Cortex connectors as defined here:
http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf

For any information, please contact Shannon at strutz.shannon@gmail.com</description>
<packages>
<package name="2X10_0.1&quot;_TH_SH">
</package>
</packages>
</library>
<library name="Vishay_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 16:36:08</description>
<packages>
<package name="RESC1005X40N">
</package>
</packages>
</library>
<library name="LTC_bhimebau">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 10:08:22</description>
<packages>
<package name="SOP65P490X110-9N">
</package>
</packages>
</library>
<library name="regulator">
<packages>
<package name="TS14002_PACK">
</package>
</packages>
</library>
<library name="battery">
<packages>
<package name="GMB031009">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="sensor">
<packages>
<package name="HLGA-10L">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="con-cypressindustries">
<description>&lt;b&gt;Connectors from Cypress Industries&lt;/b&gt;&lt;p&gt;
www.cypressindustries.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="32005-601">
<description>&lt;b&gt;MINI USB-B R/A DIP&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-601.pdf</description>
</package>
</packages>
</library>
<library name="pinhead@1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DSN2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="rtc" package="AB-RTCM032.768-PACKAGE" value="AB-RTCM032.768KHZ">
<attribute name="NAME"/>
</element>
<element name="U$3" library="stmf3" package="UFQFPN32" value="STM32F432KBU6">
<attribute name="NAME"/>
</element>
<element name="U$4" library="memory" package="WSON-8" value="GD5F1GQ4UCY1G">
<attribute name="NAME"/>
</element>
<element name="U1" library="SparkFun-Sensors" package="LGA-16-3X2.5" value="ADXL362">
<attribute name="PROD_ID" value="IC-11297"/>
</element>
<element name="C14" library="Kemet_By_element14_Batch_1" package="CAPC2013X110N" value="1uF">
<attribute name="MPN" value="C0805C105K4RACTU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9227792"/>
<attribute name="OC_NEWARK" value="77C5351"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="16V"/>
</element>
<element name="U$12" library="con-cortex" package="2X10_0.1&quot;_TH_SH" value="TRADITIONALJTAG/SWDTH_SHROUDED">
<attribute name="NAME"/>
</element>
<element name="R41" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="R40" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="R42" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="R43" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="U2" library="LTC_bhimebau" package="SOP65P490X110-9N" value="LTC4071EMS8EPBF">
<attribute name="MPN" value="LTC4071EMS8E#PBF"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1947919"/>
<attribute name="OC_NEWARK" value="13T8411"/>
<attribute name="PACKAGE" value="MSOP-8"/>
<attribute name="SUPPLIER" value="LINEAR TECHNOLOGY"/>
</element>
<element name="U$7" library="regulator" package="TS14002_PACK" value="TS14002">
<attribute name="NAME"/>
</element>
<element name="U$9" library="battery" package="GMB031009" value="GMB031009">
<attribute name="NAME"/>
</element>
<element name="C1" library="rcl" package="C0402" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C0402" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C0402" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="rcl" package="C0402" value="47pf">
<attribute name="NAME"/>
</element>
<element name="C5" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="R0402" value="300">
<attribute name="NAME"/>
</element>
<element name="U$11" library="sensor" package="HLGA-10L" value="LPS22HB">
<attribute name="NAME"/>
</element>
<element name="U$1" library="trans" package="TI-FEMTOFET-0402" value="CSC25484F4">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="R0402" value="1125">
<attribute name="NAME"/>
</element>
<element name="JP2" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0402" value="300">
<attribute name="NAME"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08575"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
</element>
<element name="C7" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="200">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="R7" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="200">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="R9" library="rcl" package="R0402" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP13" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100k">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="JP14" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP15" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP16" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-cypressindustries" package="32005-601" value="MINI-USB_SHIELD5P2-32005-601">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="JP17" library="pinhead@1" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="JP4" library="pinhead@1" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0402" value="1125">
<attribute name="NAME"/>
</element>
<element name="R10" library="rcl" package="R0402" value="1125">
<attribute name="NAME"/>
</element>
<element name="R11" library="rcl" package="R0402" value="1125">
<attribute name="NAME"/>
</element>
<element name="R12" library="rcl" package="R0402" value="1125">
<attribute name="NAME"/>
</element>
<element name="C8" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C11" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="R13" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100k">
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
</element>
<element name="JP7" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
</element>
<element name="R15" library="SparkFun-Passives" package="0603-RES" value="100k">
<attribute name="NAME"/>
</element>
<element name="U$5" library="diode" package="DSN2" value="NSR01L30NXT5G">
<attribute name="NAME"/>
</element>
<element name="JP18" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="diode" package="DSN2" value="NSR01L30NXT5G">
<attribute name="NAME"/>
</element>
<element name="U$8" library="diode" package="DSN2" value="NSR01L30NXT5G">
<attribute name="NAME"/>
</element>
<element name="C15" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VUSB">
<contactref element="C14" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="U$8" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="C14" pad="2"/>
<contactref element="U$12" pad="10"/>
<contactref element="U$12" pad="8"/>
<contactref element="U$12" pad="16"/>
<contactref element="U$12" pad="6"/>
<contactref element="U$12" pad="14"/>
<contactref element="U$12" pad="12"/>
<contactref element="U$12" pad="4"/>
<contactref element="U$12" pad="18"/>
<contactref element="U$12" pad="20"/>
<contactref element="U$12" pad="11"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="P$6"/>
<contactref element="U$2" pad="P$7"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="P$12"/>
<contactref element="U1" pad="P$16"/>
<contactref element="U1" pad="P$13"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U$3" pad="P$16"/>
<contactref element="U$3" pad="P$32"/>
<contactref element="U$3" pad="P$33"/>
<contactref element="R43" pad="2"/>
<contactref element="U$9" pad="P$2"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="9"/>
<contactref element="U$11" pad="P$9"/>
<contactref element="U$11" pad="P$8"/>
<contactref element="S3" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP10" pad="3"/>
<contactref element="JP11" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="X1" pad="5"/>
<contactref element="JP17" pad="3"/>
<contactref element="J1" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="JP7" pad="6"/>
<contactref element="JP8" pad="7"/>
<contactref element="R15" pad="2"/>
<contactref element="JP18" pad="3"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="DEBUG_SWDIO_JTMS">
<contactref element="U$12" pad="7"/>
<contactref element="R41" pad="2"/>
<contactref element="U$3" pad="P$23"/>
<contactref element="JP17" pad="4"/>
</signal>
<signal name="DEBUG_SWCLK_JTCK">
<contactref element="U$12" pad="9"/>
<contactref element="R43" pad="1"/>
<contactref element="U$3" pad="P$24"/>
<contactref element="JP17" pad="2"/>
</signal>
<signal name="DEBUG_JTDI">
<contactref element="U$12" pad="5"/>
<contactref element="R40" pad="2"/>
</signal>
<signal name="DEBUG_JTDO_TRACESWO">
<contactref element="U$12" pad="13"/>
<contactref element="JP17" pad="6"/>
</signal>
<signal name="DEBUG_TRST">
<contactref element="U$12" pad="3"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="U$1" pad="P$3"/>
<contactref element="R41" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="U$12" pad="2"/>
<contactref element="U$12" pad="1"/>
<contactref element="JP14" pad="2"/>
<contactref element="JP15" pad="2"/>
<contactref element="JP16" pad="2"/>
<contactref element="JP17" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="RTC_SDA">
<contactref element="U$2" pad="P$5"/>
<contactref element="U$3" pad="P$20"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="RTC_SCL">
<contactref element="U$2" pad="P$4"/>
<contactref element="U$3" pad="P$19"/>
<contactref element="JP10" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="P$2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="P$11"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SENSOR_MOSI">
<contactref element="U1" pad="P$6"/>
<contactref element="U$11" pad="P$4"/>
<contactref element="U$3" pad="P$13"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="SENSOR_MISO">
<contactref element="U1" pad="P$7"/>
<contactref element="U$11" pad="P$5"/>
<contactref element="U$3" pad="P$12"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="ACCEL_CS">
<contactref element="U1" pad="P$8"/>
<contactref element="U$3" pad="P$10"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="P$9"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="REG_PWR">
<contactref element="C2" pad="1"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="U$7" pad="P$6"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$9" pad="P$1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="LED1" pad="C"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="JP6" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="STM_WAKEUP">
<contactref element="U$2" pad="P$3"/>
<contactref element="R9" pad="1"/>
<contactref element="U$3" pad="P$8"/>
<contactref element="JP18" pad="2"/>
</signal>
<signal name="ACCEL_EXTI">
<contactref element="U1" pad="P$9"/>
<contactref element="JP11" pad="2"/>
<contactref element="U$3" pad="P$9"/>
</signal>
<signal name="N$15">
<contactref element="JP3" pad="2"/>
<contactref element="U$3" pad="P$31"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="D1" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$4" pad="P$8"/>
<contactref element="U$4" pad="P$7"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="JP13" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="PRESSURE_POWER">
<contactref element="C9" pad="1"/>
<contactref element="U$3" pad="P$14"/>
<contactref element="JP12" pad="2"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="FLASH_POWER">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$3" pad="P$18"/>
<contactref element="R13" pad="1"/>
<contactref element="JP7" pad="5"/>
</signal>
<signal name="PRESSURE_CS">
<contactref element="U$11" pad="P$6"/>
<contactref element="U$3" pad="P$15"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="FLASH_CS">
<contactref element="U$4" pad="P$1"/>
<contactref element="U$3" pad="P$25"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="SENSOR_SCK">
<contactref element="U$3" pad="P$11"/>
<contactref element="U1" pad="P$4"/>
<contactref element="U$11" pad="P$2"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="UART_TX">
<contactref element="U$3" pad="P$29"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="UART_RX">
<contactref element="U$3" pad="P$30"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="LED_OUT">
<contactref element="U$3" pad="P$2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R7" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U$7" pad="P$8"/>
<contactref element="U$7" pad="P$7"/>
<contactref element="C1" pad="1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="VCHG">
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="R8" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="PRESSURE_DR">
<contactref element="U$11" pad="P$7"/>
<contactref element="U$3" pad="P$3"/>
</signal>
<signal name="RTC_EXTI">
<contactref element="U$2" pad="P$8"/>
<contactref element="JP11" pad="1"/>
<contactref element="U$3" pad="P$7"/>
</signal>
<signal name="NRST_JTAG">
<contactref element="U$12" pad="15"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="S3" pad="3"/>
<contactref element="JP17" pad="5"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="JP12" pad="1"/>
<contactref element="U$11" pad="P$10"/>
<contactref element="U$11" pad="P$1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="P$1"/>
<contactref element="C3" pad="1"/>
<contactref element="JP13" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="PROC_PWR">
<contactref element="JP14" pad="1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$3" pad="P$5"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$3" pad="P$17"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="RTC_PWR">
<contactref element="JP15" pad="1"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="R9" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="ACCEL_PWR">
<contactref element="JP16" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$14"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="EXT_PWR">
<contactref element="J1" pad="1"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="USB_AVAILABLE">
<contactref element="U$3" pad="P$6"/>
<contactref element="R15" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="JP18" pad="1"/>
</signal>
<signal name="USB_DM">
<contactref element="U$3" pad="P$21"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="USB_DP">
<contactref element="U$3" pad="P$22"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="FLASH_SCK">
<contactref element="U$3" pad="P$26"/>
<contactref element="U$4" pad="P$6"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="FLASH_MISO">
<contactref element="U$3" pad="P$27"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="FLASH_MOSI">
<contactref element="U$3" pad="P$28"/>
<contactref element="U$4" pad="P$5"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="U$5" pad="P$1"/>
<contactref element="R14" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
