<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="-13.3" y1="0" x2="13.3" y2="0" width="0" layer="20"/>
<wire x1="13.3" y1="0" x2="13.3" y2="40.8" width="0" layer="20"/>
<wire x1="13.3" y1="40.8" x2="-13.3" y2="40.8" width="0" layer="20"/>
<wire x1="-13.3" y1="40.8" x2="-13.3" y2="0" width="0" layer="20"/>
<text>Rev 1</text>
<text>AVR Programmer</text>
<text>CADed by: MrSwirlyEyes</text>
<text>AVR Programmer</text>
<text>CADed by: MrSwirlyEyes</text>
<text>Rev 1</text>
<text>Power
Target</text>
<text>NO
Power</text>
</plain>
<libraries>
<library name="PiB_connectors">
<packages>
<package name="HDRV6W64P254_2X3_762X483X838B_AVR-ISP">
<description>Double-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 7.62 X 4.83 X 8.38 mm body
&lt;p&gt;Double-row (2X3), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 7.62 X 4.83 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="2X05_VERT_MALE_SHROUDED_KEYED">
</package>
<package name="USB_MICRO-B_1050170001">
</package>
</packages>
</library>
<library name="PiB_capacitors">
<packages>
<package name="CAPC1005X55_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.55 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.55 mm&lt;/p&gt;</description>
</package>
<package name="CAPMP3216X180_SMD_CAP-TANT-1206">
<description>MOLDED BODY, 3.2 X 1.65 X 1.8 mm body
&lt;p&gt;MOLDED BODY package with body size 3.2 X 1.65 X 1.8 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB">
<packages>
<package name="SOIC127P600X175-14">
<description>14-SOIC, 1.27 mm pitch, 6.00 mm span, 8.65 X 3.90 X 1.75 mm body
&lt;p&gt;14-pin SOIC package with 1.27 mm pitch, 6.00 mm span with body size 8.65 X 3.90 X 1.75 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_leds">
<packages>
<package name="LEDC1005X40_LED-0402">
<description>CHIP, 1 X 0.5 X 0.4 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.4 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_ic_microcontrollers">
<packages>
<package name="SOIC127P1032X265-20">
<description>20-SOIC, 1.27 mm pitch, 10.32 mm span, 12.80 X 7.50 X 2.65 mm body
&lt;p&gt;20-pin SOIC package with 1.27 mm pitch, 10.32 mm span with body size 12.80 X 7.50 X 2.65 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_resistors">
<packages>
<package name="RESC1005X35_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.35 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_crystals_oscillators_resonators">
<packages>
<package name="OSCCC500X320X110_CRYSTAL">
<description>OSCILLATOR CORNERCONCAVE, 5 X 3.2 X 1.1 mm body
&lt;p&gt;OSCILLATOR CORNERCONCAVE package with body size 5 X 3.2 X 1.1 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="fuses">
<packages>
<package name="FUSC1608X45">
<description>Chip, 1.60 X 0.80 X 0.45 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.80 X 0.45 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_switches">
<packages>
<package name="SW_SLIDE_SPDT_RA_SMD_4V_300MA_6.7L-2.6W">
</package>
</packages>
</library>
<library name="PiB_logo">
<packages>
<package name="MRSWIRLYEYES-LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AVR_ISP1" library="PiB_connectors" package="HDRV6W64P254_2X3_762X483X838B_AVR-ISP" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/67996.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=609-3234-ND"/>
<attribute name="DISTPN" value="609-3234-ND"/>
<attribute name="MFR" value="Amphenol FCI"/>
<attribute name="MPN" value="67997-206HLF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AVR_ISP2" library="PiB_connectors" package="2X05_VERT_MALE_SHROUDED_KEYED" value="PTH VERT SHROUDED">
<attribute name="DATASHEET" value="http://multimedia.3m.com/mws/media/22504O/3mtm-100-in-loprof-hdr-100x-100strt-ra-4-wall-ts0818.pdf"/>
<attribute name="DATASHEET_CABLE" value="https://media.digikey.com/pdf/Data%20Sheets/Sparkfun%20PDFs/DEV-09215_Web.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=30310-6002HB-ND"/>
<attribute name="DISTLINK_CABLE" value="https://www.digikey.com/products/en?keywords=1568-1361-ND"/>
<attribute name="DISTPN" value="30310-6002HB-ND"/>
<attribute name="DISTPN_CABLE" value="1568-1361-ND"/>
<attribute name="DIST_CABLE" value="Digikey"/>
<attribute name="MFR" value="3M"/>
<attribute name="MFR_CABLE" value="SparkFun Electronics"/>
<attribute name="MPN" value="30310-6002HB"/>
<attribute name="MPN_CABLE" value="DEV-09215"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="PiB_capacitors" package="CAPC1005X55_SMD-0402" value="22pF/100V">
<attribute name="DATASHEET" value="http://ds.yuden.co.jp/TYCOMPAS/ut/detail.do?productNo=HMK105CG220JV-F&amp;fileName=HMK105CG220JV-F_SS&amp;mode=specSheetDownload"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=587-5004-1-ND"/>
<attribute name="DISTPN" value="587-5004-1-ND"/>
<attribute name="MFR" value="Taiyo Yuden"/>
<attribute name="MPN" value="HMK105CG220JV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="PiB_capacitors" package="CAPC1005X55_SMD-0402" value="22pF/100V">
<attribute name="DATASHEET" value="http://ds.yuden.co.jp/TYCOMPAS/ut/detail.do?productNo=HMK105CG220JV-F&amp;fileName=HMK105CG220JV-F_SS&amp;mode=specSheetDownload"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=587-5004-1-ND"/>
<attribute name="DISTPN" value="587-5004-1-ND"/>
<attribute name="MFR" value="Taiyo Yuden"/>
<attribute name="MPN" value="HMK105CG220JV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="PiB_capacitors" package="CAPC1005X55_SMD-0402" value="0.1uF/50V">
<attribute name="DATASHEET" value="https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=445-173610-1-ND"/>
<attribute name="DISTPN" value="445-173610-1-ND"/>
<attribute name="MFR" value="TDK Corporation"/>
<attribute name="MPN" value="C1005X7R1H104K050BE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="PiB_capacitors" package="CAPMP3216X180_SMD_CAP-TANT-1206" value="10uF/16V">
<attribute name="DATASHEET" value="http://datasheets.avx.com/TCJ.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=478-3451-1-ND"/>
<attribute name="DISTPN" value="478-3451-1-ND"/>
<attribute name="MFR" value="TCJA106M016R0200"/>
<attribute name="MPN" value="TCJA106M016R0200"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="PiB" package="SOIC127P600X175-14" value="74AC125">
<attribute name="DATASHEET" value="https://www.onsemi.com/pub/Collateral/MC74AC125-D.PDF"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=MC74AC125DR2GOSCT-ND"/>
<attribute name="DISTPN" value="MC74AC125DR2GOSCT-ND"/>
<attribute name="MFR" value="ON Semiconductor"/>
<attribute name="MPN" value="MC74AC125DR2G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D+_LED" library="PiB_leds" package="LEDC1005X40_LED-0402" value="BLUE">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402BWC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2203-1-ND"/>
<attribute name="DISTPN" value="492-2203-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402BWC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D-_LED" library="PiB_leds" package="LEDC1005X40_LED-0402" value="BLUE">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402BWC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2203-1-ND"/>
<attribute name="DISTPN" value="492-2203-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402BWC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="PiB_leds" package="LEDC1005X40_LED-0402" value="GREEN">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402GC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2205-1-ND"/>
<attribute name="DISTPN" value="492-2205-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402GC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="PiB_leds" package="LEDC1005X40_LED-0402" value="RED">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402RC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2208-1-ND"/>
<attribute name="DISTPN" value="492-2208-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402RC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR_LED" library="PiB_leds" package="LEDC1005X40_LED-0402" value="BLUE">
<attribute name="DATASHEET" value="https://www.bivar.com/portals/0/products/SM0402BWC.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=492-2203-1-ND"/>
<attribute name="DISTPN" value="492-2203-1-ND"/>
<attribute name="MFR" value="Bivar Inc."/>
<attribute name="MPN" value="SM0402BWC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MCU1" library="PiB_ic_microcontrollers" package="SOIC127P1032X265-20" value="ATtiny2313">
<attribute name="DATASHEET" value="http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2543-AVR-ATtiny2313_Datasheet.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=ATTINY2313-20SU-ND"/>
<attribute name="DISTPN" value="ATTINY2313-20SU-ND"/>
<attribute name="MFR" value="Microchip Technology"/>
<attribute name="MPN" value="ATTINY2313-20SU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1.5K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.5KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.5KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071K5L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="27">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-27JRCT-ND"/>
<attribute name="DISTPN" value="311-27JRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0727RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="27">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-27JRCT-ND"/>
<attribute name="DISTPN" value="311-27JRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0727RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="22K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-3.30KLRCT-ND"/>
<attribute name="DISTPN" value="311-22KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-0722KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="100">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-AC_51_RoHS_L_6.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG3516CT-ND"/>
<attribute name="DISTPN" value="YAG3516CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="AC0402JR-07100RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="PiB_resistors" package="RESC1005X35_SMD-0402" value="100">
<attribute name="DATASHEET" value="http://www.yageo.com/NewPortal/yageodocoutput?fileName=/pdf/R-Chip/PYu-AC_51_RoHS_L_6.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=YAG3516CT-ND"/>
<attribute name="DISTPN" value="YAG3516CT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="AC0402JR-07100RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="PiB_connectors" package="USB_MICRO-B_1050170001" value="USB2.0 MICRO-B">
<attribute name="DATASHEET" value="https://www.molex.com/pdm_docs/sd/1050170001_sd.pdf"/>
<attribute name="DATASHEET_CABLE" value="http://www.qualtekusa.com/images/Cable%20Assemblies/PDF_2/3025031-06.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=WM1399CT-ND"/>
<attribute name="DISTLINK_CABLE" value="https://www.digikey.com/products/en?keywords=Q967-ND"/>
<attribute name="DISTPN" value="WM1399CT-ND"/>
<attribute name="DISTPN_CABLE" value="Q967-ND"/>
<attribute name="DIST_CABLE" value="Digikey"/>
<attribute name="MFR" value="Molex, LLC"/>
<attribute name="MFR_CABLE" value="Qualtek"/>
<attribute name="MPN" value="1050170001"/>
<attribute name="MPN_CABLE" value="3025031-06"/>
</element>
<element name="XTAL1" library="PiB_crystals_oscillators_resonators" package="OSCCC500X320X110_CRYSTAL" value="12 MHz">
<attribute name="DATASHEET" value="https://abracon.com/Resonators/abm3b.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=535-9116-1-ND"/>
<attribute name="DISTPN" value="535-9116-1-ND"/>
<attribute name="MFR" value="Abracon LLC"/>
<attribute name="MPN" value="ABM3B-12.000MHZ-B2-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="fuses" package="FUSC1608X45" value="500mA / 50V">
<attribute name="DATASHEET" value="https://www.bourns.com/pdfs/SF0603S.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=SF-0603S050-2CT-ND"/>
<attribute name="DISTPN" value="SF-0603S050-2CT-ND"/>
<attribute name="MFR" value="Bourns Inc."/>
<attribute name="MPN" value="SF-0603S050-2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="PiB_switches" package="SW_SLIDE_SPDT_RA_SMD_4V_300MA_6.7L-2.6W" value="300mA/4V">
<attribute name="CREATOR" value="MrSwirlyEyes"/>
<attribute name="DATASHEET" value="https://media.digikey.com/pdf/Data%20Sheets/APEM%20Components%20PDFs/MA_Series_.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=679-1847-1-ND"/>
<attribute name="DISTPN" value="679-1847-1-ND"/>
<attribute name="MFR" value="APEM Inc."/>
<attribute name="MPN" value="MA12RTR"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="TESTED" value="YES"/>
</element>
<element name="U$1" library="PiB_logo" package="MRSWIRLYEYES-LOGO" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="MCU1" pad="4"/>
<contactref element="XTAL1" pad="3"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="XTAL1" pad="1"/>
<contactref element="MCU1" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="MCU1" pad="10"/>
<contactref element="USB1" pad="5"/>
<contactref element="USB1" pad="GND@0"/>
<contactref element="USB1" pad="GND@1"/>
<contactref element="USB1" pad="GND@2"/>
<contactref element="USB1" pad="GND@3"/>
<contactref element="USB1" pad="GND@4"/>
<contactref element="USB1" pad="GND@5"/>
<contactref element="USB1" pad="P$1"/>
<contactref element="USB1" pad="P$2"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="K"/>
<contactref element="AVR_ISP1" pad="GND"/>
<contactref element="AVR_ISP2" pad="4"/>
<contactref element="AVR_ISP2" pad="6"/>
<contactref element="AVR_ISP2" pad="8"/>
<contactref element="AVR_ISP2" pad="10"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="PWR_LED" pad="A"/>
<contactref element="C4" pad="A"/>
<contactref element="MCU1" pad="20"/>
<contactref element="C3" pad="1"/>
<contactref element="AVR_ISP1" pad="VCC"/>
<contactref element="F1" pad="2"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="USB1" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D+_LED" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="D-_LED" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="LED3" pad="K"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="LED4" pad="K"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="PWR_LED" pad="K"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="MOSI'">
<contactref element="MCU1" pad="17"/>
<contactref element="AVR_ISP1" pad="MOSI"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="MISO'">
<contactref element="MCU1" pad="18"/>
<contactref element="IC1" pad="8"/>
<contactref element="AVR_ISP1" pad="MISO"/>
</signal>
<signal name="SCK'">
<contactref element="MCU1" pad="19"/>
<contactref element="AVR_ISP1" pad="SCK"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="RESET'">
<contactref element="MCU1" pad="16"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="MCU1" pad="12"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="TARGET-PWR">
<contactref element="IC1" pad="14"/>
<contactref element="AVR_ISP2" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="AVR_ISP1" pad="RESET"/>
<contactref element="R1" pad="1"/>
<contactref element="MCU1" pad="1"/>
</signal>
<signal name="TARGET_MOSI">
<contactref element="AVR_ISP2" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="TARGET_RESET">
<contactref element="AVR_ISP2" pad="5"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="TARGET_SCK">
<contactref element="AVR_ISP2" pad="7"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="TARGET_MISO">
<contactref element="AVR_ISP2" pad="9"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$22">
<contactref element="MCU1" pad="9"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="MCU1" pad="11"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="D-">
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="USB1" pad="2"/>
<contactref element="D-_LED" pad="A"/>
</signal>
<signal name="D+">
<contactref element="R11" pad="2"/>
<contactref element="D+_LED" pad="A"/>
<contactref element="USB1" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="R11" pad="1"/>
<contactref element="MCU1" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="R12" pad="1"/>
<contactref element="MCU1" pad="7"/>
</signal>
<signal name="CTL">
<contactref element="MCU1" pad="8"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="4"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="11"/>
<contactref element="R8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
