<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.26" y2="0" width="0" layer="20"/>
<wire x1="21.26" y1="0" x2="21.26" y2="21.834" width="0" layer="20"/>
<wire x1="21.26" y1="21.834" x2="0" y2="21.834" width="0" layer="20"/>
<wire x1="0" y1="21.834" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RFM22-XXX-S2">
<description>Package for Hope RF s RFM22-xxx-S2 SMD wireless transciever, xxx is module s frequency band.
*Unproven*''</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="minicircuits">
<description>&lt;b&gt;Mini Circuits RF library&lt;/b&gt;&lt;p&gt;
&lt;author&gt;F4BXW f4bxw@tiscali.fr&lt;/author&gt;&lt;p&gt;
Version 1.7&lt;BR&gt;&lt;BR&gt;
ChangeLog:
&lt;UL&gt;
&lt;LI&gt;V1.0: Creation
&lt;LI&gt;V1.1: Nov 20 2004
&lt;UL&gt;
	&lt;LI&gt;add all LFCF &amp; HFCN references
	&lt;LI&gt;update some MCA1-* RF mixer datum
&lt;/UL&gt;
&lt;LI&gt;V1.2: Nov 23 2004
&lt;UL&gt;
	&lt;LI&gt;add few more rf mixer
&lt;/UL&gt;
&lt;LI&gt;V1.3: Nov 30 2004
&lt;UL&gt;
	&lt;LI&gt;add most ADT transformer series
	&lt;LI&gt;add variable attenuator
&lt;/UL&gt;
&lt;LI&gt;V1.4: Dec 1 2004
&lt;UL&gt;
	&lt;LI&gt;Add full ADP power spliter familly
&lt;/UL&gt;
&lt;LI&gt;V1.5 Dec 12th 2004:
&lt;UL&gt;
	&lt;LI&gt;Minor bugfix
	&lt;LI&gt;mca1 complete familly
&lt;/UL&gt;
&lt;LI&gt;V1.6 Jan 19th 2005:
&lt;UL&gt;
	&lt;LI&gt;add directionnal coupler
&lt;/UL&gt;
&lt;LI&gt;V1.7 Jul 8th 2005:
&lt;UL&gt;
	&lt;LI&gt;Add some VCO references
	&lt;LI&gt;Add I/Q modulators (MIQA series)
&lt;/UL&gt;
&lt;/UL&gt;</description>
<packages>
<package name="FV1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-RF" package="RFM22-XXX-S2" value="RFM22SMD"/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="220R">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="SML0805" value="green">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="SML0805" value="red">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="220R">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="mmbt2222">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="FILTER-1" library="minicircuits" package="FV1206" value="LFCN-490"/>
<element name="JP2" library="SparkFun-Connectors" package="1X01" value="ANTF"/>
<element name="JP3" library="SparkFun-Connectors" package="1X01" value="RSSI"/>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value="TXD"/>
<element name="JP6" library="SparkFun-Connectors" package="1X01" value="RXD"/>
<element name="JP7" library="SparkFun-Connectors" package="1X01" value="VIN"/>
<element name="JP8" library="SparkFun-Connectors" package="1X01" value="GND"/>
<element name="JP9" library="SparkFun-Connectors" package="1X01" value="SDA"/>
<element name="JP10" library="SparkFun-Connectors" package="1X01" value="SCL"/>
<element name="JP11" library="SparkFun-Connectors" package="1X01" value="VCC"/>
<element name="JP12" library="SparkFun-Connectors" package="1X01" value="SBUS"/>
<element name="IC1" library="linear" package="SOT23" value="MCP1703CB"/>
<element name="JP4" library="SparkFun-Connectors" package="1X01" value="PPM"/>
<element name="JP13" library="SparkFun-Connectors" package="1X01" value="GND"/>
<element name="JP14" library="SparkFun-Connectors" package="1X01" value="GND"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-SMD" value="16MHz">
<attribute name="PROD_ID" value="XTAL-08900"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X01" value="DTR"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="FILTER-1" pad="2"/>
<contactref element="FILTER-1" pad="4"/>
<contactref element="FILTER-1" pad="2"/>
<contactref element="FILTER-1" pad="4"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP14" pad="1"/>
<contactref element="JP13" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="JP11" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="15"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="16"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="17"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="2"/>
<contactref element="U$1" pad="13"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="32"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="N$12">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="25"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="26"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="RXD">
<contactref element="U1" pad="30"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="U1" pad="31"/>
<contactref element="JP5" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="PPM">
<contactref element="U1" pad="13"/>
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="RSSI">
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="27"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="28"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="29"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="C10" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="SBUS">
<contactref element="Q1" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="FILTER-1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="FILTER-1" pad="3"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="JP7" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP4" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="Y1" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$20">
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R8" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
