<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="1.27" x2="18.72" y2="1.27" width="0" layer="20"/>
<wire x1="18.72" y1="1.27" x2="18.72" y2="16.5" width="0" layer="20"/>
<wire x1="18.72" y1="16.5" x2="5.08" y2="16.5" width="0" layer="20"/>
<wire x1="5.08" y1="16.5" x2="5.08" y2="1.27" width="0" layer="20"/>
<text>|Mi + 
 Sk Mo
 Rs - </text>
<text>|Mo +
 nc -
 Rs -
 Sk -
 Mi -</text>
<text>AVR prog adapter</text>
<text>(c) 2014 Tyler Bletsch</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Connectors" package="AVR_ICSP" value="AVR_SPI_PROG2PTH"/>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="10"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="7"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="9"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
