<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0.045725" y1="44.918628125" x2="20.247809375" y2="44.918628125" width="0" layer="20"/>
<wire x1="20.247809375" y1="44.918628125" x2="20.247809375" y2="79.438659375" width="0" layer="20"/>
<wire x1="20.247809375" y1="79.438659375" x2="0.045725" y2="79.438659375" width="0" layer="20"/>
<wire x1="0.045725" y1="79.438659375" x2="0.045725" y2="44.918628125" width="0" layer="20"/>
<text>flightlights v0.2</text>
<text>D</text>
<text>+</text>
<text>_</text>
<text>D</text>
<text>_</text>
<text>+</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MINI">
<description>&lt;h3&gt;Arduino Pro Mini Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 34&lt;/li&gt;
&lt;li&gt;Area: 1.7 x 0.3 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Pro Mini&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MCU" library="SparkFun-Boards" package="ARDUINO_PRO_MINI" value="ARDUINO_PRO_MINI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CH1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CH2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MCU" pad="4"/>
</signal>
<signal name="CH1_DATA">
<contactref element="CH1" pad="1"/>
<contactref element="MCU" pad="5"/>
</signal>
<signal name="CH1_VCC">
<contactref element="CH1" pad="2"/>
<contactref element="MCU" pad="24"/>
<contactref element="CH2" pad="2"/>
</signal>
<signal name="CH2_DATA">
<contactref element="CH2" pad="1"/>
<contactref element="MCU" pad="6"/>
</signal>
<signal name="LED1_GND">
<contactref element="LED1" pad="1"/>
<contactref element="LED2" pad="1"/>
<contactref element="CH2" pad="3"/>
<contactref element="CH1" pad="3"/>
<contactref element="MCU" pad="23"/>
</signal>
<signal name="LED1_DATA">
<contactref element="LED1" pad="2"/>
<contactref element="MCU" pad="7"/>
</signal>
<signal name="LED1_VCC">
<contactref element="LED1" pad="3"/>
<contactref element="LED2" pad="3"/>
<contactref element="MCU" pad="21"/>
</signal>
<signal name="LED2_DATA">
<contactref element="LED2" pad="2"/>
<contactref element="MCU" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
