<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
<wire x1="16.51" y1="18.288" x2="16.51" y2="7.112" width="0" layer="20"/>
<wire x1="16.51" y1="7.112" x2="57.15" y2="7.112" width="0" layer="20"/>
<wire x1="57.15" y1="7.112" x2="57.15" y2="18.288" width="0" layer="20"/>
<wire x1="57.15" y1="18.288" x2="16.51" y2="18.288" width="0" layer="20"/>
<text>ATtiny85</text>
<text>github.com/kesor/
attiny85-ws2812b
v1.0</text>
<text>DOUT</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>INPUT</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
<package name="1X01_LONGPAD">
<description>&lt;h3&gt;Plated Through Hole - Long Pad&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pad w/ Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to lock pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="Seeed-Capacitor">
<packages>
<package name="PC-D5.3MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="NAME"/>
</element>
<element name="-" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10k"/>
<element name="U$1" library="SparkFun" package="SO08-EIAJ" value="ATTINY85">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK"/>
<element name="C1" library="adafruit" package="C0805K" value="">
<attribute name="VALUE"/>
</element>
<element name="MODE" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="SWITCH-MOMENTARY-2-SMD-1101NE"/>
<element name="C2" library="Seeed-Capacitor" package="PC-D5.3MM" value="100uf - 1000uf">
<attribute name="MPN" value="KS 100uF/16V"/>
<attribute name="VALUE" value="100uf"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="330"/>
<element name="J2" library="SparkFun-Connectors" package="1X03_LOCK_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RST">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="MODE" pad="P$1"/>
</signal>
<signal name="2R">
<contactref element="U$1" pad="2"/>
</signal>
<signal name="3R">
<contactref element="U$1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="-" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="MODE" pad="P$2"/>
<contactref element="C2" pad="-"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="+" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="8"/>
<contactref element="J1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="7R">
<contactref element="U$1" pad="7"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="6R">
<contactref element="U$1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="5R">
<contactref element="U$1" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$1">
</signal>
<signal name="DOUT">
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
