<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="57.15" y2="0" width="0" layer="20"/>
<wire x1="57.15" y1="0" x2="57.15" y2="50.8" width="0" layer="20"/>
<wire x1="57.15" y1="50.8" x2="0" y2="50.8" width="0" layer="20"/>
<wire x1="0" y1="50.8" x2="0" y2="0" width="0" layer="20"/>
<text>TechMDi ICOM PoE rev2</text>
<text>+5</text>
<text>+12</text>
<text>GND</text>
<text>PoE IN</text>
<text>ENET OUT</text>
<text>DI-2r2</text>
<text>5V OK</text>
<text>12V OK</text>
<text>D3</text>
<text>D2</text>
<text>D1</text>
<text>J1</text>
<text>J2</text>
<text>C1</text>
<text>IC2</text>
<text>IC1</text>
<text>TechMDi ICOM PoE rev2</text>
<text>GND</text>
<text>CPU</text>
<text>GPIO</text>
<text>+5</text>
<text>GND</text>
<text>J3</text>
<text>J4</text>
<text>4.5.13</text>
<text>TO</text>
<text>CPU</text>
<text>4.5.13</text>
<text>DI-2r2</text>
<text>+</text>
<text>-</text>
<text>-</text>
<hole x="3.81" y="46.99" drill="3.81"/>
<hole x="53.34" y="46.99" drill="3.81"/>
<hole x="53.34" y="3.81" drill="3.81"/>
<hole x="3.81" y="3.81" drill="3.81"/>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="TechMDParts">
<packages>
<package name="AG94000">
</package>
<package name="TE-6605834-1">
</package>
<package name="MOLEX-44620">
</package>
<package name="OKI-78SR-VERT">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2">
</package>
<package name="MOLEX-1X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="TechMDParts" package="AG94000" value="AG94000"/>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-1000UF-25V" value="1000uF"/>
<element name="J1" library="TechMDParts" package="TE-6605834-1" value="TE-6605834-1"/>
<element name="J2" library="TechMDParts" package="MOLEX-44620" value="MOLEX-44620"/>
<element name="D2" library="SparkFun-LED" package="LED3MM" value=""/>
<element name="D3" library="SparkFun-LED" package="LED3MM" value=""/>
<element name="IC2" library="TechMDParts" package="OKI-78SR-VERT" value="LM323T"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="">
<attribute name="PROD_ID" value="DIO-09886"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="MOLEX-1X2" value=""/>
</elements>
<signals>
<signal name="+12VCC">
<contactref element="IC1" pad="P$8"/>
<contactref element="C1" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="IC2" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="VCCGND">
<contactref element="IC1" pad="P$7"/>
<contactref element="C1" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="+5VCC">
<contactref element="D3" pad="A"/>
<contactref element="IC2" pad="3"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="DGND">
<contactref element="J1" pad="S1"/>
<contactref element="J1" pad="S2"/>
<contactref element="J2" pad="S1"/>
<contactref element="J2" pad="S2"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="9"/>
<contactref element="IC1" pad="P$3"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="10"/>
<contactref element="IC1" pad="P$4"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="RDP">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="P$3"/>
</signal>
<signal name="RDN">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="P$6"/>
</signal>
<signal name="TDP">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="P$1"/>
</signal>
<signal name="TDN">
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
