<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<hole x="16.51" y="16.51" drill="3.175"/>
<text>MilesTag</text>
<text>2014</text>
<text>Rev C</text>
<text>www.AtlasIR.com</text>
<text>H</text>
<text>H</text>
<text>H</text>
<text>G</text>
<text>G</text>
<text>G</text>
<text>D</text>
<text>D</text>
<text>D</text>
<text>+</text>
<text>+</text>
<text>+</text>
<circle x="16.51" y="16.51" radius="16.51" width="0.0254" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="00-SGAMF">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="0204/8">
<description>RESISTOR</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="JR-TSOP48XX">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$5" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$6" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="LED" library="00-SGAMF" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="00-SGAMF" package="0204/8" value="51">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="00-SGAMF" package="0204/8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$7" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="00-SGAMF" package="C025-025X050" value="10uF">
<attribute name="NAME"/>
</element>
<element name="E$2" library="00-SGAMF" package="JR-TSOP48XX" value=""/>
<element name="E$3" library="00-SGAMF" package="JR-TSOP48XX" value=""/>
</elements>
<signals>
<signal name="S$6">
<contactref element="LED" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="S$1">
<contactref element="E$6" pad="2"/>
</signal>
<signal name="GROUND">
<contactref element="E$7" pad="2"/>
<contactref element="E$5" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="S$10">
<contactref element="C1" pad="2"/>
<contactref element="E$3" pad="P$3"/>
<contactref element="R1" pad="2"/>
<contactref element="E$2" pad="P$3"/>
</signal>
<signal name="DATA">
<contactref element="E$2" pad="P$1"/>
<contactref element="E$5" pad="4"/>
<contactref element="E$7" pad="4"/>
<contactref element="E$6" pad="4"/>
</signal>
<signal name="POWER">
<contactref element="E$5" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="E$7" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="E$6" pad="3"/>
</signal>
<signal name="HITLED">
<contactref element="E$5" pad="1"/>
<contactref element="LED" pad="K"/>
<contactref element="E$7" pad="1"/>
<contactref element="E$6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
