<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<text>AGROSONIC</text>
<text>10 JAN 2019</text>
<text>v3</text>
<text>PWM</text>
<text>GND</text>
<text>AGROSONIC v1</text>
<text>AGROSONIC v1</text>
<text>PWM</text>
<text>GND</text>
</plain>
<libraries>
<library name="Keystone">
<packages>
<package name="PLATED_HOLE_1.02MM">
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="0805_B">
</package>
</packages>
</library>
<library name="microchip">
<packages>
<package name="SOIC-14-N">
</package>
</packages>
</library>
<library name="Stackpole">
<packages>
<package name="0805">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="OST">
<packages>
<package name="OSTVN02">
</package>
</packages>
</library>
<library name="TAG-CONNECT">
<packages>
<package name="PLUG-OF-NAILS">
</package>
</packages>
</library>
<library name="VISHAY">
<packages>
<package name="TEPT5600">
</package>
</packages>
</library>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="HEX_22_RADIUS">
<description>Hexagonal base for SONIC project</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="MPD">
<packages>
<package name="1025-7">
<description>http://www.memoryprotectiondevices.com/datasheets/BH1000G-datasheet.pdf</description>
</package>
</packages>
</library>
<library name="FIDUCIALS">
<packages>
<package name="2MM">
<description>Fiducial 2mm no cream</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="KEMET" package="0805_B" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="microchip" package="SOIC-14-N" value="PICF1615">
<attribute name="NAME"/>
</element>
<element name="J2" library="OST" package="OSTVN02" value="M02"/>
<element name="J1" library="TAG-CONNECT" package="PLUG-OF-NAILS" value="PIC_ICPH"/>
<element name="R2" library="Stackpole" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Stackpole" package="1206" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PH1" library="VISHAY" package="TEPT5600" value="TEMT5060"/>
<element name="U$4" library="ERIC" package="HEX_22_RADIUS" value=""/>
<element name="VBAT" library="Keystone" package="PLATED_HOLE_1.02MM" value="TEST_POINTMINIATURE">
<attribute name="NAME"/>
</element>
<element name="GND" library="Keystone" package="PLATED_HOLE_1.02MM" value="TEST_POINTMINIATURE">
<attribute name="NAME"/>
</element>
<element name="U$1" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="VALUE"/>
</element>
<element name="PH3" library="VISHAY" package="TEPT5600" value="TEMT5060"/>
<element name="U$3" library="MPD" package="1025-7" value="2477"/>
<element name="U$5" library="FIDUCIALS" package="2MM" value=""/>
<element name="U$6" library="FIDUCIALS" package="2MM" value=""/>
<element name="U$7" library="FIDUCIALS" package="2MM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="U$3" pad="-"/>
</signal>
<signal name="CC">
<contactref element="PH1" pad="C"/>
<contactref element="PH3" pad="C"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="PWM">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="C1IN1-">
<contactref element="U1" pad="9"/>
<contactref element="R3" pad="2"/>
<contactref element="PH1" pad="E"/>
<contactref element="PH3" pad="E"/>
</signal>
<signal name="ICSPDAT">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="MCLR">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="ICSPCLK">
<contactref element="U1" pad="12"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="VBAT">
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="VBAT" pad="1"/>
<contactref element="U$3" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
