<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="2.54" x2="63.48" y2="2.54" width="0" layer="20"/>
<wire x1="63.48" y1="2.54" x2="63.48" y2="26.34" width="0" layer="20"/>
<wire x1="63.48" y1="26.34" x2="5.08" y2="26.34" width="0" layer="20"/>
<wire x1="5.08" y1="26.34" x2="5.08" y2="2.54" width="0" layer="20"/>
<hole x="8.89" y="24.13" drill="1"/>
<hole x="11.43" y="24.13" drill="1"/>
<hole x="13.97" y="24.13" drill="1"/>
<hole x="16.51" y="24.13" drill="1"/>
<hole x="19.05" y="24.13" drill="1"/>
<hole x="21.59" y="24.13" drill="1"/>
<hole x="24.13" y="24.13" drill="1"/>
<hole x="26.67" y="24.13" drill="1"/>
<hole x="29.21" y="24.13" drill="1"/>
<hole x="31.75" y="24.13" drill="1"/>
<hole x="34.29" y="24.13" drill="1"/>
<hole x="36.83" y="24.13" drill="1"/>
<hole x="39.37" y="24.13" drill="1"/>
<hole x="41.91" y="24.13" drill="1"/>
<hole x="44.45" y="24.13" drill="1"/>
<hole x="46.99" y="24.13" drill="1"/>
<hole x="49.53" y="24.13" drill="1"/>
<hole x="52.07" y="24.13" drill="1"/>
<hole x="54.61" y="24.13" drill="1"/>
<hole x="57.15" y="24.13" drill="1"/>
<hole x="59.69" y="24.13" drill="1"/>
<hole x="8.89" y="8.89" drill="1"/>
<hole x="11.43" y="8.89" drill="1"/>
<hole x="13.97" y="8.89" drill="1"/>
<hole x="16.51" y="8.89" drill="1"/>
<hole x="19.05" y="8.89" drill="1"/>
<hole x="21.59" y="8.89" drill="1"/>
<hole x="24.13" y="8.89" drill="1"/>
<hole x="26.67" y="8.89" drill="1"/>
<hole x="29.21" y="8.89" drill="1"/>
<hole x="31.75" y="8.89" drill="1"/>
<hole x="34.29" y="8.89" drill="1"/>
<hole x="36.83" y="8.89" drill="1"/>
<hole x="39.37" y="8.89" drill="1"/>
<hole x="41.91" y="8.89" drill="1"/>
<hole x="44.45" y="8.89" drill="1"/>
<hole x="46.99" y="8.89" drill="1"/>
<hole x="49.53" y="8.89" drill="1"/>
<hole x="52.07" y="8.89" drill="1"/>
<hole x="54.61" y="8.89" drill="1"/>
<hole x="57.15" y="8.89" drill="1"/>
<hole x="59.69" y="8.89" drill="1"/>
</plain>
<libraries>
<library name="snes_cart">
<description>&lt;b&gt;SNES Cartridge Part Library&lt;/b&gt;&lt;p&gt;

Contains board outlines and common chips used in Super Nintendo game cartridges.
&lt;ul&gt;
&lt;li&gt;MaskROM
&lt;li&gt;SRAM
&lt;li&gt;Address Decoder
&lt;li&gt;Lockout chip
&lt;/ul&gt;
Also contains many chips used in reproduction cartridges.
&lt;ul&gt;
&lt;li&gt;Flash ROM
&lt;li&gt;SuperCIC lockout chip clone
&lt;/ul&gt;
&lt;author&gt;Created by qwertymodo&lt;/author&gt;&lt;p&gt;

Additional parts added by magno:
&lt;ul&gt;
&lt;li&gt;32Mbit UV EPROM
&lt;li&gt;Various 74XXX decoders
&lt;/ul&gt;

&lt;p&gt;
Email: qwertymodo@gmail.com</description>
<packages>
<package name="32/36-PDIP">
</package>
</packages>
</library>
<library name="m27C160D">
<packages>
<package name="M27C160P">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="snes_cart" package="32/36-PDIP" value="MASKROM36-DUAL"/>
<element name="U$2" library="m27C160D" package="M27C160P" value="M27C160"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="36"/>
<contactref element="U$2" pad="P$22"/>
<contactref element="U$1" pad="34"/>
</signal>
<signal name="A18">
<contactref element="U$2" pad="P$1"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="A17">
<contactref element="U$2" pad="P$2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="A7">
<contactref element="U$2" pad="P$3"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="A6">
<contactref element="U$2" pad="P$4"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="A5">
<contactref element="U$2" pad="P$5"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="A4">
<contactref element="U$2" pad="P$6"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="A3">
<contactref element="U$2" pad="P$7"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="A2">
<contactref element="U$2" pad="P$8"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="A1">
<contactref element="U$2" pad="P$9"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="A0">
<contactref element="U$2" pad="P$10"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="E">
<contactref element="U$2" pad="P$11"/>
<contactref element="U$1" pad="24"/>
</signal>
<signal name="G">
<contactref element="U$2" pad="P$13"/>
<contactref element="U$1" pad="33"/>
</signal>
<signal name="Q0">
<contactref element="U$2" pad="P$14"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="Q1">
<contactref element="U$2" pad="P$16"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="Q2">
<contactref element="U$2" pad="P$18"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="Q3">
<contactref element="U$2" pad="P$20"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="A19">
<contactref element="U$2" pad="P$42"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="A8">
<contactref element="U$2" pad="P$41"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="A9">
<contactref element="U$2" pad="P$40"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="A10">
<contactref element="U$2" pad="P$39"/>
<contactref element="U$1" pad="27"/>
</signal>
<signal name="A11">
<contactref element="U$2" pad="P$38"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="A12">
<contactref element="U$2" pad="P$37"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="A13">
<contactref element="U$2" pad="P$36"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="A14">
<contactref element="U$2" pad="P$35"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="A15">
<contactref element="U$2" pad="P$34"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="A16">
<contactref element="U$2" pad="P$33"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="Q7">
<contactref element="U$2" pad="P$29"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="Q6">
<contactref element="U$2" pad="P$27"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="Q5">
<contactref element="U$2" pad="P$25"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="Q4">
<contactref element="U$2" pad="P$23"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="Q15A-1">
<contactref element="U$2" pad="P$30"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="18"/>
<contactref element="U$2" pad="P$32"/>
<contactref element="U$2" pad="P$31"/>
<contactref element="U$2" pad="P$12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
