<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0.381" y1="3.683" x2="33.325" y2="3.683" width="0" layer="20"/>
<wire x1="33.325" y1="3.683" x2="33.325" y2="21.707" width="0" layer="20"/>
<wire x1="33.325" y1="21.707" x2="0.381" y2="21.707" width="0" layer="20"/>
<wire x1="0.381" y1="21.707" x2="0.381" y2="3.683" width="0" layer="20"/>
<text>OSH</text>
<text>Computer</text>
<text>Peripheral</text>
<text>USB Breakout V.0.1
Calvary Eng, IICEPD</text>
<text>GND</text>
<text>D+</text>
<text>D-</text>
<text>V+</text>
<text>V+</text>
<text>D-</text>
<text>D+</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-SMT-MALE">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="Orlando">
<packages>
<package name="M04X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="COMP-USB" library="SparkFun-Connectors" package="USB-A-SMT-MALE" value="USBA-SMD-MALE"/>
<element name="PERIPHERAL-USB" library="SparkFun-Connectors" package="USB-A-S-NOSILK-FEMALE" value="USB-A-SMD">
<attribute name="PROD_ID" value="CONN-09520"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="U$1" library="Orlando" package="M04X4" value="MX4X4"/>
</elements>
<signals>
<signal name="C-D+">
<contactref element="COMP-USB" pad="D+1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="C-D-">
<contactref element="COMP-USB" pad="D-1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="C-GND">
<contactref element="U$1" pad="4"/>
<contactref element="COMP-USB" pad="GND1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="C-V+">
<contactref element="U$1" pad="1"/>
<contactref element="COMP-USB" pad="VBUS1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="P-GND">
<contactref element="U$1" pad="12"/>
<contactref element="PERIPHERAL-USB" pad="GND"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="P-V+">
<contactref element="U$1" pad="9"/>
<contactref element="PERIPHERAL-USB" pad="VBUS"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="P-D-">
<contactref element="U$1" pad="10"/>
<contactref element="PERIPHERAL-USB" pad="D-"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="P-D+">
<contactref element="U$1" pad="11"/>
<contactref element="PERIPHERAL-USB" pad="D+"/>
<contactref element="U$1" pad="15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
