<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160.02" y2="24.13" width="0" layer="20"/>
<wire x1="160.02" y1="24.13" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<hole x="35" y="5.5" drill="2.75"/>
<hole x="35" y="95.5" drill="2.75"/>
<text>sp2 Quantum</text>
<text>Output Card</text>
<text>V.1.5.6</text>
<text>20-bit 4-channel DAC System</text>
<text>DPWR</text>
<text>DGND</text>
<text>-15V</text>
<text>AGND</text>
<text>+15V</text>
<hole x="154.5" y="94.5" drill="2.75"/>
<hole x="154.5" y="5.5" drill="2.75"/>
<text>3.3V PWR</text>
<text>LDAC</text>
<text>SDIN</text>
<text>SCLK</text>
<text>SDO</text>
<text>!CS!0</text>
<text>!CS!1</text>
<text>!CS!2</text>
<text>!CS!3</text>
<text>SDIN_BUF1</text>
<text>SDIN_BUF2</text>
<text>SDIN_BUF3</text>
<text>SDIN_BUF4</text>
<text>COMM</text>
<text>DGND</text>
<text>CHANNEL 0</text>
<text>CHANNEL 1</text>
<text>CHANNEL 2</text>
<text>CHANNEL 3</text>
<text>-15V PWR</text>
<text>+15V PWR</text>
<text>JE1</text>
<text>JE2</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>C76</text>
<text>C79</text>
<text>C29</text>
<text>C74</text>
<text>C73</text>
<text>C62</text>
<text>C34</text>
<text>R23</text>
<text>R33</text>
<text>R35</text>
<text>R32</text>
<text>R34</text>
<text>C69</text>
<text>C31</text>
<text>C3</text>
<text>C32</text>
<text>C33</text>
<text>C75</text>
<text>C70</text>
<text>C78</text>
<text>C77</text>
<text>C8</text>
<text>C4</text>
<text>C28</text>
<text>U10</text>
<text>U$1</text>
<text>U15</text>
<text>COMM</text>
<text>TP6</text>
<text>TP3</text>
<text>TP2</text>
<text>TP5</text>
<text>TP1</text>
<text>TP10</text>
<text>TP11</text>
<text>TP12</text>
<text>R3</text>
<text>LED3</text>
<text>JP16</text>
<text>TP4</text>
<text>TP7</text>
<text>C72</text>
<text>C90</text>
<text>C81</text>
<text>C98</text>
<text>C87</text>
<text>C84</text>
<text>C97</text>
<text>C95</text>
<text>R42</text>
<text>R44</text>
<text>R43</text>
<text>R41</text>
<text>C89</text>
<text>TP8</text>
<text>R24</text>
<text>C64</text>
<text>C59</text>
<text>C63</text>
<text>C60</text>
<text>U5</text>
<text>R4</text>
<text>LED4</text>
<text>C80</text>
<text>C93</text>
<text>C94</text>
<text>C9</text>
<text>C99</text>
<text>C1</text>
<text>C96</text>
<text>C83</text>
<text>C88</text>
<text>C82</text>
<text>C86</text>
<text>C92</text>
<text>U7</text>
<text>U$2</text>
<text>U8</text>
<text>C110</text>
<text>C101</text>
<text>C118</text>
<text>C107</text>
<text>C115</text>
<text>C117</text>
<text>C104</text>
<text>R25</text>
<text>R26</text>
<text>U18</text>
<text>U$3</text>
<text>U19</text>
<text>R51</text>
<text>R53</text>
<text>R50</text>
<text>R52</text>
<text>C109</text>
<text>C100</text>
<text>C113</text>
<text>C114</text>
<text>C14</text>
<text>C119</text>
<text>C116</text>
<text>C103</text>
<text>C108</text>
<text>C102</text>
<text>C106</text>
<text>C112</text>
<text>C130</text>
<text>C121</text>
<text>C135</text>
<text>C138</text>
<text>C137</text>
<text>C127</text>
<text>C124</text>
<text>R60</text>
<text>R62</text>
<text>R59</text>
<text>R61</text>
<text>C129</text>
<text>C120</text>
<text>U21</text>
<text>U$4</text>
<text>U22</text>
<text>C133</text>
<text>C134</text>
<text>C15</text>
<text>C139</text>
<text>C136</text>
<text>C132</text>
<text>C128</text>
<text>C123</text>
<text>C122</text>
<text>C126</text>
<text>LED2</text>
<text>R2\</text>
<text>SJ21</text>
<text>D1</text>
<text>C67</text>
<text>C68</text>
<text>J7</text>
<text>C65</text>
<text>C66</text>
<text>SJ22</text>
<text>D2</text>
<text>R1</text>
<text>LED1</text>
<text>C7</text>
<text>C11</text>
<text>PWR JMP</text>
<hole x="60" y="6" drill="3.4"/>
<text>Exposed AGND</text>
<hole x="156" y="36" drill="3.4"/>
<text>Exposed DGND</text>
<text>50ohm</text>
<text>50ohm</text>
<text>50ohm</text>
<text>50ohm</text>
<text>1.5kOhm</text>
<text>1.5kOhm</text>
<text>1.5kOhm</text>
<text>1.5kOhm</text>
<text>-REF</text>
<text>+REF</text>
<text>AGND
</text>
</plain>
<libraries>
<library name="kometter">
<packages>
<package name="TSSOP20">
</package>
</packages>
</library>
<library name="DAC board components">
<packages>
<package name="R_8">
</package>
<package name="RU_20">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="AD5791">
<packages>
<package name="RU_20">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="Custom Headers">
<packages>
<package name="10PIN">
</package>
<package name="2PIN">
</package>
<package name="3X6PIN">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-17">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
</packages>
</library>
<library name="PowerDiodes">
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AMP_227161">
<description>&lt;b&gt;JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC&lt;/b&gt;&lt;p&gt;
Source: amp_227161.pdf</description>
</package>
</packages>
</library>
<library name="4K AMP LIBRARY">
<packages>
<package name="MC74HC1G08">
</package>
</packages>
</library>
<library name="Capacitor">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC1608X85">
<description>Chip, 1.60 X 0.80 X 0.85 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.80 X 0.85 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Inductor">
<description>&lt;B&gt;Inductors - Fixed, Variable, Coupled</description>
<packages>
<package name="INDC2009X120">
<description>Chip, 2.00 X 0.90 X 1.20 mm body
&lt;p&gt;Chip package with body size 2.00 X 0.90 X 1.20 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C59" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C60" library="rcl" package="C0603" value="1.5uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C63" library="rcl" package="C0603" value="1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C64" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="U5" library="SparkFun-PowerIC" package="SOT223" value="V_REG_MIC2920">
</element>
<element name="C65" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C66" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C67" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C68" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R23" library="adafruit" package="R0603" value="0ohm">
<attribute name="NAME"/>
</element>
<element name="R24" library="adafruit" package="R0603" value="0ohm">
<attribute name="NAME"/>
</element>
<element name="R25" library="adafruit" package="R0603" value="0ohm">
<attribute name="NAME"/>
</element>
<element name="R26" library="adafruit" package="R0603" value="0ohm">
<attribute name="NAME"/>
</element>
<element name="U7" library="DAC board components" package="R_8" value="AD8676ARZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="AD8672AR"/>
<attribute name="VENDOR" value="Vendor"/>
</element>
<element name="C80" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C81" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="U8" library="AD5791" package="RU_20" value="AD5791ARUZ">
</element>
<element name="C82" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C83" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C84" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C86" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C87" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C88" library="adafruit" package="C1210" value="10uF">
</element>
<element name="U9" library="kometter" package="TSSOP20" value="SN74HC541">
</element>
<element name="C89" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R41" library="adafruit" package="R0603" value="10K">
</element>
<element name="R42" library="adafruit" package="R0603" value="10K">
</element>
<element name="R43" library="adafruit" package="R0603" value="10K">
</element>
<element name="R44" library="adafruit" package="R0603" value="10K">
</element>
<element name="C90" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C92" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C93" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C94" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C95" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C96" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C97" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C98" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C99" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="U18" library="DAC board components" package="R_8" value="AD8676ARZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="AD8672AR"/>
<attribute name="VENDOR" value="Vendor"/>
</element>
<element name="C100" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C101" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="U19" library="AD5791" package="RU_20" value="AD5791ARUZ">
</element>
<element name="C102" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C103" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C104" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C106" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C107" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C108" library="adafruit" package="C1210" value="10uF">
</element>
<element name="U20" library="kometter" package="TSSOP20" value="SN74HC541">
</element>
<element name="C109" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R50" library="adafruit" package="R0603" value="10K">
</element>
<element name="R51" library="adafruit" package="R0603" value="10K">
</element>
<element name="R52" library="adafruit" package="R0603" value="10K">
</element>
<element name="R53" library="adafruit" package="R0603" value="10K">
</element>
<element name="C110" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C112" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C113" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C114" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C115" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C116" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C117" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C118" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C119" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="U21" library="DAC board components" package="R_8" value="AD8676ARZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="AD8672AR"/>
<attribute name="VENDOR" value="Vendor"/>
</element>
<element name="C120" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C121" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="U22" library="AD5791" package="RU_20" value="AD5791ARUZ">
</element>
<element name="C122" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C123" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C124" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C126" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C127" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C128" library="adafruit" package="C1210" value="10uF">
</element>
<element name="U23" library="kometter" package="TSSOP20" value="SN74HC541">
</element>
<element name="C129" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R59" library="adafruit" package="R0603" value="10K">
</element>
<element name="R60" library="adafruit" package="R0603" value="10K">
</element>
<element name="R61" library="adafruit" package="R0603" value="10K">
</element>
<element name="R62" library="adafruit" package="R0603" value="10K">
</element>
<element name="C130" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C132" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C133" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C134" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C135" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C136" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C137" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C138" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C139" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="U10" library="DAC board components" package="R_8" value="AD8676ARZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="AD8672AR"/>
<attribute name="VENDOR" value="Vendor"/>
</element>
<element name="C28" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C29" library="rcl" package="C0603" value="100pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="U15" library="DAC board components" package="RU_20" value="AD5791ARUZ">
</element>
<element name="C31" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C32" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C34" library="rcl" package="C0603" value="100nF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C3" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C62" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C33" library="adafruit" package="C1210" value="10uF">
</element>
<element name="U6" library="kometter" package="TSSOP20" value="SN74HC541">
</element>
<element name="C69" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R32" library="adafruit" package="R0603" value="10K">
</element>
<element name="R33" library="adafruit" package="R0603" value="10K">
</element>
<element name="R34" library="adafruit" package="R0603" value="10K">
</element>
<element name="R35" library="adafruit" package="R0603" value="10K">
</element>
<element name="C70" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C72" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C73" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C74" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C75" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C76" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C77" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C78" library="adafruit" package="C1210" value="10uF">
</element>
<element name="C79" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C8" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C9" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C14" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="C15" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
</element>
<element name="COMM" library="Custom Headers" package="10PIN" value="10PINHEADER">
</element>
<element name="JP16" library="Custom Headers" package="2PIN" value="2PINHEADER">
</element>
<element name="TP1" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="Custom Headers" package="3X6PIN" value="3X6HEADER">
</element>
<element name="TP4" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603" value="10pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C1" library="rcl" package="C0603" value="10pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C7" library="rcl" package="C0603" value="10pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C11" library="rcl" package="C0603" value="10pF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="JP13" library="pinhead" package="1X03" value="">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="JP14" library="pinhead" package="1X03" value="">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="JP15" library="pinhead" package="1X03" value="">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="DAC board components" package="R_8" value="AD8675">
</element>
<element name="U$2" library="DAC board components" package="R_8" value="AD8675">
</element>
<element name="U$3" library="DAC board components" package="R_8" value="AD8675">
</element>
<element name="U$4" library="DAC board components" package="R_8" value="AD8675">
</element>
<element name="LED1" library="led" package="SML0805" value="">
<attribute name="POPULARITY" value="17"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="SML0805" value="">
<attribute name="POPULARITY" value="17"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="SML0805" value="">
<attribute name="POPULARITY" value="17"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="1.5k">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="1.5k">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0805" value="510">
</element>
<element name="R4" library="adafruit" package="R0805" value="330">
</element>
<element name="LED4" library="led" package="SML0805" value="">
<attribute name="POPULARITY" value="17"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP11" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP12" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="PowerDiodes" package="1206" value="SD1206S040S2R0">
</element>
<element name="D2" library="PowerDiodes" package="1206" value="SD1206S040S2R0">
</element>
<element name="SJ21" library="jumper" package="SJ" value="">
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="SJ22" library="jumper" package="SJ" value="">
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="1.5K">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R6" library="rcl" package="R0603" value="1.5K">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R7" library="rcl" package="R0603" value="1.5K">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R8" library="rcl" package="R0603" value="1.5K">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="SJ17" library="jumper" package="SJ" value="">
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="R0603" value="10K">
</element>
<element name="R10" library="adafruit" package="R0603" value="10K">
</element>
<element name="R11" library="adafruit" package="R0603" value="10K">
</element>
<element name="R12" library="adafruit" package="R0603" value="10K">
</element>
<element name="X5" library="con-coax" package="AMP_227161" value="227161-8">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="X6" library="con-coax" package="AMP_227161" value="227161-8">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="X7" library="con-coax" package="AMP_227161" value="227161-8">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="X8" library="con-coax" package="AMP_227161" value="227161-8">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="U$5" library="4K AMP LIBRARY" package="MC74HC1G08" value="MC74HC1G08">
</element>
<element name="U$6" library="4K AMP LIBRARY" package="MC74HC1G08" value="MC74HC1G08">
</element>
<element name="U$7" library="4K AMP LIBRARY" package="MC74HC1G08" value="MC74HC1G08">
</element>
<element name="U$8" library="4K AMP LIBRARY" package="MC74HC1G08" value="MC74HC1G08">
</element>
<element name="C2" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C5" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C6" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C10" library="rcl" package="C0603" value="0.1uF">
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C12" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C13" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="L1" library="Inductor" package="INDC2009X120" value="800n">
<attribute name="CATEGORY" value="Inductor"/>
<attribute name="CURRENT_RATING" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="JP5" library="pinhead" package="1X03" value="">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0603" value="50">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="JP1" library="pinhead" package="1X03" value="">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C17" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="L2" library="Inductor" package="INDC2009X120" value="800n">
<attribute name="CATEGORY" value="Inductor"/>
<attribute name="CURRENT_RATING" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="R14" library="rcl" package="R0603" value="50">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="JP2" library="pinhead" package="1X03" value="">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C19" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="L3" library="Inductor" package="INDC2009X120" value="800n">
<attribute name="CATEGORY" value="Inductor"/>
<attribute name="CURRENT_RATING" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="R15" library="rcl" package="R0603" value="50">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="JP3" library="pinhead" package="1X03" value="">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C21" library="Capacitor" package="CAPC1608X85" value="160p">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0603"/>
<attribute name="PACKAGE_TYPE" value="SMD"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Ceramic Capacitors"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value="MLCC"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="L4" library="Inductor" package="INDC2009X120" value="800n">
<attribute name="CATEGORY" value="Inductor"/>
<attribute name="CURRENT_RATING" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="R16" library="rcl" package="R0603" value="50">
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="JP4" library="Connector" package="1X10" value="PINHD-1X10">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Straight, 10 Position "/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Straight"/>
</element>
<element name="JP6" library="Connector" package="1X10" value="PINHD-1X10">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Straight, 10 Position "/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Straight"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="C65" pad="2"/>
<contactref element="C66" pad="2"/>
<contactref element="C67" pad="1"/>
<contactref element="C68" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="C80" pad="2"/>
<contactref element="C81" pad="2"/>
<contactref element="C84" pad="2"/>
<contactref element="C87" pad="1"/>
<contactref element="U8" pad="19"/>
<contactref element="C83" pad="2"/>
<contactref element="C88" pad="2"/>
<contactref element="C93" pad="2"/>
<contactref element="C90" pad="1"/>
<contactref element="C95" pad="1"/>
<contactref element="C94" pad="2"/>
<contactref element="C96" pad="1"/>
<contactref element="C97" pad="2"/>
<contactref element="C99" pad="1"/>
<contactref element="C98" pad="2"/>
<contactref element="C100" pad="2"/>
<contactref element="C101" pad="2"/>
<contactref element="C104" pad="2"/>
<contactref element="C107" pad="1"/>
<contactref element="U19" pad="19"/>
<contactref element="C103" pad="2"/>
<contactref element="C108" pad="2"/>
<contactref element="C113" pad="2"/>
<contactref element="C110" pad="1"/>
<contactref element="C115" pad="1"/>
<contactref element="C114" pad="2"/>
<contactref element="C116" pad="1"/>
<contactref element="C117" pad="2"/>
<contactref element="C119" pad="1"/>
<contactref element="C118" pad="2"/>
<contactref element="C120" pad="2"/>
<contactref element="C121" pad="2"/>
<contactref element="C124" pad="2"/>
<contactref element="C127" pad="1"/>
<contactref element="U22" pad="19"/>
<contactref element="C123" pad="2"/>
<contactref element="C128" pad="2"/>
<contactref element="C133" pad="2"/>
<contactref element="C130" pad="1"/>
<contactref element="C135" pad="1"/>
<contactref element="C134" pad="2"/>
<contactref element="C136" pad="1"/>
<contactref element="C137" pad="2"/>
<contactref element="C139" pad="1"/>
<contactref element="C138" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C62" pad="1"/>
<contactref element="U15" pad="19"/>
<contactref element="C32" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C73" pad="2"/>
<contactref element="C70" pad="1"/>
<contactref element="C75" pad="1"/>
<contactref element="C74" pad="2"/>
<contactref element="C76" pad="1"/>
<contactref element="C77" pad="2"/>
<contactref element="C79" pad="1"/>
<contactref element="C78" pad="2"/>
<contactref element="J7" pad="3"/>
<contactref element="J7" pad="9"/>
<contactref element="J7" pad="4"/>
<contactref element="J7" pad="10"/>
<contactref element="JP13" pad="2"/>
<contactref element="JP14" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="A"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="X8" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="X7" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="X6" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="X5" pad="2"/>
<contactref element="JP4" pad="7"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP6" pad="4"/>
<contactref element="JP6" pad="5"/>
<contactref element="JP6" pad="6"/>
<contactref element="JP6" pad="7"/>
</signal>
<signal name="DGND">
<contactref element="C64" pad="2"/>
<contactref element="C59" pad="2"/>
<contactref element="C63" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="C60" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="C82" pad="2"/>
<contactref element="C86" pad="2"/>
<contactref element="U8" pad="15"/>
<contactref element="U9" pad="10"/>
<contactref element="C89" pad="1"/>
<contactref element="C102" pad="2"/>
<contactref element="C106" pad="2"/>
<contactref element="U19" pad="15"/>
<contactref element="U20" pad="10"/>
<contactref element="C109" pad="1"/>
<contactref element="C122" pad="2"/>
<contactref element="C126" pad="2"/>
<contactref element="U22" pad="15"/>
<contactref element="U23" pad="10"/>
<contactref element="C129" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U15" pad="15"/>
<contactref element="U6" pad="10"/>
<contactref element="C69" pad="1"/>
<contactref element="COMM" pad="10"/>
<contactref element="JP16" pad="2"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="U6" pad="7"/>
<contactref element="U6" pad="8"/>
<contactref element="U6" pad="9"/>
<contactref element="U9" pad="7"/>
<contactref element="U9" pad="8"/>
<contactref element="U9" pad="9"/>
<contactref element="U20" pad="7"/>
<contactref element="U20" pad="8"/>
<contactref element="U20" pad="9"/>
<contactref element="U23" pad="7"/>
<contactref element="U23" pad="8"/>
<contactref element="U23" pad="9"/>
<contactref element="U23" pad="19"/>
<contactref element="U20" pad="19"/>
<contactref element="U9" pad="19"/>
<contactref element="U6" pad="19"/>
<contactref element="U$5" pad="P$3"/>
<contactref element="U$6" pad="P$3"/>
<contactref element="U$7" pad="P$3"/>
<contactref element="U$8" pad="P$3"/>
<contactref element="C2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="C60" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="U8" pad="9"/>
<contactref element="C82" pad="1"/>
<contactref element="U8" pad="10"/>
<contactref element="C86" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="R42" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="U19" pad="9"/>
<contactref element="C102" pad="1"/>
<contactref element="U19" pad="10"/>
<contactref element="C106" pad="1"/>
<contactref element="R50" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="R51" pad="2"/>
<contactref element="R53" pad="2"/>
<contactref element="U22" pad="9"/>
<contactref element="C122" pad="1"/>
<contactref element="U22" pad="10"/>
<contactref element="C126" pad="1"/>
<contactref element="R59" pad="2"/>
<contactref element="R61" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R62" pad="2"/>
<contactref element="U15" pad="9"/>
<contactref element="C31" pad="1"/>
<contactref element="U15" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="U6" pad="20"/>
<contactref element="C69" pad="2"/>
<contactref element="U9" pad="20"/>
<contactref element="C89" pad="2"/>
<contactref element="U20" pad="20"/>
<contactref element="C109" pad="2"/>
<contactref element="U23" pad="20"/>
<contactref element="C129" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="SJ17" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="U$5" pad="P$4"/>
<contactref element="U$6" pad="P$4"/>
<contactref element="U$7" pad="P$4"/>
<contactref element="U$8" pad="P$4"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="+15V">
<contactref element="C83" pad="1"/>
<contactref element="U8" pad="5"/>
<contactref element="C88" pad="1"/>
<contactref element="C93" pad="1"/>
<contactref element="C92" pad="1"/>
<contactref element="C98" pad="1"/>
<contactref element="C94" pad="1"/>
<contactref element="C97" pad="1"/>
<contactref element="U7" pad="8"/>
<contactref element="C103" pad="1"/>
<contactref element="U19" pad="5"/>
<contactref element="C108" pad="1"/>
<contactref element="C113" pad="1"/>
<contactref element="C112" pad="1"/>
<contactref element="C118" pad="1"/>
<contactref element="C114" pad="1"/>
<contactref element="C117" pad="1"/>
<contactref element="U18" pad="8"/>
<contactref element="C123" pad="1"/>
<contactref element="U22" pad="5"/>
<contactref element="C128" pad="1"/>
<contactref element="C133" pad="1"/>
<contactref element="C132" pad="1"/>
<contactref element="C138" pad="1"/>
<contactref element="C134" pad="1"/>
<contactref element="C137" pad="1"/>
<contactref element="U21" pad="8"/>
<contactref element="C32" pad="1"/>
<contactref element="U15" pad="5"/>
<contactref element="C33" pad="1"/>
<contactref element="C73" pad="1"/>
<contactref element="C72" pad="1"/>
<contactref element="C78" pad="1"/>
<contactref element="C74" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="U10" pad="8"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="JP14" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="7"/>
<contactref element="U$3" pad="7"/>
<contactref element="U$4" pad="7"/>
<contactref element="R1" pad="2"/>
<contactref element="D2" pad="P$2"/>
<contactref element="SJ22" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="-15V">
<contactref element="U8" pad="18"/>
<contactref element="C84" pad="1"/>
<contactref element="C87" pad="2"/>
<contactref element="C92" pad="2"/>
<contactref element="C90" pad="2"/>
<contactref element="C95" pad="2"/>
<contactref element="C96" pad="2"/>
<contactref element="C99" pad="2"/>
<contactref element="U7" pad="4"/>
<contactref element="U19" pad="18"/>
<contactref element="C104" pad="1"/>
<contactref element="C107" pad="2"/>
<contactref element="C112" pad="2"/>
<contactref element="C110" pad="2"/>
<contactref element="C115" pad="2"/>
<contactref element="C116" pad="2"/>
<contactref element="C119" pad="2"/>
<contactref element="U18" pad="4"/>
<contactref element="U22" pad="18"/>
<contactref element="C124" pad="1"/>
<contactref element="C127" pad="2"/>
<contactref element="C132" pad="2"/>
<contactref element="C130" pad="2"/>
<contactref element="C135" pad="2"/>
<contactref element="C136" pad="2"/>
<contactref element="C139" pad="2"/>
<contactref element="U21" pad="4"/>
<contactref element="U15" pad="18"/>
<contactref element="C34" pad="1"/>
<contactref element="C62" pad="2"/>
<contactref element="C72" pad="2"/>
<contactref element="C70" pad="2"/>
<contactref element="C75" pad="2"/>
<contactref element="C76" pad="2"/>
<contactref element="C79" pad="2"/>
<contactref element="U10" pad="4"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="JP14" pad="3"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$4" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="P$1"/>
<contactref element="SJ21" pad="1"/>
<contactref element="JP6" pad="8"/>
<contactref element="JP6" pad="9"/>
<contactref element="JP6" pad="10"/>
</signal>
<signal name="+REF_10V">
<contactref element="U10" pad="5"/>
<contactref element="C28" pad="1"/>
<contactref element="U7" pad="5"/>
<contactref element="C80" pad="1"/>
<contactref element="U18" pad="5"/>
<contactref element="C100" pad="1"/>
<contactref element="U21" pad="5"/>
<contactref element="C120" pad="1"/>
<contactref element="JP13" pad="1"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="-REF_10V">
<contactref element="U10" pad="3"/>
<contactref element="C29" pad="1"/>
<contactref element="U7" pad="3"/>
<contactref element="C81" pad="1"/>
<contactref element="U18" pad="3"/>
<contactref element="C101" pad="1"/>
<contactref element="U21" pad="3"/>
<contactref element="C121" pad="1"/>
<contactref element="JP13" pad="3"/>
<contactref element="JP4" pad="10"/>
<contactref element="JP4" pad="9"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="VREFNS[1]">
<contactref element="U10" pad="2"/>
<contactref element="U15" pad="17"/>
</signal>
<signal name="VREFPS[1]">
<contactref element="U10" pad="6"/>
<contactref element="U15" pad="3"/>
</signal>
<signal name="VREFPF[1]">
<contactref element="U10" pad="7"/>
<contactref element="U15" pad="4"/>
</signal>
<signal name="VREFNF[1]">
<contactref element="U10" pad="1"/>
<contactref element="U15" pad="16"/>
</signal>
<signal name="VOUT[1]">
<contactref element="U15" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="RESET[1]">
<contactref element="U15" pad="6"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="LDAC">
<contactref element="U9" pad="5"/>
<contactref element="U23" pad="5"/>
<contactref element="U6" pad="5"/>
<contactref element="COMM" pad="2"/>
<contactref element="TP6" pad="TP"/>
<contactref element="U20" pad="5"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="SDIN">
<contactref element="U9" pad="4"/>
<contactref element="U23" pad="4"/>
<contactref element="U6" pad="4"/>
<contactref element="COMM" pad="6"/>
<contactref element="TP3" pad="TP"/>
<contactref element="U20" pad="4"/>
</signal>
<signal name="SCLK">
<contactref element="U9" pad="3"/>
<contactref element="U23" pad="3"/>
<contactref element="COMM" pad="4"/>
<contactref element="TP2" pad="TP"/>
<contactref element="U20" pad="3"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="SYNC[1]">
<contactref element="COMM" pad="1"/>
<contactref element="TP1" pad="TP"/>
<contactref element="U6" pad="2"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="INV[1]">
<contactref element="U15" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="VOUT_BUF[1]">
<contactref element="U15" pad="20"/>
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="6"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="SYNC[2]">
<contactref element="COMM" pad="3"/>
<contactref element="TP10" pad="TP"/>
<contactref element="U9" pad="2"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="SYNC[3]">
<contactref element="COMM" pad="5"/>
<contactref element="U20" pad="2"/>
<contactref element="TP11" pad="TP"/>
<contactref element="U$7" pad="P$2"/>
</signal>
<signal name="SYNC[4]">
<contactref element="COMM" pad="7"/>
<contactref element="U23" pad="2"/>
<contactref element="TP12" pad="TP"/>
<contactref element="U$8" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="C64" pad="1"/>
<contactref element="C59" pad="1"/>
<contactref element="C63" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="JP16" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="SJ17" pad="2"/>
</signal>
<signal name="SDIN_CON[1]">
<contactref element="U15" pad="12"/>
<contactref element="U6" pad="16"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="SCLK_CON[1]">
<contactref element="U15" pad="13"/>
<contactref element="U6" pad="17"/>
</signal>
<signal name="SYNC_CON[1]">
<contactref element="U15" pad="14"/>
<contactref element="R35" pad="1"/>
<contactref element="U6" pad="18"/>
</signal>
<signal name="LDAC_CON[1]">
<contactref element="R34" pad="1"/>
<contactref element="U15" pad="8"/>
<contactref element="U6" pad="15"/>
</signal>
<signal name="N$72">
<contactref element="U8" pad="7"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="U19" pad="7"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="U22" pad="7"/>
<contactref element="R59" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U15" pad="7"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="VREFNF[2]">
<contactref element="U7" pad="1"/>
<contactref element="U8" pad="16"/>
</signal>
<signal name="VREFNS[2]">
<contactref element="U7" pad="2"/>
<contactref element="U8" pad="17"/>
</signal>
<signal name="VREFPF[2]">
<contactref element="U7" pad="7"/>
<contactref element="U8" pad="4"/>
</signal>
<signal name="VREFPS[2]">
<contactref element="U7" pad="6"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="VOUT[2]">
<contactref element="U8" pad="2"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="INV[2]">
<contactref element="U8" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="SDIN_CON[2]">
<contactref element="U8" pad="12"/>
<contactref element="U9" pad="16"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="SCLK_CON[2]">
<contactref element="U8" pad="13"/>
<contactref element="U9" pad="17"/>
</signal>
<signal name="VOUT_BUF[2]">
<contactref element="U8" pad="20"/>
<contactref element="U$2" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SYNC_CON[2]">
<contactref element="U8" pad="14"/>
<contactref element="R44" pad="1"/>
<contactref element="U9" pad="18"/>
</signal>
<signal name="RESET[2]">
<contactref element="U8" pad="6"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="LDAC_CON[2]">
<contactref element="R43" pad="1"/>
<contactref element="U8" pad="8"/>
<contactref element="U9" pad="15"/>
</signal>
<signal name="VREFNF[3]">
<contactref element="U18" pad="1"/>
<contactref element="U19" pad="16"/>
</signal>
<signal name="VREFNS[3]">
<contactref element="U18" pad="2"/>
<contactref element="U19" pad="17"/>
</signal>
<signal name="VREFPF[3]">
<contactref element="U18" pad="7"/>
<contactref element="U19" pad="4"/>
</signal>
<signal name="VREFPS[3]">
<contactref element="U18" pad="6"/>
<contactref element="U19" pad="3"/>
</signal>
<signal name="VOUT[3]">
<contactref element="U19" pad="2"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="INV[3]">
<contactref element="U19" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="SDIN_CON[3]">
<contactref element="U19" pad="12"/>
<contactref element="U20" pad="16"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="SCLK_CON[3]">
<contactref element="U19" pad="13"/>
<contactref element="U20" pad="17"/>
</signal>
<signal name="VOUT_BUF[3]">
<contactref element="U19" pad="20"/>
<contactref element="C7" pad="1"/>
<contactref element="U$3" pad="6"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="RESET[3]">
<contactref element="U19" pad="6"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="SYNC_CON[3]">
<contactref element="U19" pad="14"/>
<contactref element="R53" pad="1"/>
<contactref element="U20" pad="18"/>
</signal>
<signal name="LDAC_CON[3]">
<contactref element="R52" pad="1"/>
<contactref element="U19" pad="8"/>
<contactref element="U20" pad="15"/>
</signal>
<signal name="VREFNF[4]">
<contactref element="U21" pad="1"/>
<contactref element="U22" pad="16"/>
</signal>
<signal name="VREFNS[4]">
<contactref element="U21" pad="2"/>
<contactref element="U22" pad="17"/>
</signal>
<signal name="VREFPF[4]">
<contactref element="U21" pad="7"/>
<contactref element="U22" pad="4"/>
</signal>
<signal name="VREFPS[4]">
<contactref element="U21" pad="6"/>
<contactref element="U22" pad="3"/>
</signal>
<signal name="VOUT[4]">
<contactref element="U22" pad="2"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="INV[4]">
<contactref element="U22" pad="1"/>
<contactref element="U$4" pad="2"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="SDIN_CON[4]">
<contactref element="U22" pad="12"/>
<contactref element="U23" pad="16"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="SCLK_CON[4]">
<contactref element="U22" pad="13"/>
<contactref element="U23" pad="17"/>
</signal>
<signal name="SYNC_CON[4]">
<contactref element="U22" pad="14"/>
<contactref element="R62" pad="1"/>
<contactref element="U23" pad="18"/>
</signal>
<signal name="VOUT_BUF[4]">
<contactref element="U22" pad="20"/>
<contactref element="C11" pad="1"/>
<contactref element="U$4" pad="6"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="RESET[4]">
<contactref element="U22" pad="6"/>
<contactref element="R60" pad="1"/>
</signal>
<signal name="LDAC_CON[4]">
<contactref element="R61" pad="1"/>
<contactref element="U22" pad="8"/>
<contactref element="U23" pad="15"/>
</signal>
<signal name="SDO1">
</signal>
<signal name="SYNC[1]1">
</signal>
<signal name="5V1">
</signal>
<signal name="SDO_CON[1]1">
</signal>
<signal name="SCLK_CON[1]1">
</signal>
<signal name="LDAC_CON[1]1">
</signal>
<signal name="SDO2">
</signal>
<signal name="SYNC[1]2">
</signal>
<signal name="5V2">
</signal>
<signal name="SDO_CON[1]2">
</signal>
<signal name="SDO3">
</signal>
<signal name="SYNC[1]3">
</signal>
<signal name="5V3">
</signal>
<signal name="SDO_CON[1]3">
</signal>
<signal name="SYNC_CON[1]1">
</signal>
<signal name="N$20">
</signal>
<signal name="+15V1">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="+REF_10V[1]1">
</signal>
<signal name="-REF_10V[1]1">
</signal>
<signal name="+15V2">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="+REF_10V[1]2">
</signal>
<signal name="-REF_10V[1]2">
</signal>
<signal name="+15V3">
</signal>
<signal name="N$37">
</signal>
<signal name="N$38">
</signal>
<signal name="N$39">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="+REF_10V[1]3">
</signal>
<signal name="-REF_10V[1]3">
</signal>
<signal name="VCC1">
</signal>
<signal name="+15V4">
</signal>
<signal name="+REF_10V[1]4">
</signal>
<signal name="-REF_10V[1]4">
</signal>
<signal name="VREFPS[1]1">
</signal>
<signal name="VREFPF[1]1">
</signal>
<signal name="VREFNF[1]1">
</signal>
<signal name="VOUT[1]1">
</signal>
<signal name="VOUT_BUF[1]1">
</signal>
<signal name="VCC2">
</signal>
<signal name="+15V5">
</signal>
<signal name="-15V1">
</signal>
<signal name="+REF_10V[1]5">
</signal>
<signal name="VREFNS[1]1">
</signal>
<signal name="VREFPS[1]2">
</signal>
<signal name="VREFPF[1]2">
</signal>
<signal name="VREFNF[1]2">
</signal>
<signal name="VOUT[1]2">
</signal>
<signal name="INV[1]1">
</signal>
<signal name="VOUT_BUF[1]2">
</signal>
<signal name="VCC3">
</signal>
<signal name="+15V6">
</signal>
<signal name="-15V2">
</signal>
<signal name="+REF_10V[1]6">
</signal>
<signal name="-REF_10V[1]6">
</signal>
<signal name="VREFNS[1]2">
</signal>
<signal name="VREFPS[1]3">
</signal>
<signal name="VREFPF[1]3">
</signal>
<signal name="VREFNF[1]3">
</signal>
<signal name="VOUT[1]3">
</signal>
<signal name="INV[1]2">
</signal>
<signal name="VOUT_BUF[1]3">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="LED3" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="LED4" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="+15V_CONN">
<contactref element="D2" pad="P$1"/>
<contactref element="J7" pad="11"/>
<contactref element="J7" pad="5"/>
<contactref element="J7" pad="6"/>
<contactref element="J7" pad="12"/>
<contactref element="C65" pad="1"/>
<contactref element="C66" pad="1"/>
<contactref element="SJ22" pad="2"/>
</signal>
<signal name="-15V_CONN">
<contactref element="J7" pad="8"/>
<contactref element="J7" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="J7" pad="7"/>
<contactref element="D1" pad="P$2"/>
<contactref element="C67" pad="2"/>
<contactref element="C68" pad="2"/>
<contactref element="SJ21" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="X8" pad="1"/>
</signal>
<signal name="SDO_CON">
<contactref element="COMM" pad="8"/>
<contactref element="U6" pad="14"/>
<contactref element="U9" pad="14"/>
<contactref element="U20" pad="14"/>
<contactref element="U23" pad="14"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="SDO[1]">
<contactref element="U15" pad="11"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="SDO[2]">
<contactref element="U8" pad="11"/>
<contactref element="U9" pad="6"/>
</signal>
<signal name="SDO[3]">
<contactref element="U19" pad="11"/>
<contactref element="U20" pad="6"/>
</signal>
<signal name="SDO[4]">
<contactref element="U22" pad="11"/>
<contactref element="U23" pad="6"/>
</signal>
<signal name="ENABLE">
<contactref element="U$5" pad="P$5"/>
<contactref element="U6" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="ENABLE2">
<contactref element="U$6" pad="P$5"/>
<contactref element="U9" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="ENABLE3">
<contactref element="U$7" pad="P$5"/>
<contactref element="U20" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="ENABLE4">
<contactref element="U$8" pad="P$5"/>
<contactref element="U23" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="C12" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R13" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="JP5" pad="3"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="C17" pad="1"/>
<contactref element="L2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="X7" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="L2" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R14" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="C19" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="X6" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="L3" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R15" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R8" pad="2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="C21" pad="1"/>
<contactref element="L4" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="X5" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="L4" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R16" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
