<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.76" y2="0" width="0" layer="20"/>
<wire x1="17.76" y1="0" x2="17.76" y2="15.2275" width="0" layer="20"/>
<wire x1="17.76" y1="15.2275" x2="0" y2="15.2275" width="0" layer="20"/>
<wire x1="0" y1="15.2275" x2="0" y2="0" width="0" layer="20"/>
<text>SDA</text>
<text>SCL</text>
<text>CFD</text>
<text>EN</text>
<text>GND</text>
<text>IN</text>
<text>OUT</text>
<text>V5</text>
<text>CS-</text>
<text>CS+</text>
<text>DIM</text>
<text>GND</text>
<text>MAXIM16805
Breakout Board</text>
<text>ELECTRONILAB.CO</text>
</plain>
<libraries>
<library name="ELECTRONILAB">
<packages>
<package name="TQFN20-5X5">
<description>THIN QFN 20 5x5x0.75mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1X06-CLEANBIG">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ELECTRONILAB" package="TQFN20-5X5" value="MAX16805"/>
<element name="C1" library="adafruit" package="C0805" value="100nF"/>
<element name="C2" library="adafruit" package="C0805" value="100nF"/>
<element name="JP1" library="adafruit" package="1X06-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="adafruit" package="1X06-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
</elements>
<signals>
<signal name="N.C.">
<contactref element="U$1" pad="18"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="16"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="10"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="OUT">
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="IN">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="CFD">
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="V5">
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="15"/>
<contactref element="C2" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="CS-">
<contactref element="U$1" pad="14"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="CS+">
<contactref element="U$1" pad="13"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="EN">
<contactref element="U$1" pad="19"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="DIM">
<contactref element="U$1" pad="17"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="9"/>
</signal>
<signal name="EXT">
</signal>
</signals>
</board>
</drawing>
</eagle>
