<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>EPICUREAN
SHOPPE</text>
<text>(C) 2019 Z. Weeks</text>
<text>EPICUREAN SHOPPE Cab PCB v2.1</text>
<text>(C)2019 Zach Weeks
made in Salem, MA</text>
<text>www.zachweeks.com/pedals</text>
<text>WARNING!!! Use plastic jacks or plate. DO NOT GROUND JACKS!!! </text>
<wire x1="12.7" y1="58.42" x2="12.7" y2="20.32" width="0" layer="20"/>
<wire x1="12.7" y1="20.32" x2="86.36" y2="20.32" width="0" layer="20"/>
<wire x1="86.36" y1="20.32" x2="86.36" y2="58.42" width="0" layer="20"/>
<wire x1="86.36" y1="58.42" x2="12.7" y2="58.42" width="0" layer="20"/>
<text>Terminal pins are Molex 19705-4003 (6.35 mm x 0.81 mm)</text>
<text>VERSION 2.1 / JULY 2019</text>
<text>use Neutrik
NMJ6HCD2 jacks</text>
</plain>
<libraries>
<library name="con-faston">
<description>&lt;b&gt;FASTON Connector&lt;/b&gt; Printed Circuit Board Tabs&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F061.100">
<description>&lt;b&gt;FASTON 6.3 mm x 0.8 mm&lt;/b&gt; DIN 46342 Teil 1&lt;p&gt;
Flachstecker Typ Vogt 3866B.68 (F061.100)&lt;br&gt;
Distributor: Bürklin 05 F 270</description>
</package>
</packages>
</library>
<library name="eae_logos">
<description>eae logo drawn</description>
<packages>
<package name="BIGESLOGO">
</package>
<package name="ESLOGO">
</package>
</packages>
</library>
<library name="mb2017_jacks">
<packages>
<package name="TRS_SW">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1+" library="con-faston" package="F061.100" value="S1+">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1-" library="con-faston" package="F061.100" value="S1-">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2+" library="con-faston" package="F061.100" value="S2+">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2-" library="con-faston" package="F061.100" value="S2-">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="eae_logos" package="BIGESLOGO" value=""/>
<element name="U$3" library="eae_logos" package="BIGESLOGO" value=""/>
<element name="PARALLEL" library="mb2017_jacks" package="TRS_SW" value=""/>
<element name="SERIES" library="mb2017_jacks" package="TRS_SW" value=""/>
<element name="U$1" library="eae_logos" package="ESLOGO" value=""/>
<element name="PAD1" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD3" library="wirepad" package="3,81/1,4" value=""/>
<element name="PAD4" library="wirepad" package="3,81/1,4" value=""/>
</elements>
<signals>
<signal name="N$4">
<contactref element="SERIES" pad="RN"/>
<contactref element="S1-" pad="A1"/>
<contactref element="S1-" pad="A2"/>
<contactref element="PARALLEL" pad="S"/>
<contactref element="PARALLEL" pad="R"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="S2+" pad="A1"/>
<contactref element="S2+" pad="A2"/>
<contactref element="PARALLEL" pad="RN"/>
<contactref element="SERIES" pad="TN"/>
<contactref element="PAD3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="S2-" pad="A1"/>
<contactref element="S2-" pad="A2"/>
<contactref element="SERIES" pad="R"/>
<contactref element="SERIES" pad="S"/>
<contactref element="PAD4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="SERIES" pad="T"/>
<contactref element="S1+" pad="A1"/>
<contactref element="S1+" pad="A2"/>
<contactref element="PARALLEL" pad="T"/>
<contactref element="PAD1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
