<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-10" x2="48" y2="-10" width="0" layer="20"/>
<wire x1="48" y1="-10" x2="48" y2="76" width="0" layer="20"/>
<wire x1="48" y1="76" x2="0" y2="76" width="0" layer="20"/>
<wire x1="0" y1="76" x2="0" y2="-10" width="0" layer="20"/>
<text>ON</text>
<hole x="6" y="3" drill="2.11"/>
<hole x="42" y="3" drill="2.11"/>
<text>P</text>
<text>I</text>
<text>D</text>
<text>Idlehandsdevelopment.com</text>
<text>PIDDYBOT_V4</text>
<text>#PIDDYBOT_V1.1</text>
<text>IDLE HANDS DEV.</text>
<text>CHG</text>
<text>1:ISP</text>
<text>B.TECH McMaster/Mohawk</text>
<text>BT RST</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="LED-0603">
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="EIA3528">
</package>
<package name="1X01NS">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="EIA3216">
</package>
<package name="PTC-1206">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="QFN-24-4MM2">
</package>
<package name="USB_AB_MICRO_1:1_V2">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LONGPADS">
</package>
<package name="JST-2-PTH">
</package>
<package name="1X06-1MM">
<description>Works with part #579 (https://www.sparkfun.com/products/579). Commonly used on GPS modules EM408, EM406 and GP-635T. Also compatible with cable 9123 (https://www.sparkfun.com/products/9123) and cable 574 (https://www.sparkfun.com/products/574).</description>
</package>
<package name="2X3-NS">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="ScratchPad">
<packages>
<package name="RN41">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ALPS_POT">
</package>
<package name="SWITCH-SPDT">
</package>
</packages>
</library>
<library name="murata-filter">
<description>&lt;b&gt;Murata Filters&lt;/b&gt;&lt;p&gt;
Distributor RS Components&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CSTCR6M">
<description>Source: http://search.murata.co.jp/Ceramy/CatalogshowpageAction.do?sDirnm=A07X&amp;sFilnm=81G07006&amp;sType=2&amp;sLang=en&amp;sNHinnm=CSTCR6M00G53Z-R0&amp;sCapt=Standard_Land_Pattern_Dimensions</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
</packages>
</library>
<library name="IdleHandsProject">
<packages>
<package name="IHD-LOGO-L">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="scout">
<packages>
<package name="WSON-12">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C9" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="SparkFun" package="0603-CAP" value="2.2nF">
<attribute name="NAME"/>
</element>
<element name="C14" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C16" library="SparkFun" package="0603-CAP" value="10nF">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun" package="0603-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun" package="0603-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="U1" library="Testing" package="QFN-24-4MM2" value="MPU-6050-1"/>
<element name="R12" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
</element>
<element name="D2" library="SparkFun" package="LED-0603" value="Green">
<attribute name="NAME"/>
</element>
<element name="R21" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
</element>
<element name="U5" library="ScratchPad" package="RN41" value="BLUETOOTH-RN41">
<attribute name="NAME"/>
</element>
<element name="D3" library="SparkFun" package="LED-0603" value="Red">
<attribute name="NAME"/>
</element>
<element name="R22" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun" package="1X01NS" value="M01SMDNS"/>
<element name="CN2" library="SparkFun-Connectors" package="JST-2-PTH" value="M02JST-PTH-2">
<attribute name="NAME"/>
</element>
<element name="U$16" library="SparkFun-Electromechanical" package="ALPS_POT" value=""/>
<element name="U$17" library="SparkFun-Electromechanical" package="ALPS_POT" value=""/>
<element name="U$18" library="SparkFun-Electromechanical" package="ALPS_POT" value=""/>
<element name="MTA" library="SparkFun-Connectors" package="1X02_LONGPADS" value="M02PTH3"/>
<element name="MTB" library="SparkFun-Connectors" package="1X02_LONGPADS" value="M02PTH3"/>
<element name="D11" library="SparkFun" package="LED-0603" value="RED">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
</element>
<element name="U2" library="SparkFun" package="SOT23-5" value="MCP73831">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun" package="0603-RES" value="2K">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun" package="0603-RES" value="1K">
<attribute name="NAME"/>
</element>
<element name="LED2" library="SparkFun" package="LED-0603" value="Red">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="C11" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun" package="LED-0603" value="Green">
<attribute name="NAME"/>
</element>
<element name="U6" library="SparkFun" package="SOT23-5" value="MIC5219">
<attribute name="NAME"/>
</element>
<element name="C15" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C22" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C23" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun" package="0603-RES" value="330">
<attribute name="NAME"/>
</element>
<element name="D5" library="SparkFun" package="LED-0603" value="Yellow">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun" package="0603-RES" value="22">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun" package="0603-RES" value="22">
<attribute name="NAME"/>
</element>
<element name="X2" library="Testing" package="USB_AB_MICRO_1:1_V2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="SparkFun" package="PTC-1206" value="500mA">
<attribute name="NAME"/>
</element>
<element name="D6" library="SparkFun" package="SOD-323" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="murata-filter" package="CSTCR6M" value="8Mhz">
<attribute name="OC_NEWARK" value=""/>
<attribute name="MPN" value="CSTCE8M00G55-R0"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="NAME"/>
</element>
<element name="RESET" library="SparkFun" package="TACTILE_SWITCH_SMD" value="RESET">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X06-1MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X06-1MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-DigitalIC" package="SPARKFUN-DIGITALIC_TQFP44" value="ATMEGA32U4TQFP">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="IdleHandsProject" package="IHD-LOGO-L" value="IDLEHANDS_LOGOL"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="S4" library="SparkFun-Electromechanical" package="SWITCH-SPDT" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0603-RES" value="1M">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun" package="0603-RES" value="470k">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="U$2" library="scout" package="WSON-12" value="DRV8835"/>
<element name="C5" library="SparkFun" package="EIA3528" value="10uf , 20V">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="BT_PWR" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
</element>
<element name="BATT_JP" library="SparkFun-Passives" package="SJ_2S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C16" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="R12" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="12"/>
<contactref element="U5" pad="25"/>
<contactref element="U5" pad="27"/>
<contactref element="U5" pad="28"/>
<contactref element="U5" pad="29"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="U$16" pad="P$1"/>
<contactref element="U$17" pad="P$1"/>
<contactref element="U$18" pad="P$1"/>
<contactref element="C6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C7" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U6" pad="2"/>
<contactref element="C15" pad="C"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="X2" pad="GND"/>
<contactref element="CN2" pad="1"/>
<contactref element="Y1" pad="2"/>
<contactref element="RESET" pad="2"/>
<contactref element="RESET" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="35"/>
<contactref element="U$1" pad="43"/>
<contactref element="U$1" pad="33"/>
<contactref element="U$1" pad="5"/>
<contactref element="JP5" pad="6"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="C14" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U$2" pad="THERM4"/>
<contactref element="U$2" pad="THERMCENTER"/>
<contactref element="U$2" pad="THERM1"/>
<contactref element="U$2" pad="THERM2"/>
<contactref element="U$2" pad="P6"/>
<contactref element="U$2" pad="THERM3"/>
<contactref element="C5" pad="C"/>
<contactref element="U$2" pad="THERMCENTER2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="U$2" pad="THERMCENTER1"/>
</signal>
<signal name="AREF">
<contactref element="C12" pad="2"/>
<contactref element="U$1" pad="42"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="9"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="RX-I">
<contactref element="U$1" pad="20"/>
<contactref element="U5" pad="14"/>
</signal>
<signal name="TX-O">
<contactref element="U$1" pad="21"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="20"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="10"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="AUX_SDA">
<contactref element="U1" pad="6"/>
</signal>
<signal name="AUX_SCL">
<contactref element="U1" pad="7"/>
</signal>
<signal name="SCL">
<contactref element="R10" pad="1"/>
<contactref element="U1" pad="23"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="SDA">
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="24"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="12"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="A01">
<contactref element="MTA" pad="1"/>
<contactref element="JP3" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="P2"/>
</signal>
<signal name="A02">
<contactref element="MTA" pad="2"/>
<contactref element="JP3" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="U$2" pad="P3"/>
</signal>
<signal name="B02">
<contactref element="MTB" pad="2"/>
<contactref element="JP4" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="U$2" pad="P4"/>
</signal>
<signal name="B01">
<contactref element="MTB" pad="1"/>
<contactref element="JP4" pad="5"/>
<contactref element="C4" pad="2"/>
<contactref element="U$2" pad="P5"/>
</signal>
<signal name="PWMA">
<contactref element="U$2" pad="P9"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="AIN1">
<contactref element="U$2" pad="P10"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="BIN1">
<contactref element="U$2" pad="P8"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="PWMB">
<contactref element="U$1" pad="32"/>
<contactref element="U$2" pad="P7"/>
</signal>
<signal name="D1">
<contactref element="R12" pad="1"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="RTS">
<contactref element="U5" pad="15"/>
</signal>
<signal name="CTS">
<contactref element="U5" pad="16"/>
</signal>
<signal name="D2">
<contactref element="D2" pad="C"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D3" pad="A"/>
<contactref element="U5" pad="21"/>
</signal>
<signal name="N$11">
<contactref element="U5" pad="19"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="PIO4">
<contactref element="U5" pad="22"/>
<contactref element="R22" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="POTP">
<contactref element="U$16" pad="P$2"/>
<contactref element="U$1" pad="39"/>
</signal>
<signal name="POTI">
<contactref element="U$17" pad="P$2"/>
<contactref element="U$1" pad="40"/>
</signal>
<signal name="POTD">
<contactref element="U$18" pad="P$2"/>
<contactref element="U$1" pad="41"/>
</signal>
<signal name="V_BATT">
<contactref element="CN2" pad="2"/>
<contactref element="S4" pad="1"/>
<contactref element="BATT_JP" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="D11" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PROG">
<contactref element="U2" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="STAT">
<contactref element="D11" pad="C"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R5" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="MTE_B_2">
<contactref element="JP4" pad="2"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="MTE_B_1">
<contactref element="JP4" pad="3"/>
<contactref element="U$1" pad="27"/>
</signal>
<signal name="N$15">
<contactref element="C22" pad="2"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="UVCC">
<contactref element="C23" pad="2"/>
<contactref element="X2" pad="VBUS"/>
<contactref element="F1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="D-">
<contactref element="R13" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="D+">
<contactref element="R9" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="MTE_A_2">
<contactref element="JP3" pad="3"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="D14">
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="TXLED">
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="N$16">
<contactref element="R13" pad="2"/>
<contactref element="X2" pad="D-"/>
</signal>
<signal name="N$17">
<contactref element="R9" pad="2"/>
<contactref element="X2" pad="D+"/>
</signal>
<signal name="N$19">
<contactref element="R8" pad="2"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$20">
<contactref element="R7" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="3.3V">
<contactref element="C10" pad="1"/>
<contactref element="C7" pad="A"/>
<contactref element="U6" pad="5"/>
<contactref element="C11" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="U$16" pad="P$3"/>
<contactref element="U$17" pad="P$3"/>
<contactref element="U$18" pad="P$3"/>
<contactref element="R6" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP4" pad="4"/>
<contactref element="U$1" pad="24"/>
<contactref element="U$1" pad="44"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="34"/>
<contactref element="JP5" pad="2"/>
<contactref element="U$2" pad="P11"/>
<contactref element="C8" pad="1"/>
<contactref element="U$2" pad="P12"/>
<contactref element="BT_PWR" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="C14" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$1">
<contactref element="Y1" pad="1"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="N$2">
<contactref element="Y1" pad="3"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="MISO-MTE_A_1">
<contactref element="U$1" pad="11"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="10"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="JP5" pad="5"/>
<contactref element="R6" pad="1"/>
<contactref element="RESET" pad="4"/>
<contactref element="RESET" pad="3"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$5">
</signal>
<signal name="D7">
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="F1" pad="2"/>
<contactref element="D6" pad="2"/>
</signal>
<signal name="RAW">
<contactref element="C15" pad="A"/>
<contactref element="D6" pad="1"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="3"/>
<contactref element="S4" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C5" pad="A"/>
<contactref element="U$2" pad="P1"/>
</signal>
<signal name="BATT">
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="36"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="37"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="38"/>
</signal>
<signal name="N$12">
<contactref element="BT_PWR" pad="1"/>
<contactref element="U5" pad="11"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="BATT_JP" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
