<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.254" x2="70.917" y2="-0.254" width="0" layer="20"/>
<wire x1="70.917" y1="-0.254" x2="70.917" y2="51.552" width="0" layer="20"/>
<wire x1="70.917" y1="51.552" x2="0" y2="51.552" width="0" layer="20"/>
<wire x1="0" y1="51.552" x2="0" y2="-0.254" width="0" layer="20"/>
<text>davewerld 2014</text>
<text>74hc595 rev 1</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TSSOP16">
<description>&lt;b&gt;TSOP16&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MINI">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun-DigitalIC" package="TSSOP16" value="74595"/>
<element name="IC2" library="SparkFun-DigitalIC" package="TSSOP16" value="74595"/>
<element name="R1" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R8" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R9" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R10" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R11" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R12" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R13" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R14" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R15" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="R16" library="adafruit" package="R0603" value="220">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED10" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED11" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED12" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED13" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED14" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED15" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED16" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Boards" package="ARDUINO_MINI" value="ARDUINO_MINI"/>
<element name="JP1" library="pinhead" package="1X03" value=""/>
<element name="R17" library="adafruit" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
</elements>
<signals>
<signal name="N$9">
<contactref element="IC1" pad="14"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="11"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="11"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="7"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="8"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="9"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="13"/>
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="LED10" pad="K"/>
<contactref element="LED11" pad="K"/>
<contactref element="LED12" pad="K"/>
<contactref element="LED13" pad="K"/>
<contactref element="LED14" pad="K"/>
<contactref element="LED15" pad="K"/>
<contactref element="LED16" pad="K"/>
<contactref element="R17" pad="2"/>
<contactref element="J1" pad="GND"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED5" pad="K"/>
<contactref element="LED6" pad="K"/>
<contactref element="LED7" pad="K"/>
<contactref element="LED8" pad="K"/>
<contactref element="LED9" pad="K"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC2" pad="10"/>
<contactref element="U$1" pad="21"/>
<contactref element="JP1" pad="2"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="N$19">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="17"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="15"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="5"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="7"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="15"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="3"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="IC2" pad="4"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC2" pad="5"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="IC2" pad="6"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="IC2" pad="7"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$25">
<contactref element="R2" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="R3" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$27">
<contactref element="R4" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$28">
<contactref element="R5" pad="2"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="R6" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$30">
<contactref element="R7" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$31">
<contactref element="R8" pad="2"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$32">
<contactref element="R9" pad="2"/>
<contactref element="LED9" pad="A"/>
</signal>
<signal name="N$33">
<contactref element="R10" pad="2"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="N$34">
<contactref element="R11" pad="2"/>
<contactref element="LED11" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="R12" pad="2"/>
<contactref element="LED12" pad="A"/>
</signal>
<signal name="N$36">
<contactref element="R13" pad="2"/>
<contactref element="LED13" pad="A"/>
</signal>
<signal name="N$37">
<contactref element="R14" pad="2"/>
<contactref element="LED14" pad="A"/>
</signal>
<signal name="N$38">
<contactref element="R15" pad="2"/>
<contactref element="LED15" pad="A"/>
</signal>
<signal name="N$39">
<contactref element="R16" pad="2"/>
<contactref element="LED16" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
