<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<circle x="48.26" y="36.83" radius="18.542" width="0.0254" layer="20"/>
<text>IN</text>
<text>QA</text>
<text>VCC</text>
<text>QB</text>
<text>QC</text>
<text>QD</text>
<text>QE</text>
<text>/OE</text>
<text>LAT</text>
<text>CLK</text>
<text>/RST</text>
<text>OUT</text>
<text>GND</text>
<text>QH</text>
<text>QG</text>
<text>QF</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="LilyPad-Wearables">
<packages>
<package name="PETAL-LONG-1-2SIDE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun-DigitalIC" package="SO16" value="74LS595D"/>
<element name="U$1" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$2" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$3" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$4" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$5" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$6" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$7" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$8" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$9" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$10" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$11" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$12" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$13" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$14" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$15" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
<element name="U$16" library="LilyPad-Wearables" package="PETAL-LONG-1-2SIDE" value="SEWTAP9"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="16"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="15"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="1"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="3"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="4"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="5"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="6"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="7"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="8"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="14"/>
<contactref element="U$11" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="11"/>
<contactref element="U$12" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="10"/>
<contactref element="U$13" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="12"/>
<contactref element="U$14" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="13"/>
<contactref element="U$15" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="9"/>
<contactref element="U$16" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
