<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="114.3" y2="0" width="0" layer="20"/>
<wire x1="114.3" y1="0" x2="114.3" y2="38.1" width="0" layer="20"/>
<wire x1="114.3" y1="38.1" x2="0" y2="38.1" width="0" layer="20"/>
<wire x1="0" y1="38.1" x2="0" y2="0" width="0" layer="20"/>
<text>github.com/dvdfreitag/2x6</text>
</plain>
<libraries>
<library name="Atmel">
<packages>
<package name="TQFP-32">
</package>
</packages>
</library>
<library name="Passives">
<packages>
<package name="0603-CAP">
</package>
<package name="FA-238">
</package>
<package name="1206-PTC">
</package>
<package name="0603-LED">
</package>
<package name="SOD-123">
</package>
<package name="OSHW">
</package>
<package name="TWITTER">
</package>
</packages>
</library>
<library name="Connectors">
<packages>
<package name="10118192-0001LF">
</package>
</packages>
</library>
<library name="Cherry-MX">
<packages>
<package name="CHERRY-MX">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Atmel" package="TQFP-32" value="ATMEGA32U2-TQFP32">
<attribute name="NAME"/>
</element>
<element name="C1" library="Passives" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="Y1" library="Passives" package="FA-238" value="16MHz">
<attribute name="NAME"/>
</element>
<element name="R1" library="Passives" package="0603-CAP" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="F1" library="Passives" package="1206-PTC" value="">
<attribute name="NAME"/>
</element>
<element name="J1" library="Connectors" package="10118192-0001LF" value="USB-MICROB-3">
<attribute name="NAME"/>
</element>
<element name="D1" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="C2" library="Passives" package="0603-CAP" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="Passives" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R2" library="Passives" package="0603-CAP" value="1.5kΩ">
<attribute name="NAME"/>
</element>
<element name="C4" library="Passives" package="0603-CAP" value="10pF">
<attribute name="NAME"/>
</element>
<element name="C5" library="Passives" package="0603-CAP" value="10pF">
<attribute name="NAME"/>
</element>
<element name="S1" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="D2" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="S2" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S3" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S4" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S5" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S6" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S7" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S8" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S9" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S10" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S11" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="S12" library="Cherry-MX" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="D3" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D4" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D5" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D6" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D7" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D8" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D9" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D10" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D11" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D12" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D13" library="Passives" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D14" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="R3" library="Passives" package="0603-CAP" value="1.5kΩ">
<attribute name="NAME"/>
</element>
<element name="D15" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="R4" library="Passives" package="0603-CAP" value="1.5kΩ">
<attribute name="NAME"/>
</element>
<element name="D16" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="R5" library="Passives" package="0603-CAP" value="1.5kΩ">
<attribute name="NAME"/>
</element>
<element name="D17" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="R6" library="Passives" package="0603-CAP" value="1.5kΩ">
<attribute name="NAME"/>
</element>
<element name="D18" library="Passives" package="0603-LED" value="">
<attribute name="NAME"/>
</element>
<element name="R7" library="Passives" package="0603-CAP" value="1.5kΩ">
<attribute name="NAME"/>
</element>
<element name="C6" library="Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="U$1" library="Passives" package="OSHW" value=""/>
<element name="U$2" library="Passives" package="TWITTER" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="P$6"/>
<contactref element="J1" pad="P$7"/>
<contactref element="J1" pad="P$8"/>
<contactref element="J1" pad="P$9"/>
<contactref element="J1" pad="P$10"/>
<contactref element="J1" pad="P$11"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="28"/>
<contactref element="R2" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="U1" pad="13"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="27"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="D_P">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="D_N">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="1"/>
<contactref element="F1" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="F1" pad="P$1"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="31"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="D18" pad="A"/>
<contactref element="D14" pad="A"/>
<contactref element="D15" pad="A"/>
<contactref element="D16" pad="A"/>
<contactref element="D17" pad="A"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="24"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="ROW0">
<contactref element="D2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="D7" pad="1"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="N$8">
<contactref element="S6" pad="S2"/>
<contactref element="S6" pad="S3"/>
<contactref element="D7" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="S5" pad="S2"/>
<contactref element="S5" pad="S3"/>
<contactref element="D6" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="S4" pad="S2"/>
<contactref element="S4" pad="S3"/>
<contactref element="D5" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="S3" pad="S2"/>
<contactref element="S3" pad="S3"/>
<contactref element="D4" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="S2" pad="S2"/>
<contactref element="S2" pad="S3"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="S1" pad="S2"/>
<contactref element="S1" pad="S3"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="ROW1">
<contactref element="D8" pad="1"/>
<contactref element="D9" pad="1"/>
<contactref element="D10" pad="1"/>
<contactref element="D11" pad="1"/>
<contactref element="D12" pad="1"/>
<contactref element="D13" pad="1"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$15">
<contactref element="S7" pad="S2"/>
<contactref element="S7" pad="S3"/>
<contactref element="D8" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="S8" pad="S2"/>
<contactref element="S8" pad="S3"/>
<contactref element="D9" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="S9" pad="S2"/>
<contactref element="S9" pad="S3"/>
<contactref element="D10" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="S10" pad="S2"/>
<contactref element="S10" pad="S3"/>
<contactref element="D11" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="S11" pad="S2"/>
<contactref element="S11" pad="S3"/>
<contactref element="D12" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="S12" pad="S2"/>
<contactref element="S12" pad="S3"/>
<contactref element="D13" pad="2"/>
</signal>
<signal name="COL0">
<contactref element="S7" pad="S1"/>
<contactref element="S7" pad="S4"/>
<contactref element="S1" pad="S1"/>
<contactref element="S1" pad="S4"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="COL1">
<contactref element="S8" pad="S1"/>
<contactref element="S8" pad="S4"/>
<contactref element="S2" pad="S1"/>
<contactref element="S2" pad="S4"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="COL2">
<contactref element="S9" pad="S1"/>
<contactref element="S9" pad="S4"/>
<contactref element="S3" pad="S1"/>
<contactref element="S3" pad="S4"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="COL3">
<contactref element="S10" pad="S1"/>
<contactref element="S10" pad="S4"/>
<contactref element="S4" pad="S1"/>
<contactref element="S4" pad="S4"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="COL4">
<contactref element="S11" pad="S1"/>
<contactref element="S11" pad="S4"/>
<contactref element="S5" pad="S1"/>
<contactref element="S5" pad="S4"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="COL5">
<contactref element="S12" pad="S1"/>
<contactref element="S12" pad="S4"/>
<contactref element="S6" pad="S1"/>
<contactref element="S6" pad="S4"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="D14" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="2"/>
<contactref element="D15" pad="C"/>
</signal>
<signal name="N$21">
<contactref element="R5" pad="2"/>
<contactref element="D16" pad="C"/>
</signal>
<signal name="N$22">
<contactref element="R6" pad="2"/>
<contactref element="D17" pad="C"/>
</signal>
<signal name="N$23">
<contactref element="R7" pad="2"/>
<contactref element="D18" pad="C"/>
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
</signals>
</board>
</drawing>
</eagle>
