<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>YEL</text>
<text>RED</text>
<text>BLK</text>
<hole x="56.6928" y="11.8872" drill="3.175"/>
<hole x="56.6928" y="26.1112" drill="3.175"/>
<hole x="40.513" y="31.3436" drill="3.175"/>
<hole x="19.5072" y="38.989" drill="3.175"/>
<text>LASER</text>
<text>+</text>
<text>-</text>
<text>TMP/HMD</text>
<text>FLYPEZ_J005412A</text>
<text>GATE</text>
<text>SWEEP</text>
<text>20190422</text>
<text>S</text>
<text>S</text>
<wire x1="59.6392" y1="28.3972" x2="59.6392" y2="7.9756" width="0" layer="20"/>
<wire x1="0" y1="14.986" x2="0" y2="35.56" width="0" layer="20"/>
<text>LIN_ARRAY</text>
<wire x1="25.4" y1="40.894" x2="21.8186" y2="30.9626" width="0" layer="20"/>
<wire x1="21.8186" y1="30.9626" x2="28.0162" y2="28.7274" width="0" layer="20"/>
<wire x1="28.0162" y1="28.7274" x2="31.5976" y2="38.6588" width="0" layer="20"/>
<wire x1="31.5976" y1="38.6588" x2="59.6392" y2="28.3972" width="0" layer="20"/>
<wire x1="59.6392" y1="7.9756" x2="0" y2="14.986" width="0" layer="20" curve="-82.37185"/>
<text>LED/TEM CONTROL</text>
<wire x1="13.5128" y1="35.56" x2="0" y2="35.56" width="0" layer="20"/>
<wire x1="25.4" y1="40.894" x2="16.6624" y2="44.069" width="0" layer="20"/>
<wire x1="16.6624" y1="44.069" x2="13.5128" y2="35.56" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
</packages>
</library>
<library name="STEVES_BU">
<packages>
<package name="CON5_DF13_STTH">
</package>
<package name="1206S">
</package>
<package name="0805S">
</package>
<package name="PRECON_SENSOR">
</package>
<package name="LOGO_BMP_OP">
</package>
<package name="AMPMODU6">
</package>
<package name="SOT23-6">
</package>
<package name="SOIC8">
</package>
<package name="AMPMODU-2">
</package>
</packages>
</library>
<library name="Teensy_3_and_LC_Series_Boards_v1.4">
<packages>
<package name="TEENSY_3.0-3.2&amp;LC_DIL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="STEVES_BU" package="CON5_DF13_STTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="STEVES_BU" package="1206S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="STEVES_BU" package="1206S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="STEVES_BU" package="0805S" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="STEVES_BU" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="STEVES_BU" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="STEVES_BU" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="STEVES_BU" package="0805S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="STEVES_BU" package="AMPMODU-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="STEVES_BU" package="PRECON_SENSOR" value="PRECON_SENSOR"/>
<element name="U$1" library="STEVES_BU" package="LOGO_BMP_OP" value="JFRC-LOGOLOGO_OP"/>
<element name="J1" library="STEVES_BU" package="AMPMODU6" value="CON6AMPMODU6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="STEVES_BU" package="SOT23-6" value="SIP32431">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="STEVES_BU" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M1" library="Teensy_3_and_LC_Series_Boards_v1.4" package="TEENSY_3.0-3.2&amp;LC_DIL" value="TEENSY_3.1-3.2_DIL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="STEVES_BU" package="SOIC8" value="TMP75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="STEVES_BU" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="STEVES_BU" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="STEVES_BU" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="STEVES_BU" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="M1" pad="GND"/>
<contactref element="U2" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="+5VS">
<contactref element="JP2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="+5VD">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="M1" pad="VIN"/>
</signal>
<signal name="AGND">
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="M1" pad="AGND"/>
<contactref element="J2" pad="P$3"/>
</signal>
<signal name="T/H">
<contactref element="U$2" pad="P$3"/>
<contactref element="M1" pad="0"/>
</signal>
<signal name="ACLK">
<contactref element="M1" pad="16/A2"/>
<contactref element="J2" pad="P$4"/>
</signal>
<signal name="ASYN">
<contactref element="M1" pad="15/A1"/>
<contactref element="J2" pad="P$5"/>
</signal>
<signal name="+3V3">
<contactref element="C5" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="M1" pad="3.3V"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="C6" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="+3V3A">
<contactref element="R2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="J2" pad="P$1"/>
</signal>
<signal name="SWEEP">
<contactref element="JP1" pad="1"/>
<contactref element="M1" pad="9"/>
</signal>
<signal name="GATE">
<contactref element="JP2" pad="1"/>
<contactref element="M1" pad="10"/>
</signal>
<signal name="AOUT">
<contactref element="M1" pad="14/A0"/>
<contactref element="J2" pad="P$2"/>
</signal>
<signal name="PELTIER">
<contactref element="J1" pad="1"/>
<contactref element="M1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="4"/>
<contactref element="M1" pad="11"/>
</signal>
<signal name="SCLK">
<contactref element="J1" pad="5"/>
<contactref element="M1" pad="13"/>
</signal>
<signal name="CS">
<contactref element="J1" pad="3"/>
<contactref element="M1" pad="8"/>
</signal>
<signal name="ENABLE">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="M1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="M1" pad="18/A4"/>
<contactref element="R5" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="M1" pad="19/A5"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="M1" pad="20/A6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
