<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="65" y2="0" width="0" layer="20"/>
<wire x1="65" y1="0" x2="65" y2="50" width="0" layer="20"/>
<wire x1="65" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>SIG</text>
<text>SIG</text>
<text>SIG</text>
<text>SIG</text>
<text>SIG</text>
<text>SIG</text>
<text>S10</text>
<text>S11</text>
<text>S09</text>
<text>S08</text>
<text>S07</text>
<text>S06</text>
<text>S00</text>
<text>S01</text>
<text>S02</text>
<text>S03</text>
<text>S05</text>
<text>S04</text>
</plain>
<libraries>
<library name="RPI-Zero">
<description>Generated from &lt;b&gt;TMC2660-test-with-grbl.brd&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-2.5MM-5MM">
<description>2.5 mm spaced PTHs with 5 mm diameter outline and standard solder mask</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SPARKFUN_PRO_MICRO">
<description>&lt;h3&gt;SparkFun Pro Mico Footprint (with USB connector)&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 24&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:0.7x1.3"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Pro Micro&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electromechanical Parts&lt;/h3&gt;
This library contains electromechanical devices, like motors, speakers,servos, and relays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
<description>&lt;h3&gt;3-Pin Header&lt;/h3&gt;
&lt;p&gt;0.1"-spaced 3-pin header. 
&lt;ul&gt;&lt;li&gt;Drill diameter: 40 mil&lt;/li&gt;
&lt;li&gt;Copper diameter: 74 mil&lt;/li&gt;&lt;/ul&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;SERVO&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="RPI-Zero" package="RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL" value="RPI-ZERO"/>
<element name="C3" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="B1" library="SparkFun-Boards" package="SPARKFUN_PRO_MICRO" value="SPARKFUN_PRO_MICRO"/>
<element name="M1" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M2" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M3" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M4" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M5" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M6" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M7" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M8" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M9" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M10" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M11" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="M12" library="SparkFun-Electromechanical" package="1X03" value="SERVO"/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="39"/>
<contactref element="U$1" pad="25"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="30"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="B1" pad="4"/>
<contactref element="B1" pad="23"/>
<contactref element="B1" pad="3"/>
<contactref element="M1" pad="3"/>
<contactref element="M2" pad="3"/>
<contactref element="M3" pad="3"/>
<contactref element="M4" pad="3"/>
<contactref element="M5" pad="3"/>
<contactref element="M6" pad="3"/>
<contactref element="M7" pad="3"/>
<contactref element="M8" pad="3"/>
<contactref element="M9" pad="3"/>
<contactref element="M10" pad="3"/>
<contactref element="M11" pad="3"/>
<contactref element="M12" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="M1" pad="2"/>
<contactref element="M2" pad="2"/>
<contactref element="M3" pad="2"/>
<contactref element="M4" pad="2"/>
<contactref element="M5" pad="2"/>
<contactref element="M6" pad="2"/>
<contactref element="M7" pad="2"/>
<contactref element="M8" pad="2"/>
<contactref element="M9" pad="2"/>
<contactref element="M10" pad="2"/>
<contactref element="M11" pad="2"/>
<contactref element="M12" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="RAW">
<contactref element="B1" pad="24"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="1"/>
<contactref element="B1" pad="21"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="S3">
<contactref element="M1" pad="1"/>
<contactref element="B1" pad="10"/>
</signal>
<signal name="S2">
<contactref element="M2" pad="1"/>
<contactref element="B1" pad="9"/>
</signal>
<signal name="S1">
<contactref element="M3" pad="1"/>
<contactref element="B1" pad="8"/>
</signal>
<signal name="S0">
<contactref element="M4" pad="1"/>
<contactref element="B1" pad="7"/>
</signal>
<signal name="S4">
<contactref element="M8" pad="1"/>
<contactref element="B1" pad="11"/>
</signal>
<signal name="S5">
<contactref element="M7" pad="1"/>
<contactref element="B1" pad="12"/>
</signal>
<signal name="S6">
<contactref element="M6" pad="1"/>
<contactref element="B1" pad="18"/>
</signal>
<signal name="S7">
<contactref element="M5" pad="1"/>
<contactref element="B1" pad="17"/>
</signal>
<signal name="S11">
<contactref element="M9" pad="1"/>
<contactref element="B1" pad="13"/>
</signal>
<signal name="S10">
<contactref element="M10" pad="1"/>
<contactref element="B1" pad="14"/>
</signal>
<signal name="S9">
<contactref element="M11" pad="1"/>
<contactref element="B1" pad="15"/>
</signal>
<signal name="S8">
<contactref element="M12" pad="1"/>
<contactref element="B1" pad="16"/>
</signal>
<signal name="SDA">
<contactref element="B1" pad="5"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="B1" pad="6"/>
<contactref element="U$1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
