<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="41.58" y2="0" width="0" layer="20"/>
<wire x1="41.58" y1="0" x2="41.58" y2="24.12" width="0" layer="20"/>
<wire x1="41.58" y1="24.12" x2="0" y2="24.12" width="0" layer="20"/>
<wire x1="0" y1="24.12" x2="0" y2="0" width="0" layer="20"/>
<text>1</text>
<text>SO16 Adapter</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>use solder bridge to connect ground pin</text>
<text>Free for non
commercial use</text>
</plain>
<libraries>
<library name="phils">
<packages>
<package name="SOP16">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
<package name="1X16/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="SJ-NO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="phils" package="SOP16" value="CH340G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="phils" package="1X16/90" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ2" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ3" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ4" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ5" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ6" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ7" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ8" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ9" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ10" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ11" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ12" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ13" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ14" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ15" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
<element name="SJ16" library="SparkFun" package="SJ-NO" value="SOLDERJUMPERNO"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="8"/>
<contactref element="SJ9" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="10"/>
<contactref element="SJ7" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="11"/>
<contactref element="SJ6" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="5"/>
<contactref element="JP1" pad="12"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="13"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="3"/>
<contactref element="JP1" pad="14"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="10"/>
<contactref element="JP1" pad="7"/>
<contactref element="SJ10" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="11"/>
<contactref element="JP1" pad="6"/>
<contactref element="SJ11" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="12"/>
<contactref element="JP1" pad="5"/>
<contactref element="SJ12" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="13"/>
<contactref element="JP1" pad="4"/>
<contactref element="SJ13" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="9"/>
<contactref element="SJ8" pad="2"/>
</signal>
<signal name="GND">
<contactref element="SJ1" pad="1"/>
<contactref element="SJ16" pad="1"/>
<contactref element="SJ15" pad="1"/>
<contactref element="SJ14" pad="1"/>
<contactref element="SJ13" pad="1"/>
<contactref element="SJ12" pad="1"/>
<contactref element="SJ11" pad="1"/>
<contactref element="SJ10" pad="1"/>
<contactref element="SJ9" pad="1"/>
<contactref element="SJ8" pad="1"/>
<contactref element="SJ7" pad="1"/>
<contactref element="SJ6" pad="1"/>
<contactref element="SJ5" pad="1"/>
<contactref element="SJ4" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="COMM">
<contactref element="IC1" pad="15"/>
<contactref element="JP1" pad="2"/>
<contactref element="SJ15" pad="2"/>
</signal>
<signal name="SW2">
<contactref element="IC1" pad="2"/>
<contactref element="JP1" pad="15"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="SW1">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="16"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="Q1">
<contactref element="IC1" pad="16"/>
<contactref element="JP1" pad="1"/>
<contactref element="SJ16" pad="2"/>
</signal>
<signal name="Q2">
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="3"/>
<contactref element="SJ14" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
