<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0.3302" y1="0.0762" x2="18.7706" y2="0.0762" width="0.2032" layer="20"/>
<wire x1="18.7706" y1="0.0762" x2="18.796" y2="21.0312" width="0.2032" layer="20"/>
<wire x1="18.796" y1="21.0312" x2="0.3556" y2="21.0312" width="0.2032" layer="20"/>
<wire x1="0.3556" y1="21.0312" x2="0.3302" y2="0.0762" width="0.2032" layer="20"/>
<text>RFM69CW Breakout
Rev. 2 - 1/28/2017</text>
<text>915MHz</text>
<text>ANT</text>
<text>3V3</text>
<text>GND</text>
<text>MOSI</text>
<text>SCK</text>
<text>NSS</text>
<text>DIO0</text>
<text>MISO</text>
<text>GND</text>
<text>ANT</text>
<text>GND</text>
<text>ANT</text>
<text>GND</text>
<text>GND</text>
<text>3V3</text>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>NSS</text>
<text>DIO0</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun RF, WiFi, Cellular, and Bluetooth&lt;/h3&gt;
In this library you'll find things that send or receive RF-- cellular modules, Bluetooth, WiFi, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RFM69CW-XXXS2">
<description>&lt;h3&gt;Hope RF RFM69CW RF Transciever&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM69CW-V1.1.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANT" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-RF" package="RFM69CW-XXXS2" value="915MHz">
<attribute name="PROD_ID" value="IC-11996"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ANT">
<contactref element="U1" pad="1"/>
<contactref element="ANT" pad="1"/>
</signal>
<signal name="DIO0">
<contactref element="U1" pad="9"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="2"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="8"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="5"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="6"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="NSS">
<contactref element="U1" pad="7"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="3"/>
<contactref element="J4" pad="8"/>
<contactref element="GND" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
