<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="6.604" x2="-0.254" y2="1.016" width="0" layer="20"/>
<wire x1="-0.254" y1="1.016" x2="1.016" y2="-0.254" width="0" layer="20" curve="90"/>
<wire x1="1.016" y1="-0.254" x2="11.684" y2="-0.254" width="0" layer="20"/>
<wire x1="11.684" y1="-0.254" x2="12.954" y2="1.016" width="0" layer="20" curve="90"/>
<wire x1="12.954" y1="1.016" x2="12.954" y2="6.604" width="0" layer="20"/>
<wire x1="12.954" y1="6.604" x2="11.684" y2="7.874" width="0" layer="20" curve="90"/>
<wire x1="11.684" y1="7.874" x2="1.016" y2="7.874" width="0" layer="20"/>
<wire x1="1.016" y1="7.874" x2="-0.254" y2="6.604" width="0" layer="20" curve="90"/>
<text>&gt;VERSION</text>
<text>5V</text>
<text>SDA</text>
<text>SCL</text>
<text>3V</text>
<text>SDA</text>
<text>SCL</text>
<text>i c</text>
<text>2</text>
<text>by &lt;sean@yak.net&gt;</text>
<text>LEVEL</text>
<text>SHIFTER</text>
</plain>
<libraries>
<library name="A_butts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
</packages>
</library>
<library name="a_parts">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="1X03-CENTERED">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v2.2"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="A_butts" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value="v2.2"/>
<attribute name="DESIGNER" value="sean@yak.net"/>
</element>
<element name="Q2" library="a_parts" package="SOT23" value="IRLML2502">
<attribute name="NAME"/>
</element>
<element name="Q1" library="a_parts" package="SOT23" value="IRLML2502">
<attribute name="NAME"/>
</element>
<element name="R1" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
</element>
<element name="R2" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
</element>
<element name="R3" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
</element>
<element name="R4" library="a_parts" package="R0603" value="4K7">
<attribute name="NAME"/>
</element>
<element name="LV" library="a_parts" package="1X03-CENTERED" value="M03PTH-CENTERED"/>
<element name="HV" library="a_parts" package="1X03-CENTERED" value="M03PTH-CENTERED"/>
</elements>
<signals>
<signal name="5V">
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="HV" pad="2"/>
</signal>
<signal name="SCL_3V3">
<contactref element="Q2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="LV" pad="1"/>
</signal>
<signal name="SDA_3V3">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="LV" pad="3"/>
</signal>
<signal name="SCL_5V">
<contactref element="Q2" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="HV" pad="1"/>
</signal>
<signal name="SDA_5V">
<contactref element="Q1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="HV" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="LV" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
