<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0.9525" y1="19.3675" x2="0.9525" y2="0.965" width="0" layer="20"/>
<wire x1="0.9525" y1="0.965" x2="21.8975" y2="0.965" width="0" layer="20"/>
<wire x1="21.8975" y1="0.965" x2="21.8975" y2="19.3675" width="0" layer="20"/>
<wire x1="21.8975" y1="19.3675" x2="0.9525" y2="19.3675" width="0" layer="20"/>
<text>ESP8266, ESP-03
Breakout board
(c) Mats Karlsson, 2015</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_SMD">
</package>
</packages>
</library>
<library name="#ESP8266">
<packages>
<package name="ESP-03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="SparkFun-Connectors" package="1X08_SMD" value="">
<attribute name="PROD_ID" value="CONN-10204"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="#ESP8266" package="ESP-03" value="ESP8266-03"/>
<element name="JP1" library="SparkFun-Connectors" package="1X08_SMD" value="">
<attribute name="PROD_ID" value="CONN-10204"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GPIO0">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="GPIO0"/>
</signal>
<signal name="GPIO2">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="GPIO2"/>
</signal>
<signal name="GPIO15">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="GPIO15"/>
</signal>
<signal name="GPIO13">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="GPIO13"/>
</signal>
<signal name="GPIO12">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="GPIO12"/>
</signal>
<signal name="GPIO14">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="GPIO14"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="VCC"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="NC">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="NC"/>
</signal>
<signal name="TXD">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="UTXD"/>
</signal>
<signal name="RXD">
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="URXD"/>
</signal>
<signal name="GPIO18">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="GPIO18"/>
</signal>
<signal name="CH_PD">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="CH_PD"/>
</signal>
<signal name="ANT">
<contactref element="JP2" pad="7"/>
<contactref element="U$1" pad="ANT"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
