<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>RL</text>
<text>GND</text>
<text>3.3</text>
<text>OUT</text>
<text>IN+</text>
<wire x1="41.529" y1="57.785" x2="41.402" y2="57.658" width="0.1524" layer="20"/>
<wire x1="41.402" y1="57.658" x2="39.37" y2="55.626" width="0.1524" layer="20"/>
<wire x1="39.37" y1="55.626" x2="39.37" y2="26.924" width="0.1524" layer="20"/>
<wire x1="39.37" y1="26.924" x2="41.402" y2="24.892" width="0.1524" layer="20"/>
<wire x1="41.402" y1="24.892" x2="68.707" y2="24.892" width="0.1524" layer="20"/>
<wire x1="68.707" y1="24.892" x2="70.866" y2="27.051" width="0.1524" layer="20"/>
<wire x1="70.866" y1="27.051" x2="70.866" y2="55.499" width="0.1524" layer="20"/>
<wire x1="70.866" y1="55.499" x2="68.326" y2="58.039" width="0.1524" layer="20"/>
<wire x1="68.326" y1="58.039" x2="41.783" y2="58.039" width="0.1524" layer="20"/>
<wire x1="41.783" y1="58.039" x2="41.529" y2="57.785" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="02016D105MAT2A">
<packages>
<package name="CAPC0603X33N">
</package>
</packages>
</library>
<library name="F980J476MSA">
<packages>
<package name="CAPC2012X140N">
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="06P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="AD8232">
<packages>
<package name="LFCSP_20">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603" value=".33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="02016D105MAT2A" package="CAPC0603X33N" value="02016D105MAT2A">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 1 µF ±20% 6.3V Ceramic Capacitor X5R 0201 (0603 Metric) "/>
<attribute name="MF" value="KYOCERA AVX"/>
<attribute name="MP" value="02016D105MAT2A"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/02016D105MAT2A/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-07886"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="F980J476MSA" package="CAPC2012X140N" value="F980J476MSA">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 47 µF Molded Tantalum Capacitors 6.3 V 0805 (2012 Metric) 6Ohm "/>
<attribute name="MF" value="AVX"/>
<attribute name="MP" value="F980J476MSA"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SMD-2 AVX"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/F980J476MSA/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="con-amp-quick" package="03P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="12"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="con-amp-quick" package="06P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="5"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="280k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603" value="10M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="180k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="180k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="360k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="10M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603" value="10M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603" value="0">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0603" value="0">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0603" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07868"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1000k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="1500k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08269"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="2000k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08269"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="10000k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07868"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="10000k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07868"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="0">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="0">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="10M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="AD8232" package="LFCSP_20" value="AD8232">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" AD8232 Analog Front End Evaluation Board "/>
<attribute name="MF" value="Analog Devices, Inc."/>
<attribute name="MP" value="AD8232"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/AD8232/?ref=eda"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="9"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="10"/>
<contactref element="C1" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="20"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="8"/>
<contactref element="R1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R12" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="R11" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="+IN">
<contactref element="R11" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="R13" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="17"/>
<contactref element="R14" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U$1" pad="15"/>
<contactref element="R7" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R17" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="16"/>
<contactref element="C5" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U$1" pad="PAD"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="RL">
<contactref element="R13" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R14" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="N$20">
<contactref element="R5" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="C7" pad="2"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$15">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$21">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$22">
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
