<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>-</text>
<wire x1="12.065" y1="0" x2="1.15061875" y2="10.91438125" width="0.025" layer="20"/>
<wire x1="0" y1="50.15738125" x2="0" y2="10.91438125" width="0.025" layer="20"/>
<wire x1="1.408" y1="48.719" x2="1.408" y2="48.679" width="0.025" layer="20"/>
<wire x1="1.408" y1="43.269" x2="1.408" y2="43.229" width="0.025" layer="20"/>
<wire x1="2.608" y1="43.229" x2="2.608" y2="43.269" width="0.025" layer="20"/>
<wire x1="2.608" y1="48.679" x2="2.608" y2="48.719" width="0.025" layer="20"/>
<wire x1="3.175" y1="58.293" x2="3.175" y2="51.17338125" width="0.025" layer="20"/>
<wire x1="3.175" y1="51.17338125" x2="2.159" y2="50.15738125" width="0.025" layer="20"/>
<wire x1="12.065" y1="0" x2="91.44" y2="0" width="0.025" layer="20"/>
<wire x1="3.175" y1="58.293" x2="31.115" y2="66.675" width="0.025" layer="20"/>
<wire x1="0" y1="10.91438125" x2="1.15061875" y2="10.91438125" width="0.025" layer="20"/>
<wire x1="91.44" y1="20.12195" x2="85.09" y2="20.12195" width="0.025" layer="20"/>
<wire x1="46.53788125" y1="74.295" x2="46.53788125" y2="66.675" width="0.025" layer="20"/>
<wire x1="1.738" y1="42.899" x2="2.278" y2="42.899" width="0.025" layer="20"/>
<wire x1="4.843" y1="43.219" x2="5.233" y2="43.219" width="0.025" layer="20"/>
<wire x1="2.278" y1="43.599" x2="1.738" y2="43.599" width="0.025" layer="20"/>
<wire x1="5.233" y1="43.879" x2="4.843" y2="43.879" width="0.025" layer="20"/>
<wire x1="4.843" y1="48.069" x2="5.233" y2="48.069" width="0.025" layer="20"/>
<wire x1="1.738" y1="48.349" x2="2.278" y2="48.349" width="0.025" layer="20"/>
<wire x1="5.233" y1="48.729" x2="4.843" y2="48.729" width="0.025" layer="20"/>
<wire x1="2.278" y1="49.049" x2="1.738" y2="49.049" width="0.025" layer="20"/>
<wire x1="2.159" y1="50.15738125" x2="0" y2="50.15738125" width="0.025" layer="20"/>
<wire x1="31.115" y1="66.675" x2="46.53788125" y2="66.675" width="0.025" layer="20"/>
<wire x1="85.09" y1="58.58261875" x2="85.09" y2="20.12195" width="0.025" layer="20"/>
<wire x1="69.37761875" y1="74.295" x2="46.53788125" y2="74.295" width="0.025" layer="20"/>
<wire x1="69.37761875" y1="74.295" x2="85.09" y2="58.58261875" width="0.025" layer="20"/>
<wire x1="91.44" y1="0" x2="91.44" y2="20.12195" width="0.025" layer="20"/>
<wire x1="2.278" y1="48.349" x2="2.608" y2="48.679" width="0.025" layer="20" curve="90"/>
<wire x1="1.408" y1="48.679" x2="1.738" y2="48.349" width="0.025" layer="20" curve="90"/>
<wire x1="1.738" y1="49.049" x2="1.408" y2="48.719" width="0.025" layer="20" curve="90"/>
<wire x1="2.608" y1="48.719" x2="2.278" y2="49.049" width="0.025" layer="20" curve="90"/>
<wire x1="2.278" y1="42.899" x2="2.608" y2="43.229" width="0.025" layer="20" curve="90"/>
<wire x1="1.408" y1="43.229" x2="1.738" y2="42.899" width="0.025" layer="20" curve="90"/>
<wire x1="1.738" y1="43.599" x2="1.408" y2="43.269" width="0.025" layer="20" curve="90"/>
<wire x1="2.608" y1="43.269" x2="2.278" y2="43.599" width="0.025" layer="20" curve="90"/>
<wire x1="4.843" y1="43.879" x2="4.843" y2="43.219" width="0.025" layer="20" curve="180"/>
<wire x1="5.233" y1="43.219" x2="5.233" y2="43.879" width="0.025" layer="20" curve="180"/>
<wire x1="4.843" y1="48.729" x2="4.843" y2="48.069" width="0.025" layer="20" curve="180"/>
<wire x1="5.233" y1="48.069" x2="5.233" y2="48.729" width="0.025" layer="20" curve="180"/>
<hole x="9.5" y="40" drill="3.6576"/>
<hole x="12.065" y="8.89" drill="3.6576"/>
<hole x="24.765" y="60.96" drill="3.6576"/>
<hole x="52.07" y="70.993" drill="3.6576"/>
<hole x="86.995" y="4.1275" drill="3.6576"/>
<text>Offboard Parts</text>
<text>Airbeam</text>
<text>v1.0</text>
<wire x1="5.81025" y1="33.75025" x2="5.81025" y2="23.59025" width="2.54" layer="20"/>
<wire x1="13.43025" y1="23.59025" x2="13.43025" y2="33.75025" width="2.54" layer="20"/>
<wire x1="5.81025" y1="23.59025" x2="13.43025" y2="23.59025" width="2.54" layer="20"/>
<wire x1="13.43025" y1="33.75025" x2="5.81025" y2="33.75025" width="2.54" layer="20"/>
</plain>
<libraries>
<library name="SmartPrj">
<packages>
<package name="TQFP44-PAD">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
<package name="FIDUCIA-MOUNT">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="QFN44ML7X7">
</package>
</packages>
</library>
<library name="varistor">
<packages>
<package name="CT/CN0603">
<description>&lt;b&gt;EPCOS SMD Varistors, MLV; Standard Series&lt;/b&gt;&lt;p&gt;
Source: www.farnell.com/datasheets/49238.pdf</description>
</package>
</packages>
</library>
<library name="Airbeam">
<packages>
<package name="BT_NVC-MDCS42A">
</package>
<package name="RHT03">
</package>
<package name="S4B-EH">
</package>
<package name="EAGLE_FREESPACE">
</package>
<package name="USB-FCI">
</package>
<package name="WFDFN-10">
</package>
<package name="SOT23-5">
</package>
<package name="SOT23">
</package>
<package name="SOD123_DIODE">
</package>
<package name="PUSHBUTTON">
</package>
<package name="LED_550">
</package>
<package name="CON_5_2MM">
</package>
<package name="SWITCH_TACTILE">
</package>
<package name="UFDFN-8">
</package>
<package name="EMPTY">
</package>
<package name="U_FB1">
</package>
<package name="MSOP-8">
</package>
<package name="2917_CAP">
</package>
<package name="JST-0.8MM">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
<package name="1210">
</package>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PTC-1206-WIDE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CON_ICSP" library="SmartPrj" package="2X03" value="ICSP">
<attribute name="NAME"/>
<attribute name="PARTNO" value="67997-206HLF "/>
</element>
<element name="FID1" library="SmartPrj" package="FIDUCIA-MOUNT" value="FIDUCIALMOUNT">
<attribute name="PARTNO" value="DNP"/>
</element>
<element name="FID2" library="SmartPrj" package="FIDUCIA-MOUNT" value="FIDUCIALMOUNT">
<attribute name="PARTNO" value="DNP"/>
</element>
<element name="FID3" library="SmartPrj" package="FIDUCIA-MOUNT" value="FIDUCIALMOUNT">
<attribute name="PARTNO" value="DNP"/>
</element>
<element name="U_Z1" library="varistor" package="CT/CN0603" value="CG0603MLC-05E">
<attribute name="PARTNO" value="CG0603MLC-05E"/>
<attribute name="NAME"/>
</element>
<element name="U_Z2" library="varistor" package="CT/CN0603" value="CG0603MLC-05E">
<attribute name="PARTNO" value="CG0603MLC-05E"/>
</element>
<element name="UC_C2" library="SparkFun-Passives" package="0603-CAP" value="100n">
<attribute name="PARTNO" value="C1608X7R1E104K080AA"/>
<attribute name="NAME"/>
</element>
<element name="UC_C1" library="SparkFun-Passives" package="0603-CAP" value="100n">
<attribute name="PARTNO" value="C1608X7R1E104K080AA"/>
<attribute name="NAME"/>
</element>
<element name="U_MEGA32U-Q" library="SmartPrj" package="QFN44ML7X7" value="DNP">
<attribute name="PARTNO" value="DNP"/>
</element>
<element name="ATMEGA32U4-T" library="SmartPrj" package="TQFP44-PAD" value="ATMEGA32U4-XUAU">
<attribute name="PARTNO" value="AtMega32U4-XUAU"/>
</element>
<element name="UBT" library="Airbeam" package="BT_NVC-MDCS42A" value="BT-NVC-MDCS42A">
<attribute name="PARTNO" value="NVC-MDCS42A"/>
<attribute name="NAME"/>
</element>
<element name="U_TEMP-HUM" library="Airbeam" package="RHT03" value="RHT03">
<attribute name="PARTNO" value="RHT03 "/>
<attribute name="NAME"/>
</element>
<element name="U$6" library="Airbeam" package="EAGLE_FREESPACE" value=""/>
<element name="CON_USB" library="Airbeam" package="USB-FCI" value="USB-FCI">
<attribute name="PARTNO" value="10103594-0001LF"/>
</element>
<element name="UC_CRYSTAL" library="SparkFun-FreqCtrl" package="HC49UP" value="16MHz">
<attribute name="PARTNO" value="ECS-160-20-3X-TR "/>
<attribute name="NAME"/>
</element>
<element name="U_R1" library="SparkFun-Passives" package="0603-RES" value="22">
<attribute name="PARTNO" value="RC0603JR-0722RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_R2" library="SparkFun-Passives" package="0603-RES" value="22">
<attribute name="PARTNO" value="RC0603JR-0722RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_VR3" library="Airbeam" package="WFDFN-10" value="VREG-RTEC6150">
<attribute name="PARTNO" value="RT6150BGQW"/>
<attribute name="NAME"/>
</element>
<element name="VR3_C1" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
</element>
<element name="VR3_R1" library="SparkFun-Resistors" package="0603-RES" value="487k">
<attribute name="PARTNO" value="ERJ-3EKF4873V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR3_R2" library="SparkFun-Resistors" package="0603-RES" value="86.6k">
<attribute name="PARTNO" value="ERJ-3EKF8662V"/>
<attribute name="NAME"/>
</element>
<element name="VR3_L1" library="SparkFun-Passives" package="1210" value="2.2uH">
<attribute name="PARTNO" value="BRL3225T2R2M"/>
<attribute name="NAME"/>
</element>
<element name="U_VR5" library="Airbeam" package="WFDFN-10" value="VREG-RTEC6150">
<attribute name="PARTNO" value="RT6150BGQW"/>
<attribute name="NAME"/>
</element>
<element name="VR5_C1" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR5_R1" library="SparkFun-Resistors" package="0603-RES" value="487k">
<attribute name="PARTNO" value="ERJ-3EKF4873V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR5_R2" library="SparkFun-Resistors" package="0603-RES" value="53.6k">
<attribute name="PARTNO" value="RC0805FR-0753K6L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR5_L1" library="SparkFun-Passives" package="1210" value="6uH">
<attribute name="PARTNO" value="NRS5020T6R8MMGJ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR5_C2" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR5_C3" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR3_C2" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR3_C3" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON_BAT" library="SparkFun-Connectors" package="JST-2-SMD" value="CON_BAT">
<attribute name="PROD_ID" value="CONN-08352"/>
<attribute name="PARTNO" value="S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_LED_CH" library="SparkFun-Passives" package="0603-RES" value="1.4k">
<attribute name="PARTNO" value="RC0603FR-071K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UR_R2" library="SparkFun-Passives" package="0603-RES" value="6.65k">
<attribute name="PARTNO" value="RC0603FR-076K65L "/>
<attribute name="NAME"/>
</element>
<element name="VR_D1" library="Airbeam" package="SOD123_DIODE" value="DIODESOD123">
<attribute name="PARTNO" value="B130LAW-7-F"/>
<attribute name="NAME"/>
</element>
<element name="VR_R1" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="PARTNO" value="RC0603JR-0710KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VDETECT" library="Airbeam" package="SOT23" value="VDETEC_APX">
<attribute name="PARTNO" value="APX809-31SAG-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_ONOFF" library="Airbeam" package="PUSHBUTTON" value="PUSHBUTTON">
<attribute name="PARTNO" value="LC2259EENP"/>
<attribute name="NAME"/>
</element>
<element name="VR_R2" library="SparkFun-Resistors" package="0603-RES" value="487k">
<attribute name="PARTNO" value="ERJ-3EKF4873V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR_R3" library="SparkFun-Resistors" package="0603-RES" value="DNP">
<attribute name="PARTNO" value="RC0603JR-070RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON_DUST" library="Airbeam" package="S4B-EH" value="CON_DUST">
<attribute name="PARTNO" value="S4B-EH"/>
<attribute name="NAME"/>
</element>
<element name="LED_CH" library="Airbeam" package="LED_550" value="LED">
<attribute name="PARTNO" value="550-1307F"/>
<attribute name="NAME"/>
</element>
<element name="UC_R3" library="SparkFun-Passives" package="0603-RES" value="DNP">
<attribute name="PARTNO" value="RC0603JR-070RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UC_R1" library="SparkFun-Passives" package="0603-RES" value="1M">
<attribute name="PARTNO" value="RC0603FR-071ML"/>
<attribute name="NAME"/>
</element>
<element name="UC_R2" library="SparkFun-Passives" package="0603-RES" value="10k">
<attribute name="PARTNO" value="RC0603JR-0710KL"/>
<attribute name="NAME"/>
</element>
<element name="U_C1" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_C2" library="SparkFun-Passives" package="0603-CAP" value="100nF">
<attribute name="PARTNO" value="C1608X7R1E104K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UC_C7" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="PARTNO" value="C1608X5R1C105K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UC_C5" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="PARTNO" value="C1608X5R1C105K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UC_C6" library="SparkFun-Passives" package="0603-CAP" value="100nF">
<attribute name="PARTNO" value="C1608X7R1E104K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UC_C4" library="SparkFun-Passives" package="0603-CAP" value="20pF">
<attribute name="PARTNO" value="CL10C200JB8NNNC"/>
<attribute name="NAME"/>
</element>
<element name="UC_C3" library="SparkFun-Passives" package="0603-CAP" value="20pF">
<attribute name="PARTNO" value="CL10C200JB8NNNC"/>
<attribute name="NAME"/>
</element>
<element name="UC_R4" library="SparkFun-Passives" package="0603-RES" value="10k">
<attribute name="PARTNO" value="RC0603JR-0710KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR_R4" library="SparkFun-Resistors" package="0603-RES" value="0">
<attribute name="PARTNO" value="RC0603JR-070RL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_LED_BT" library="SparkFun-Passives" package="0603-RES" value="1.4k">
<attribute name="PARTNO" value="RC0603FR-071K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_BT" library="Airbeam" package="LED_550" value="LED">
<attribute name="PARTNO" value="550-1107F "/>
<attribute name="NAME"/>
</element>
<element name="VR_MOS-P1" library="Airbeam" package="SOT23" value="MOSFET-P">
<attribute name="PARTNO" value="IRLML2246TRPBF "/>
<attribute name="NAME"/>
</element>
<element name="UR_C1" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
</element>
<element name="CON_ADDON" library="Airbeam" package="CON_5_2MM" value="CON_1X52MM">
<attribute name="PARTNO" value="950505-5002-AR"/>
<attribute name="NAME"/>
</element>
<element name="U_BT_TX" library="Airbeam" package="SOT23-5" value="V_BUFFER">
<attribute name="PARTNO" value="SN74LVC1G125DBVR"/>
<attribute name="NAME"/>
</element>
<element name="U_BT_RX" library="Airbeam" package="SOT23-5" value="V_BUFFER">
<attribute name="PARTNO" value="SN74LVC1G125DBVR"/>
<attribute name="NAME"/>
</element>
<element name="VR3_0R1" library="SparkFun-Passives" package="0603-RES" value="0">
<attribute name="PARTNO" value="RC0603JR-070RL"/>
<attribute name="NAME"/>
</element>
<element name="VR3_0R2" library="SparkFun-Passives" package="0603-RES" value="DNP">
<attribute name="PARTNO" value="RC0603JR-070RL"/>
<attribute name="NAME"/>
</element>
<element name="VR5_0R1" library="SparkFun-Passives" package="0603-RES" value="DNP">
<attribute name="PARTNO" value="RC0603JR-070RL"/>
<attribute name="NAME"/>
</element>
<element name="VR5_0R2" library="SparkFun-Passives" package="0603-RES" value="0">
<attribute name="PARTNO" value="RC0603JR-070RL"/>
<attribute name="NAME"/>
</element>
<element name="RESET_SWITCH" library="Airbeam" package="SWITCH_TACTILE" value="SWITCH">
<attribute name="PARTNO" value="TL3315NF250Q"/>
</element>
<element name="U_Z3" library="varistor" package="CT/CN0603" value="CG0603MLC-05E">
<attribute name="PARTNO" value="CG0603MLC-05E"/>
<attribute name="NAME"/>
</element>
<element name="U_Z4" library="varistor" package="CT/CN0603" value="CG0603MLC-05E">
<attribute name="PARTNO" value="CG0603MLC-05E"/>
<attribute name="NAME"/>
</element>
<element name="U_VRUSB" library="Airbeam" package="UFDFN-8" value="VREG_MC34673">
<attribute name="PARTNO" value="MC34673AEPR2"/>
<attribute name="NAME"/>
</element>
<element name="UC_C8" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="PARTNO" value="C1608X5R1C105K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_Z5" library="varistor" package="CT/CN0603" value="CG0603MLC-05E">
<attribute name="PARTNO" value="CG0603MLC-05E"/>
<attribute name="NAME"/>
</element>
<element name="U_Z6" library="varistor" package="CT/CN0603" value="CG0603MLC-05E">
<attribute name="PARTNO" value="CG0603MLC-05E"/>
<attribute name="NAME"/>
</element>
<element name="DUST_SENSOR" library="Airbeam" package="EMPTY" value="OFF_BOARD">
<attribute name="PARTNO" value="PPD60PV-T2"/>
</element>
<element name="3_3V_FAN_COPOL" library="Airbeam" package="EMPTY" value="OFF_BOARD">
<attribute name="PARTNO" value="F16FB-05LLC/E"/>
</element>
<element name="LION_BATTERY" library="Airbeam" package="EMPTY" value="OFF_BOARD">
<attribute name="PARTNO" value="585460_2000mAh"/>
</element>
<element name="BT_C1" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="PARTNO" value="C1608X5R1C105K080AA"/>
<attribute name="NAME"/>
</element>
<element name="BT_C2" library="SparkFun-Passives" package="0603-CAP" value="100nF">
<attribute name="PARTNO" value="C1608X7R1E104K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CE_C1" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="PARTNO" value="C1608X5R1C105K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CD_C1" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="PARTNO" value="C1608X5R1C105K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CTH_C1" library="SparkFun-Passives" package="0603-CAP" value="1uF">
<attribute name="PARTNO" value="C1608X5R1C105K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR5_C4" library="SparkFun-Passives" package="0603-CAP" value="100nF">
<attribute name="PARTNO" value="C1608X7R1E104K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_FB1" library="Airbeam" package="U_FB1" value="FERITE_BEAD">
<attribute name="PARTNO" value="MH2029-300Y"/>
<attribute name="NAME"/>
</element>
<element name="CA_FB1" library="Airbeam" package="U_FB1" value="FERITE_BEAD">
<attribute name="PARTNO" value="MH2029-300Y"/>
<attribute name="NAME"/>
</element>
<element name="U_FB2" library="Airbeam" package="U_FB1" value="FERITE_BEAD">
<attribute name="PARTNO" value="MH2029-300Y"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="Airbeam" package="SOT23" value="MOSFET-N">
<attribute name="PARTNO" value="NDS331N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_ILIM" library="Airbeam" package="MSOP-8" value="USB-OVERCURRENT">
<attribute name="PARTNO" value="AP2161DM8G-13 "/>
<attribute name="NAME"/>
</element>
<element name="U_R3" library="SparkFun-Passives" package="0603-RES" value="10k">
<attribute name="PARTNO" value="RC0603JR-0710KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_C3" library="SparkFun-Passives" package="0805" value="10uF">
<attribute name="PARTNO" value="C2012X5R1C106K085AC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U_C4" library="SparkFun-Passives" package="0603-CAP" value="100nF">
<attribute name="PARTNO" value="C1608X7R1E104K080AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR_C1" library="Airbeam" package="2917_CAP" value="DNP">
<attribute name="PARTNO" value="T491D107K010AT "/>
<attribute name="NAME"/>
</element>
<element name="VR_FUSE" library="SparkFun-PowerIC" package="PTC-1206-WIDE" value="1A">
<attribute name="PARTNO" value="0ZCJ0100FF2E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Airbeam" package="JST-0.8MM" value="SUR_2PIN">
<attribute name="PARTNO" value="SM02B-SURS-TF"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="+5V">
<contactref element="CON_ICSP" pad="2"/>
<contactref element="ATMEGA32U4-T" pad="34"/>
<contactref element="ATMEGA32U4-T" pad="2"/>
<contactref element="U_MEGA32U-Q" pad="2"/>
<contactref element="U_MEGA32U-Q" pad="14"/>
<contactref element="U_MEGA32U-Q" pad="34"/>
<contactref element="U_TEMP-HUM" pad="P$1"/>
<contactref element="U_VR5" pad="P$1"/>
<contactref element="VR5_R1" pad="1"/>
<contactref element="VR5_C2" pad="1"/>
<contactref element="VR5_C3" pad="1"/>
<contactref element="CON_DUST" pad="P$3"/>
<contactref element="UC_R2" pad="2"/>
<contactref element="CON_ADDON" pad="P$4"/>
<contactref element="U_BT_TX" pad="5"/>
<contactref element="UC_C2" pad="1"/>
<contactref element="UC_C1" pad="1"/>
<contactref element="UC_C8" pad="1"/>
<contactref element="ATMEGA32U4-T" pad="14"/>
<contactref element="U_Z6" pad="1"/>
<contactref element="BT_C2" pad="1"/>
<contactref element="CE_C1" pad="1"/>
<contactref element="CD_C1" pad="1"/>
<contactref element="CTH_C1" pad="1"/>
<contactref element="U_FB2" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="CON_ICSP" pad="6"/>
<contactref element="UC_C2" pad="2"/>
<contactref element="UC_C1" pad="2"/>
<contactref element="U_MEGA32U-Q" pad="15"/>
<contactref element="U_MEGA32U-Q" pad="EXP"/>
<contactref element="U_MEGA32U-Q" pad="23"/>
<contactref element="U_MEGA32U-Q" pad="35"/>
<contactref element="ATMEGA32U4-T" pad="P$1"/>
<contactref element="U_Z2" pad="2"/>
<contactref element="U_Z1" pad="2"/>
<contactref element="U_TEMP-HUM" pad="P$4"/>
<contactref element="CON_USB" pad="BPBL"/>
<contactref element="CON_USB" pad="BPBR"/>
<contactref element="UBT" pad="P$13"/>
<contactref element="UBT" pad="P$19"/>
<contactref element="UBT" pad="P$14"/>
<contactref element="VR3_C1" pad="2"/>
<contactref element="VR3_R2" pad="2"/>
<contactref element="VR5_C1" pad="2"/>
<contactref element="VR5_R2" pad="2"/>
<contactref element="VR3_C2" pad="2"/>
<contactref element="VR3_C3" pad="2"/>
<contactref element="VR5_C2" pad="2"/>
<contactref element="VR5_C3" pad="2"/>
<contactref element="CON_BAT" pad="1"/>
<contactref element="VR_R1" pad="2"/>
<contactref element="VDETECT" pad="1"/>
<contactref element="VR_R2" pad="2"/>
<contactref element="CON_DUST" pad="P$1"/>
<contactref element="U_MEGA32U-Q" pad="43"/>
<contactref element="UC_R3" pad="1"/>
<contactref element="U_C1" pad="2"/>
<contactref element="U_C2" pad="2"/>
<contactref element="UC_C5" pad="2"/>
<contactref element="UC_C6" pad="2"/>
<contactref element="UC_C3" pad="1"/>
<contactref element="UC_C4" pad="1"/>
<contactref element="UC_R4" pad="1"/>
<contactref element="UR_C1" pad="2"/>
<contactref element="UBT" pad="P$2"/>
<contactref element="R_LED_BT" pad="1"/>
<contactref element="U_BT_RX" pad="3"/>
<contactref element="U_BT_RX" pad="1"/>
<contactref element="U_BT_TX" pad="3"/>
<contactref element="U_BT_TX" pad="1"/>
<contactref element="VR3_0R1" pad="1"/>
<contactref element="VR5_0R1" pad="1"/>
<contactref element="U_VR3" pad="P$3"/>
<contactref element="U_VR3" pad="MID_PAD"/>
<contactref element="U_VR3" pad="P$9"/>
<contactref element="U_VR5" pad="P$3"/>
<contactref element="U_VR5" pad="MID_PAD"/>
<contactref element="U_VR5" pad="P$9"/>
<contactref element="RESET_SWITCH" pad="P1"/>
<contactref element="RESET_SWITCH" pad="P2"/>
<contactref element="U_VRUSB" pad="P$4"/>
<contactref element="U_VRUSB" pad="P$5"/>
<contactref element="U_VRUSB" pad="P$9"/>
<contactref element="UR_R2" pad="1"/>
<contactref element="UC_C8" pad="2"/>
<contactref element="CON_BAT" pad="NC2"/>
<contactref element="CON_BAT" pad="NC1"/>
<contactref element="CON_USB" pad="PTR"/>
<contactref element="CON_USB" pad="PBR2"/>
<contactref element="CON_USB" pad="PBR"/>
<contactref element="ATMEGA32U4-T" pad="23"/>
<contactref element="ATMEGA32U4-T" pad="15"/>
<contactref element="CON_USB" pad="PTL"/>
<contactref element="CON_USB" pad="PBL2"/>
<contactref element="CON_USB" pad="PBL"/>
<contactref element="U_Z6" pad="2"/>
<contactref element="U_Z5" pad="2"/>
<contactref element="U_Z4" pad="2"/>
<contactref element="U_Z3" pad="2"/>
<contactref element="ATMEGA32U4-T" pad="43"/>
<contactref element="ATMEGA32U4-T" pad="35"/>
<contactref element="BT_C1" pad="2"/>
<contactref element="BT_C2" pad="2"/>
<contactref element="CE_C1" pad="2"/>
<contactref element="CD_C1" pad="2"/>
<contactref element="CTH_C1" pad="2"/>
<contactref element="VR5_C4" pad="2"/>
<contactref element="U_FB1" pad="P$1"/>
<contactref element="CA_FB1" pad="P$1"/>
<contactref element="VR_C1" pad="T-"/>
<contactref element="U$2" pad="P2"/>
<contactref element="U$2" pad="PAD1"/>
<contactref element="U$2" pad="PAD2"/>
</signal>
<signal name="AREF">
<contactref element="U_MEGA32U-Q" pad="42"/>
<contactref element="ATMEGA32U4-T" pad="42"/>
<contactref element="UC_C6" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="CON_ICSP" pad="5"/>
<contactref element="U_MEGA32U-Q" pad="13"/>
<contactref element="ATMEGA32U4-T" pad="13"/>
<contactref element="UC_R2" pad="1"/>
<contactref element="RESET_SWITCH" pad="P4"/>
<contactref element="RESET_SWITCH" pad="P3"/>
</signal>
<signal name="SCK">
<contactref element="CON_ICSP" pad="3"/>
<contactref element="U_MEGA32U-Q" pad="9"/>
<contactref element="ATMEGA32U4-T" pad="9"/>
</signal>
<signal name="D-">
<contactref element="U_Z2" pad="1"/>
<contactref element="CON_USB" pad="T2"/>
<contactref element="U_R1" pad="1"/>
</signal>
<signal name="D+">
<contactref element="U_Z1" pad="1"/>
<contactref element="CON_USB" pad="T3"/>
<contactref element="U_R2" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="CON_ICSP" pad="1"/>
<contactref element="U_MEGA32U-Q" pad="11"/>
<contactref element="ATMEGA32U4-T" pad="11"/>
</signal>
<signal name="MOSI">
<contactref element="CON_ICSP" pad="4"/>
<contactref element="U_MEGA32U-Q" pad="10"/>
<contactref element="ATMEGA32U4-T" pad="10"/>
</signal>
<signal name="XTAL2">
<contactref element="U_MEGA32U-Q" pad="16"/>
<contactref element="ATMEGA32U4-T" pad="16"/>
<contactref element="UC_CRYSTAL" pad="2"/>
<contactref element="UC_R1" pad="2"/>
<contactref element="UC_C3" pad="2"/>
</signal>
<signal name="XTAL1">
<contactref element="U_MEGA32U-Q" pad="17"/>
<contactref element="ATMEGA32U4-T" pad="17"/>
<contactref element="UC_CRYSTAL" pad="1"/>
<contactref element="UC_R1" pad="1"/>
<contactref element="UC_C4" pad="2"/>
</signal>
<signal name="RD-">
<contactref element="U_MEGA32U-Q" pad="3"/>
<contactref element="ATMEGA32U4-T" pad="3"/>
<contactref element="U_R1" pad="2"/>
</signal>
<signal name="RD+">
<contactref element="U_MEGA32U-Q" pad="4"/>
<contactref element="ATMEGA32U4-T" pad="4"/>
<contactref element="U_R2" pad="2"/>
</signal>
<signal name="UGND">
<contactref element="U_MEGA32U-Q" pad="5"/>
<contactref element="ATMEGA32U4-T" pad="5"/>
<contactref element="CON_USB" pad="T5"/>
<contactref element="UC_R3" pad="2"/>
<contactref element="UC_C7" pad="2"/>
<contactref element="U_FB1" pad="P$2"/>
<contactref element="U_ILIM" pad="P$1"/>
<contactref element="U_ILIM" pad="P$4"/>
<contactref element="U_C4" pad="2"/>
<contactref element="U_C3" pad="2"/>
</signal>
<signal name="XUSB">
<contactref element="CON_USB" pad="T1"/>
<contactref element="U_ILIM" pad="P$3"/>
<contactref element="U_ILIM" pad="P$2"/>
<contactref element="U_C3" pad="1"/>
<contactref element="U_C4" pad="1"/>
</signal>
<signal name="D2/SDA">
<contactref element="U_MEGA32U-Q" pad="19"/>
<contactref element="ATMEGA32U4-T" pad="19"/>
</signal>
<signal name="IO12">
<contactref element="U_MEGA32U-Q" pad="26"/>
<contactref element="ATMEGA32U4-T" pad="26"/>
</signal>
<signal name="D3/SCL">
<contactref element="U_MEGA32U-Q" pad="18"/>
<contactref element="ATMEGA32U4-T" pad="18"/>
</signal>
<signal name="D1/TX">
<contactref element="U_MEGA32U-Q" pad="21"/>
<contactref element="ATMEGA32U4-T" pad="21"/>
</signal>
<signal name="IO11*/BT_RX">
<contactref element="U_MEGA32U-Q" pad="12"/>
<contactref element="ATMEGA32U4-T" pad="12"/>
<contactref element="U_BT_RX" pad="2"/>
</signal>
<signal name="IO9*/TH_DETECT">
<contactref element="U_MEGA32U-Q" pad="29"/>
<contactref element="ATMEGA32U4-T" pad="29"/>
<contactref element="U_TEMP-HUM" pad="P$2"/>
</signal>
<signal name="IO10*/BT_TX">
<contactref element="U_MEGA32U-Q" pad="30"/>
<contactref element="ATMEGA32U4-T" pad="30"/>
<contactref element="U_BT_TX" pad="4"/>
</signal>
<signal name="A3">
<contactref element="U_MEGA32U-Q" pad="39"/>
<contactref element="ATMEGA32U4-T" pad="39"/>
</signal>
<signal name="A2">
<contactref element="U_MEGA32U-Q" pad="38"/>
<contactref element="ATMEGA32U4-T" pad="38"/>
<contactref element="CON_ADDON" pad="P$2"/>
<contactref element="U_Z4" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U_MEGA32U-Q" pad="37"/>
<contactref element="ATMEGA32U4-T" pad="37"/>
<contactref element="CON_ADDON" pad="P$1"/>
<contactref element="U_Z3" pad="1"/>
</signal>
<signal name="A0/DUST_DETECT">
<contactref element="U_MEGA32U-Q" pad="36"/>
<contactref element="ATMEGA32U4-T" pad="36"/>
<contactref element="CON_DUST" pad="P$2"/>
</signal>
<signal name="A4">
<contactref element="U_MEGA32U-Q" pad="40"/>
<contactref element="ATMEGA32U4-T" pad="40"/>
</signal>
<signal name="A5">
<contactref element="U_MEGA32U-Q" pad="41"/>
<contactref element="ATMEGA32U4-T" pad="41"/>
</signal>
<signal name="D5*/FAN_CONTROL">
<contactref element="ATMEGA32U4-T" pad="31"/>
<contactref element="U_MEGA32U-Q" pad="31"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="D0/RX">
<contactref element="U_MEGA32U-Q" pad="20"/>
<contactref element="ATMEGA32U4-T" pad="20"/>
</signal>
<signal name="VUSB">
<contactref element="U_MEGA32U-Q" pad="7"/>
<contactref element="ATMEGA32U4-T" pad="7"/>
<contactref element="LED_CH" pad="ANODE"/>
<contactref element="U_C1" pad="1"/>
<contactref element="U_C2" pad="1"/>
<contactref element="U_VRUSB" pad="P$1"/>
<contactref element="U_ILIM" pad="P$6"/>
<contactref element="U_ILIM" pad="P$7"/>
<contactref element="U_R3" pad="2"/>
<contactref element="VR_D1" pad="P$1"/>
<contactref element="VR_R1" pad="1"/>
<contactref element="VR_MOS-P1" pad="1"/>
</signal>
<signal name="RXLED">
<contactref element="U_MEGA32U-Q" pad="8"/>
<contactref element="ATMEGA32U4-T" pad="8"/>
</signal>
<signal name="D6*">
<contactref element="U_MEGA32U-Q" pad="27"/>
<contactref element="ATMEGA32U4-T" pad="27"/>
</signal>
<signal name="IO13*/BT_LED">
<contactref element="ATMEGA32U4-T" pad="32"/>
<contactref element="U_MEGA32U-Q" pad="32"/>
<contactref element="LED_BT" pad="ANODE"/>
</signal>
<signal name="IO8">
<contactref element="U_MEGA32U-Q" pad="28"/>
<contactref element="ATMEGA32U4-T" pad="28"/>
</signal>
<signal name="D7">
<contactref element="U_MEGA32U-Q" pad="1"/>
<contactref element="ATMEGA32U4-T" pad="1"/>
</signal>
<signal name="AVCC">
<contactref element="U_MEGA32U-Q" pad="44"/>
<contactref element="ATMEGA32U4-T" pad="44"/>
<contactref element="U_MEGA32U-Q" pad="24"/>
<contactref element="ATMEGA32U4-T" pad="24"/>
<contactref element="UC_C5" pad="1"/>
<contactref element="U_FB2" pad="P$2"/>
</signal>
<signal name="UCAP">
<contactref element="U_MEGA32U-Q" pad="6"/>
<contactref element="ATMEGA32U4-T" pad="6"/>
<contactref element="UC_C7" pad="1"/>
</signal>
<signal name="HWB">
<contactref element="ATMEGA32U4-T" pad="33"/>
<contactref element="U_MEGA32U-Q" pad="33"/>
<contactref element="UC_R4" pad="2"/>
</signal>
<signal name="D4">
<contactref element="ATMEGA32U4-T" pad="25"/>
<contactref element="U_MEGA32U-Q" pad="25"/>
</signal>
<signal name="TXLED">
<contactref element="ATMEGA32U4-T" pad="22"/>
<contactref element="U_MEGA32U-Q" pad="22"/>
</signal>
<signal name="+3V3">
<contactref element="UBT" pad="P$12"/>
<contactref element="U_VR3" pad="P$1"/>
<contactref element="VR3_R1" pad="1"/>
<contactref element="VR3_C2" pad="1"/>
<contactref element="VR3_C3" pad="1"/>
<contactref element="VR_R4" pad="1"/>
<contactref element="CON_ADDON" pad="P$3"/>
<contactref element="U_BT_RX" pad="5"/>
<contactref element="U_Z5" pad="1"/>
<contactref element="BT_C1" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="VEN">
<contactref element="U_VR3" pad="P$6"/>
<contactref element="U_VR5" pad="P$6"/>
<contactref element="VDETECT" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U_VR3" pad="P$10"/>
<contactref element="VR3_R1" pad="2"/>
<contactref element="VR3_R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U_VR3" pad="P$2"/>
<contactref element="VR3_L1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U_VR3" pad="P$4"/>
<contactref element="VR3_L1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U_VR5" pad="P$10"/>
<contactref element="VR5_R1" pad="2"/>
<contactref element="VR5_R2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U_VR5" pad="P$2"/>
<contactref element="VR5_L1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U_VR5" pad="P$4"/>
<contactref element="VR5_L1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R_LED_CH" pad="2"/>
<contactref element="LED_CH" pad="CATHODE"/>
</signal>
<signal name="N$13">
<contactref element="R_LED_CH" pad="1"/>
<contactref element="U_VRUSB" pad="P$3"/>
</signal>
<signal name="N$16">
<contactref element="UR_R2" pad="2"/>
<contactref element="U_VRUSB" pad="P$7"/>
</signal>
<signal name="V_BAT">
<contactref element="CON_BAT" pad="2"/>
<contactref element="VR_R3" pad="1"/>
<contactref element="VR_MOS-P1" pad="2"/>
<contactref element="UR_C1" pad="1"/>
<contactref element="U_VRUSB" pad="P$8"/>
</signal>
<signal name="VREG_IN">
<contactref element="U_VR5" pad="P$5"/>
<contactref element="U_VR5" pad="P$8"/>
<contactref element="VR5_C1" pad="1"/>
<contactref element="U_ONOFF" pad="P$4"/>
<contactref element="U_ONOFF" pad="P$6"/>
<contactref element="U_ONOFF" pad="P$3"/>
<contactref element="U_ONOFF" pad="P$1"/>
<contactref element="VR3_0R2" pad="1"/>
<contactref element="VR5_0R2" pad="1"/>
<contactref element="VR5_C4" pad="1"/>
<contactref element="VR_FUSE" pad="2"/>
<contactref element="U_VR3" pad="P$5"/>
<contactref element="U_VR3" pad="P$8"/>
<contactref element="VR3_C1" pad="1"/>
<contactref element="VR_C1" pad="T+"/>
<contactref element="VR_D1" pad="P$2"/>
</signal>
<signal name="VDETECT_VDD">
<contactref element="U_ONOFF" pad="P$2"/>
<contactref element="U_ONOFF" pad="P$5"/>
<contactref element="VDETECT" pad="3"/>
<contactref element="VR_R2" pad="1"/>
</signal>
<signal name="VFAN">
<contactref element="VR_R4" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="P1"/>
</signal>
<signal name="N$3">
<contactref element="R_LED_BT" pad="2"/>
<contactref element="LED_BT" pad="CATHODE"/>
</signal>
<signal name="BT_TX">
<contactref element="UBT" pad="P$21"/>
<contactref element="U_BT_TX" pad="2"/>
</signal>
<signal name="BT_RX">
<contactref element="UBT" pad="P$20"/>
<contactref element="U_BT_RX" pad="4"/>
</signal>
<signal name="VR3_PS">
<contactref element="U_VR3" pad="P$7"/>
<contactref element="VR3_0R1" pad="2"/>
<contactref element="VR3_0R2" pad="2"/>
</signal>
<signal name="VR5_PS">
<contactref element="VR5_0R1" pad="2"/>
<contactref element="VR5_0R2" pad="2"/>
<contactref element="U_VR5" pad="P$7"/>
</signal>
<signal name="N$7">
<contactref element="CON_ADDON" pad="P$5"/>
<contactref element="CA_FB1" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="U_ILIM" pad="P$5"/>
<contactref element="U_R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="VR_R3" pad="2"/>
<contactref element="VR_MOS-P1" pad="3"/>
<contactref element="VR_FUSE" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
