<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="23.368" y1="79.502" x2="23.368" y2="27.432" width="0.2032" layer="20"/>
<wire x1="14.224" y1="70.104" x2="14.224" y2="79.502" width="0.2032" layer="20"/>
<wire x1="14.224" y1="79.502" x2="23.368" y2="79.502" width="0.2032" layer="20"/>
<wire x1="23.368" y1="27.432" x2="19.558" y2="27.432" width="0.2032" layer="20"/>
<wire x1="19.558" y1="27.432" x2="19.558" y2="70.104" width="0.2032" layer="20"/>
<wire x1="19.558" y1="70.104" x2="14.224" y2="70.104" width="0.2032" layer="20"/>
<text>Stratux Fan Control v1.1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH-VERT">
</package>
<package name="1X20">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="JST-2-PTH-VERT" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X20" value=""/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="220"/>
<element name="T1" library="transistor" package="SOT23-BEC" value=""/>
</elements>
<signals>
<signal name="N$3">
<contactref element="J1" pad="2"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="3"/>
<contactref element="T1" pad="E"/>
<contactref element="J2" pad="17"/>
</signal>
<signal name="5V">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
