<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.0">
<drawing>
<board>
<plain>
<wire x1="43.18" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="43.18" width="0.2032" layer="20"/>
<wire x1="0" y1="43.18" x2="43.18" y2="43.18" width="0.2032" layer="20"/>
<wire x1="43.18" y1="43.18" x2="43.18" y2="0" width="0.2032" layer="20"/>
<text>v12-SMA</text>
<text>Measurements in inches</text>
<text>Board thickness is 1.6mm</text>
<text>No clean process</text>
<text>4 Layer Board</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_2-NC_TRACE_SILK">
</package>
<package name="SMT-JUMPER_2_NC_TRACE_SILK">
</package>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
</packages>
</library>
<library name="SparkX">
<packages>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -9 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-C-16P-2LAYER-PADS">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSHW-LOGO-MINI">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Mini - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFE_LOGO_FLAME_.1">
<description>&lt;h3&gt;SparkFun Flame Logo - 0.1" Height - Silkscreen&lt;/h3&gt;
&lt;p&gt;SparkFun Flame Logo&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;SFE_LOGO_FLAME&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFE_LOGO_NAME_FLAME_.1">
<description>&lt;h3&gt;SparkFun Font Logo w/ Flame - 0.1" Height - Silkscreen&lt;/h3&gt;
&lt;p&gt;SparkFun font logo with flame logo&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;SFE_LOGO_NAME_FLAME&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ORDERING_INSTRUCTIONS">
<description>&lt;h3&gt;Special Ordering Instructions Alert&lt;/h3&gt;
&lt;p&gt;Indicates that the PCB material, colors, copper weights, and/or thickness are non-standard.&lt;/p&gt;
&lt;p&gt;(Standard is 1.6mm FR4, 1 oz copper, immersion silver plating, red soldermask, white silkscreen.)&lt;/p&gt;
&lt;p&gt;Use 0.7" Vector font @ 8% ratio</description>
</package>
<package name="QWIIC_4MM">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
<description>SOD-323 (Small Outline Diode)</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ML414H_IV01E">
<description>&lt;h3&gt;SEIKO ML414H-IV01E Reflowable Lithium Battery&lt;/h3&gt;

&lt;p&gt;
ML414H is a rechargeable, coin type battery with features
such as Pb-free reflowable (Peak temperature: 260 C) and
high temperature heat resistance.
&lt;/p&gt;

&lt;ul&gt;
&lt;li&gt;3V&lt;/li&gt;
&lt;li&gt;1mAH&lt;/li&gt;
&lt;li&gt;4.8mm Diamter&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="Labels">
<packages>
<package name="SDA-[)">
</package>
<package name="SCL-[)">
</package>
<package name="3V3-04">
</package>
<package name="GND-04">
</package>
<package name="I_SUPER2_C-()-03">
</package>
<package name="PWR-()-03">
</package>
<package name="5V">
</package>
<package name="CS#-&lt;]">
</package>
<package name="SCK-(]-04">
</package>
</packages>
</library>
<library name="buzzard_labels (5)">
<packages>
<package name="INT8">
</package>
<package name="U#BLOX3">
</package>
</packages>
</library>
<library name="buzzard_labels (7)">
<packages>
<package name="#RST3">
</package>
<package name="#SAFE1">
</package>
<package name="PPS5">
</package>
</packages>
</library>
<library name="SparkFun-Coils">
<description>&lt;h3&gt;SparkFun Coils&lt;/h3&gt;
In this library you'll find magnetics.

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Inductors&lt;/li&gt;
&lt;li&gt;Ferrite Beads&lt;/li&gt;
&lt;li&gt;Transformers&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;br&gt;
&lt;p&gt;We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.&lt;/p&gt;</description>
<packages>
<package name="0402_MURATA">
</package>
</packages>
</library>
<library name="buzzard_labels (33)">
<packages>
<package name="PPS0">
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOT886">
<description>&lt;h3&gt;SOT886&lt;/h3&gt;
&lt;p&gt;Package for "F" variant of PRTR5V0U2F&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="buzzard_labels">
<packages>
<package name="FENCE2">
</package>
<package name="RTK1">
</package>
</packages>
</library>
<library name="buzzard_labels (1)">
<packages>
<package name="FENCE0">
</package>
<package name="RTK1">
</package>
</packages>
</library>
<library name="buzzard_labels (6)">
<packages>
<package name="DSEL0">
</package>
</packages>
</library>
<library name="buzzard_labels (36)">
<packages>
<package name="RX#MOSI3">
</package>
<package name="TX#MISO1">
</package>
</packages>
</library>
<library name="ZED-F9P">
<packages>
<package name="ZED-F9P">
</package>
</packages>
</library>
<library name="buzzard_labels (4)">
<packages>
<package name="CORRECTION0">
</package>
<package name="GND3">
</package>
<package name="RTCM5">
</package>
<package name="ZED#F9P6">
</package>
<package name="GPS0">
</package>
<package name="GPS#RTK#SMA5">
</package>
</packages>
</library>
<library name="buzzard_labels (8)">
<packages>
<package name="ACTIVE_L1#L21">
</package>
<package name="ANTENNA2">
</package>
</packages>
</library>
<library name="buzzard_labels (10)">
<packages>
<package name="RX20">
</package>
<package name="RX22">
</package>
<package name="TX21">
</package>
<package name="TX23">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun RF, WiFi, Cellular, and Bluetooth&lt;/h3&gt;
In this library you'll find things that send or receive RF-- cellular modules, Bluetooth, WiFi, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
</packages>
</library>
<library name="buzzard_labels (2)">
<packages>
<package name="PPS1">
</package>
</packages>
</library>
<library name="buzzard_labels (3)">
<packages>
<package name="RTK#SMA4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP31" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP41" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP21" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP61" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="J2" library="SparkFun-Connectors" package="JST04_1MM_RA" value="Qwiic Right Angle">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-13694"/>
<attribute name="VALUE" value="Qwiic Right Angle"/>
</element>
<element name="J3" library="SparkX" package="1X04_NO_SILK" value="PTH">
<attribute name="NAME"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="JST04_1MM_RA" value="Qwiic Right Angle">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-13694"/>
<attribute name="VALUE" value="Qwiic Right Angle"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-MINI" value="OSHW-LOGOMINI"/>
<element name="R3" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE" value="33"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE" value="33"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-13930"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="SparkFun-Batteries" package="ML414H_IV01E" value="6.8MM_COIN_CELL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="BATT-14267"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="2.2k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE" value="2.2k"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="2.2k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="VALUE" value="2.2k"/>
</element>
<element name="JP5" library="SparkFun-Jumpers" package="SMT-JUMPER_3_2-NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="Yellow">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09003"/>
<attribute name="VALUE"/>
</element>
<element name="PPS_LED" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="0.5A/40V/420mV">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-10955"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="JP71" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP81" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="R2" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="JP91" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP101" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$1" library="Labels" package="SDA-[)" value=""/>
<element name="U$3" library="Labels" package="SCL-[)" value=""/>
<element name="U$4" library="Labels" package="SDA-[)" value=""/>
<element name="U$5" library="Labels" package="SCL-[)" value=""/>
<element name="U$6" library="Labels" package="3V3-04" value=""/>
<element name="U$7" library="Labels" package="3V3-04" value=""/>
<element name="U$8" library="Labels" package="GND-04" value=""/>
<element name="U$9" library="Labels" package="GND-04" value=""/>
<element name="U$10" library="Labels" package="I_SUPER2_C-()-03" value=""/>
<element name="U$15" library="buzzard_labels (5)" package="INT8" value=""/>
<element name="U$16" library="buzzard_labels (5)" package="INT8" value=""/>
<element name="U$22" library="buzzard_labels (5)" package="U#BLOX3" value=""/>
<element name="U$35" library="buzzard_labels (7)" package="#RST3" value=""/>
<element name="U$36" library="buzzard_labels (7)" package="#RST3" value=""/>
<element name="U$39" library="buzzard_labels (7)" package="#SAFE1" value=""/>
<element name="U$40" library="buzzard_labels (7)" package="#SAFE1" value=""/>
<element name="U$43" library="buzzard_labels (7)" package="PPS5" value=""/>
<element name="U$44" library="buzzard_labels (7)" package="PPS5" value=""/>
<element name="U$52" library="buzzard_labels (33)" package="PPS0" value=""/>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-13930"/>
<attribute name="VALUE" value="1.0uF"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE" value="RED"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="U2" library="SparkFun-IC-Power" package="SOT23-5" value="3.3V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="VREG-12457"/>
<attribute name="VALUE" value="3.3V"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-13930"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="27">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-09334"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603" value="27">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-09334"/>
<attribute name="VALUE"/>
</element>
<element name="SPI" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="VALUE"/>
</element>
<element name="RTK" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="VALUE"/>
</element>
<element name="FENCE" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0402" value="47pF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-15063"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE" value="33"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="SparkFun-Coils" package="0402_MURATA" value="120NH">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="NDUC-15072"/>
<attribute name="VALUE" value="120NH"/>
</element>
<element name="U$11" library="buzzard_labels" package="FENCE2" value=""/>
<element name="U$13" library="buzzard_labels" package="RTK1" value=""/>
<element name="U$14" library="buzzard_labels (1)" package="FENCE0" value=""/>
<element name="U$17" library="buzzard_labels (1)" package="FENCE0" value=""/>
<element name="U$28" library="buzzard_labels (1)" package="RTK1" value=""/>
<element name="U$29" library="buzzard_labels (1)" package="RTK1" value=""/>
<element name="U$60" library="Labels" package="3V3-04" value=""/>
<element name="U$61" library="Labels" package="3V3-04" value=""/>
<element name="U$62" library="Labels" package="GND-04" value=""/>
<element name="U$63" library="Labels" package="GND-04" value=""/>
<element name="U$27" library="buzzard_labels (6)" package="DSEL0" value=""/>
<element name="U$18" library="Labels" package="PWR-()-03" value=""/>
<element name="U$19" library="Labels" package="5V" value=""/>
<element name="U$20" library="Labels" package="5V" value=""/>
<element name="U$23" library="Labels" package="CS#-&lt;]" value=""/>
<element name="U$24" library="Labels" package="CS#-&lt;]" value=""/>
<element name="U$38" library="Labels" package="SCK-(]-04" value=""/>
<element name="U$41" library="Labels" package="SCK-(]-04" value=""/>
<element name="U$33" library="SparkFun-Aesthetics" package="SFE_LOGO_FLAME_.1" value=""/>
<element name="U$31" library="buzzard_labels (36)" package="RX#MOSI3" value=""/>
<element name="U$37" library="buzzard_labels (36)" package="TX#MISO1" value=""/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_FLAME_.1" value="SFE_LOGO_NAME_FLAME.1_INCH"/>
<element name="U3" library="ZED-F9P" package="ZED-F9P" value="ZED-F9P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603" value="5.1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12083"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0603" value="5.1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12083"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="USB-C-16P-2LAYER-PADS" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-14122"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="ORDERING_INSTRUCTIONS" value="SPECIAL_INSTRUCTIONS-ORDERING"/>
<element name="J7" library="SparkFun-Connectors" package="1X09_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_NO_SILK" value="Radio">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$45" library="buzzard_labels (4)" package="GND3" value=""/>
<element name="U$66" library="Labels" package="3V3-04" value=""/>
<element name="U$67" library="Labels" package="3V3-04" value=""/>
<element name="U$68" library="buzzard_labels (4)" package="GND3" value=""/>
<element name="U$69" library="buzzard_labels (4)" package="CORRECTION0" value=""/>
<element name="U$70" library="buzzard_labels (4)" package="RTCM5" value=""/>
<element name="U$49" library="buzzard_labels (4)" package="ZED#F9P6" value=""/>
<element name="U$48" library="buzzard_labels (4)" package="RTCM5" value=""/>
<element name="U$53" library="buzzard_labels (4)" package="CORRECTION0" value=""/>
<element name="U$26" library="buzzard_labels (36)" package="RX#MOSI3" value=""/>
<element name="U$34" library="buzzard_labels (36)" package="TX#MISO1" value=""/>
<element name="U$65" library="buzzard_labels (8)" package="ACTIVE_L1#L21" value=""/>
<element name="U$71" library="buzzard_labels (8)" package="ANTENNA2" value=""/>
<element name="U$21" library="buzzard_labels (10)" package="RX20" value=""/>
<element name="U$42" library="buzzard_labels (10)" package="RX22" value=""/>
<element name="U$50" library="buzzard_labels (10)" package="TX21" value=""/>
<element name="U$51" library="buzzard_labels (10)" package="TX23" value=""/>
<element name="U$55" library="buzzard_labels (10)" package="TX21" value=""/>
<element name="U$56" library="buzzard_labels (10)" package="RX20" value=""/>
<element name="U$57" library="buzzard_labels (10)" package="TX21" value=""/>
<element name="U$58" library="buzzard_labels (10)" package="RX20" value=""/>
<element name="R18" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-13930"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="U$59" library="buzzard_labels (4)" package="GPS0" value=""/>
<element name="R24" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-IC-Power" package="SOT886" value="PRTR5V0U2F">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-14084"/>
<attribute name="VALUE"/>
</element>
<element name="E1" library="SparkFun-RF" package="SMA-EDGE" value="SMA">
<attribute name="PROD_ID" value="CONN-08289"/>
</element>
<element name="U$30" library="SparkFun-Aesthetics" package="QWIIC_4MM" value=""/>
<element name="PPS" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E2" library="SparkFun-RF" package="SMA-EDGE" value="SMA">
<attribute name="PROD_ID" value="CONN-08289"/>
</element>
<element name="PWR" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$47" library="buzzard_labels (2)" package="PPS1" value=""/>
<element name="U$12" library="Labels" package="PWR-()-03" value=""/>
<element name="U$25" library="buzzard_labels (33)" package="PPS0" value=""/>
<element name="U$32" library="buzzard_labels" package="RTK1" value=""/>
<element name="U$54" library="buzzard_labels" package="FENCE2" value=""/>
<element name="U$72" library="buzzard_labels (33)" package="PPS0" value=""/>
<element name="U$73" library="buzzard_labels (3)" package="RTK#SMA4" value=""/>
<element name="U$74" library="buzzard_labels (2)" package="PPS1" value=""/>
<element name="U$75" library="buzzard_labels (8)" package="ANTENNA2" value=""/>
<element name="U$76" library="buzzard_labels (4)" package="GPS#RTK#SMA5" value=""/>
<element name="FRAME2" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LEDGER">
<attribute name="DESIGNER" value=""/>
<attribute name="REV" value=""/>
</element>
</elements>
<signals>
<signal name="3.3V">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="U2" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="U3" pad="33"/>
<contactref element="U3" pad="34"/>
<contactref element="J7" pad="7"/>
<contactref element="J1" pad="4"/>
<contactref element="R15" pad="2"/>
<contactref element="U3" pad="38"/>
<contactref element="C2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="PWR" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="B1" pad="-"/>
<contactref element="D1" pad="C"/>
<contactref element="C4" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="SPI" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="U3" pad="92"/>
<contactref element="U3" pad="90"/>
<contactref element="U3" pad="72"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="76"/>
<contactref element="U3" pad="57"/>
<contactref element="U3" pad="48"/>
<contactref element="U3" pad="95"/>
<contactref element="U3" pad="70"/>
<contactref element="U3" pad="73"/>
<contactref element="U3" pad="93"/>
<contactref element="U3" pad="101"/>
<contactref element="U3" pad="69"/>
<contactref element="U3" pad="71"/>
<contactref element="U3" pad="86"/>
<contactref element="U3" pad="83"/>
<contactref element="U3" pad="100"/>
<contactref element="U3" pad="59"/>
<contactref element="U3" pad="56"/>
<contactref element="U3" pad="99"/>
<contactref element="U3" pad="55"/>
<contactref element="U3" pad="64"/>
<contactref element="U3" pad="41"/>
<contactref element="U3" pad="87"/>
<contactref element="U3" pad="80"/>
<contactref element="U3" pad="98"/>
<contactref element="U3" pad="68"/>
<contactref element="U3" pad="89"/>
<contactref element="U3" pad="84"/>
<contactref element="U3" pad="67"/>
<contactref element="U3" pad="88"/>
<contactref element="U3" pad="94"/>
<contactref element="U3" pad="85"/>
<contactref element="U3" pad="61"/>
<contactref element="U3" pad="12"/>
<contactref element="U3" pad="91"/>
<contactref element="U3" pad="63"/>
<contactref element="U3" pad="66"/>
<contactref element="U3" pad="58"/>
<contactref element="U3" pad="62"/>
<contactref element="U3" pad="97"/>
<contactref element="U3" pad="79"/>
<contactref element="U3" pad="14"/>
<contactref element="U3" pad="82"/>
<contactref element="U3" pad="78"/>
<contactref element="U3" pad="96"/>
<contactref element="U3" pad="37"/>
<contactref element="U3" pad="77"/>
<contactref element="U3" pad="65"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="102"/>
<contactref element="U3" pad="74"/>
<contactref element="U3" pad="32"/>
<contactref element="U3" pad="81"/>
<contactref element="U3" pad="75"/>
<contactref element="U3" pad="60"/>
<contactref element="J5" pad="GND2"/>
<contactref element="J5" pad="GND"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="J7" pad="9"/>
<contactref element="J1" pad="6"/>
<contactref element="C7" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="J5" pad="SHLD2"/>
<contactref element="J5" pad="SHLD4"/>
<contactref element="J5" pad="SHLD3"/>
<contactref element="J5" pad="SHLD1"/>
<contactref element="E1" pad="GND@1"/>
<contactref element="E1" pad="GND@3"/>
<contactref element="E1" pad="GND@0"/>
<contactref element="E1" pad="GND@2"/>
<contactref element="E2" pad="GND@1"/>
<contactref element="E2" pad="GND@3"/>
<contactref element="E2" pad="GND@0"/>
<contactref element="E2" pad="GND@2"/>
</signal>
<signal name="SCL/SCK">
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="R7" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="SDA/!CS">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="R8" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="!RESET">
<contactref element="J6" pad="4"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="TXLV">
<contactref element="R3" pad="1"/>
<contactref element="U3" pad="42"/>
</signal>
<signal name="RXLV">
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="43"/>
</signal>
<signal name="BACKUP">
<contactref element="C3" pad="1"/>
<contactref element="B1" pad="+"/>
<contactref element="R5" pad="1"/>
<contactref element="U3" pad="36"/>
</signal>
<signal name="INT">
<contactref element="J6" pad="6"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="PPS_STAT">
<contactref element="PPS_LED" pad="2"/>
<contactref element="J6" pad="3"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R8" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="2"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="PPS_LED" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="D2" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SDA_LV">
<contactref element="R2" pad="1"/>
<contactref element="U3" pad="44"/>
</signal>
<signal name="SCL_LV">
<contactref element="R4" pad="1"/>
<contactref element="U3" pad="45"/>
</signal>
<signal name="!SAFE">
<contactref element="J6" pad="5"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="RXI/MOSI">
<contactref element="R6" pad="2"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="TXO/MISO">
<contactref element="R3" pad="2"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="GPS_ANT1">
<contactref element="FB1" pad="P1"/>
<contactref element="U3" pad="2"/>
<contactref element="E1" pad="SIG"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="J5" pad="VBUS1"/>
<contactref element="J5" pad="VBUS2"/>
<contactref element="J7" pad="8"/>
<contactref element="D6" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="R9" pad="2"/>
<contactref element="U3" pad="40"/>
</signal>
<signal name="N$12">
<contactref element="R10" pad="2"/>
<contactref element="U3" pad="39"/>
</signal>
<signal name="D_SEL">
<contactref element="SPI" pad="2"/>
<contactref element="U3" pad="47"/>
</signal>
<signal name="RTK_STAT">
<contactref element="RTK" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="FENCE_STAT">
<contactref element="FENCE" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="D3" pad="A"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="RTK" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D4" pad="A"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="FENCE" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R14" pad="2"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="ANT_VCC">
<contactref element="R14" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="FB1" pad="P2"/>
</signal>
<signal name="D+">
<contactref element="R9" pad="1"/>
<contactref element="D6" pad="4"/>
</signal>
<signal name="D-">
<contactref element="R10" pad="1"/>
<contactref element="D6" pad="6"/>
</signal>
<signal name="TX2">
<contactref element="J7" pad="6"/>
<contactref element="J1" pad="2"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="RX2">
<contactref element="J7" pad="5"/>
<contactref element="J1" pad="3"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="CC1">
<contactref element="R17" pad="2"/>
<contactref element="J5" pad="A5"/>
</signal>
<signal name="CC2">
<contactref element="R16" pad="2"/>
<contactref element="J5" pad="B5"/>
</signal>
<signal name="UNP_D+">
<contactref element="J5" pad="A6"/>
<contactref element="J5" pad="B6"/>
<contactref element="D6" pad="3"/>
</signal>
<signal name="UNP_D-">
<contactref element="J5" pad="B7"/>
<contactref element="J5" pad="A7"/>
<contactref element="D6" pad="1"/>
</signal>
<signal name="TX2_P">
<contactref element="U3" pad="27"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="26"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="51"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U3" pad="49"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="PPS">
<contactref element="U3" pad="53"/>
<contactref element="PPS" pad="2"/>
<contactref element="E2" pad="SIG"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="50"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U3" pad="20"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U3" pad="19"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R21" pad="1"/>
<contactref element="PPS" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="PWR" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
