<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.23" y2="0" width="0" layer="20"/>
<wire x1="35.23" y1="0" x2="35.23" y2="33.01" width="0" layer="20"/>
<wire x1="35.23" y1="33.01" x2="0" y2="33.01" width="0" layer="20"/>
<wire x1="0" y1="33.01" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>PB4</text>
<text>PB3</text>
<text>RST</text>
<text>PB0</text>
<text>PB1</text>
<text>PB2</text>
<text>VCC</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>GND</text>
<text>RST</text>
<text>VCC</text>
</plain>
<libraries>
<library name="EAGLE_chiefenne">
<description>EAGLE library made by chiefenne</description>
<packages>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
<package name="SOCKED-08">
<description>&lt;b&gt;Dual In Line Socked&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;FEMALE Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE04-1Y">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="EAGLE_chiefenne" package="AVR-ISP-6" value="AVR-ISP-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ATTINY-SOCKET" library="EAGLE_chiefenne" package="SOCKED-08" value="DIL8S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="EAGLE_chiefenne" package="R1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="EAGLE_chiefenne" package="C1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="con-lsta" package="FE04-1Y" value="FE04-1Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="con-lsta" package="FE04-1Y" value="FE04-1Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="EAGLE_chiefenne" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="EAGLE_chiefenne" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="POWER">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="EAGLE_chiefenne" package="R1206" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="ATTINY-SOCKET" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="VCC"/>
<contactref element="JP3" pad="3"/>
<contactref element="P2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="ATTINY-SOCKET" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="P1" pad="4"/>
<contactref element="JP1" pad="RST"/>
</signal>
<signal name="GND">
<contactref element="ATTINY-SOCKET" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="GND"/>
<contactref element="JP3" pad="1"/>
<contactref element="P1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="ATTINY-SOCKET" pad="5"/>
<contactref element="JP2" pad="3"/>
<contactref element="P2" pad="4"/>
<contactref element="JP1" pad="MOSI"/>
</signal>
<signal name="N$4">
<contactref element="ATTINY-SOCKET" pad="6"/>
<contactref element="JP2" pad="2"/>
<contactref element="P2" pad="3"/>
<contactref element="JP1" pad="MISO"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="1"/>
<contactref element="ATTINY-SOCKET" pad="7"/>
<contactref element="P2" pad="2"/>
<contactref element="JP1" pad="SCK"/>
</signal>
<signal name="N$5">
<contactref element="P1" pad="2"/>
<contactref element="ATTINY-SOCKET" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="P1" pad="3"/>
<contactref element="ATTINY-SOCKET" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
