<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.915" y2="0" width="0" layer="20"/>
<wire x1="54.915" y1="0" x2="54.915" y2="40.63" width="0" layer="20"/>
<wire x1="54.915" y1="40.63" x2="0" y2="40.63" width="0" layer="20"/>
<wire x1="0" y1="40.63" x2="0" y2="0" width="0" layer="20"/>
<text>USB Joystick</text>
<text>Ver 1.0</text>
<text>NES</text>
<text>SNES</text>
<text>PS1A</text>
<text>PS1B</text>
<text>N64</text>
<text>USB</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-123">
<description>100V/150mA 1N4148 - Super Cheap</description>
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
<package name="1X04">
</package>
<package name="1X06">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="SO14">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STANDOFF-ELECTRICAL">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="LocalParts">
<packages>
<package name="ECS-160">
</package>
</packages>
</library>
<library name="linear-technology">
<description>&lt;b&gt;Linear Technology Devices&lt;/b&gt;&lt;p&gt;
http://www.linear-tech.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="20pf">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="20pf">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0805" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Passives" package="0805" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.6V">
<attribute name="PROD_ID" value="DIO-11284"/>
<attribute name="NAME"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-123" value="1N5819HW-7-F">
<attribute name="NAME"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.6V">
<attribute name="PROD_ID" value="DIO-11284"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK">
<attribute name="NAME"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="68">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="68">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="1.5k">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S3" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S4" library="SparkFun-Electromechanical" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="U2" library="SparkFun-DigitalIC" package="SO14" value="">
<attribute name="PROD_ID" value="IC-11329"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-PowerIC" package="SOT23-5" value="AP2202-ADJ">
<attribute name="PROD_ID" value="VREG-12189"/>
<attribute name="NAME"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0805" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="C9" library="SparkFun-Passives" package="0805" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="50k">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="50k">
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="50k">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="50k">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Passives" package="0805" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="C11" library="SparkFun-Passives" package="0805" value="100pf">
<attribute name="NAME"/>
</element>
<element name="C12" library="SparkFun-Passives" package="0805" value="10uf">
<attribute name="NAME"/>
</element>
<element name="C13" library="SparkFun-Passives" package="0805" value=".1uf">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0805" value="10uf">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Passives" package="0805" value="10uf">
<attribute name="NAME"/>
</element>
<element name="C14" library="SparkFun-Passives" package="0805" value="10uf">
<attribute name="NAME"/>
</element>
<element name="Y1" library="LocalParts" package="ECS-160" value="ECS-160">
<attribute name="NAME"/>
</element>
<element name="IC1" library="linear-technology" package="SOT223" value="">
<attribute name="OC_NEWARK" value="57M2069"/>
<attribute name="MPN" value="LT1129CST-5#PBF"/>
<attribute name="OC_FARNELL" value="1663375"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="NAME"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="NAME"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J13" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="J4" pad="4"/>
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="U2" pad="7"/>
<contactref element="J7" pad="3"/>
<contactref element="J7" pad="6"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="6"/>
<contactref element="J5" pad="4"/>
<contactref element="J6" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="J4" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="5V">
<contactref element="D2" pad="C"/>
<contactref element="R7" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J5" pad="3"/>
<contactref element="J6" pad="3"/>
<contactref element="U2" pad="14"/>
<contactref element="C8" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="J4" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="J4" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="RST">
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="29"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="ND0">
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="ND1">
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="6"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="ND2">
<contactref element="R4" pad="2"/>
<contactref element="J3" pad="4"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="ND3">
<contactref element="R5" pad="2"/>
<contactref element="J3" pad="5"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="5"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="D2">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="D7">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="PDAT">
<contactref element="R9" pad="2"/>
<contactref element="J5" pad="6"/>
<contactref element="J6" pad="6"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="PCLK">
<contactref element="J5" pad="1"/>
<contactref element="U1" pad="23"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="PCS1">
<contactref element="J5" pad="2"/>
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="3"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="PCS2">
<contactref element="J6" pad="2"/>
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="NCLK">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="2"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="NLAT">
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="3"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J7" pad="4"/>
<contactref element="U2" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N64D1">
<contactref element="J7" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N64D2">
<contactref element="J7" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="SP33A">
<contactref element="U2" pad="4"/>
<contactref element="R12" pad="1"/>
<contactref element="J12" pad="1"/>
</signal>
<signal name="SP33B">
<contactref element="U2" pad="5"/>
<contactref element="R13" pad="1"/>
<contactref element="J13" pad="1"/>
</signal>
<signal name="N64D1A">
<contactref element="U2" pad="13"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N64D1B">
<contactref element="U2" pad="12"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="SP5A">
<contactref element="U2" pad="11"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="SP5B">
<contactref element="U2" pad="10"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="4"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="PCMD">
<contactref element="J5" pad="5"/>
<contactref element="J6" pad="5"/>
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R15" pad="1"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="D5" pad="A"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="J8" pad="1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="22"/>
<contactref element="J9" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
