<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="86.03" x2="1.27" y2="2.54" width="0" layer="20"/>
<wire x1="1.27" y1="2.54" x2="3.81" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="0" x2="69.83" y2="0" width="0" layer="20"/>
<wire x1="69.83" y1="0" x2="72.37" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="72.37" y1="2.54" x2="72.37" y2="86.03" width="0" layer="20"/>
<wire x1="72.37" y1="86.03" x2="69.83" y2="89.205" width="0" layer="20" curve="90"/>
<wire x1="69.83" y1="89.205" x2="5.08" y2="89.205" width="0" layer="20"/>
<wire x1="5.08" y1="89.205" x2="1.27" y2="86.03" width="0" layer="20" curve="90"/>
<text>D0</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>3V3</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>DAC</text>
<text>WKP</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>5V</text>
<text>GND</text>
<text>VBAT</text>
<text>RST</text>
<text>3V3</text>
<text>5V</text>
<text>3V3</text>
<text>DCJACK</text>
<text>GND</text>
<text>POWER</text>
<text>3V3</text>
<text>5V</text>
<text>DCJACK</text>
<text>GND</text>
<text>POWER</text>
<text>Spies&amp;Assassins Photon Prototyping Board
ver. 1.00</text>
<text>GND</text>
<text>GND</text>
<text>OFF  ON</text>
</plain>
<libraries>
<library name="Spark">
<packages>
<package name="PHOTON">
</package>
<package name="1X12-SMALL-PADS">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SPRINGTERMINAL-17">
</package>
<package name="153CLV-0505">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1X04-CLEANBIG">
</package>
<package name="1X12-CB">
</package>
<package name="1X01-CLEANBIG">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SWITCH-SPST">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PTC-1206">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PHOTON" library="Spark" package="PHOTON" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="Spark" package="1X12-SMALL-PADS" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="Spark" package="1X12-SMALL-PADS" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="SPRINGTERMINAL-17" value="1X17-SPRINGTERMINAL"/>
<element name="Q2" library="adafruit" package="SPRINGTERMINAL-17" value="1X17-SPRINGTERMINAL"/>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="C1" library="adafruit" package="153CLV-0505" value="100uF/25V">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="153CLV-0505" value="10uF/10V">
<attribute name="NAME"/>
</element>
<element name="OFF---ON" library="SparkFun" package="SWITCH-SPST" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value=""/>
<element name="ON" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="330">
<attribute name="NAME"/>
</element>
<element name="DCJACK2" library="adafruit" package="DCJACK_2MM_PTH" value="DCJACK 7-20V">
<attribute name="VALUE"/>
</element>
<element name="F1" library="SparkFun-PowerIC" package="PTC-1206" value="250mA PTC"/>
<element name="JP19" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP20" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP21" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP22" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP23" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP24" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP25" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="adafruit" package="TO252" value="7805DT"/>
<element name="JP8" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP9" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP10" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN2" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="JP11" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP12" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="TX">
<contactref element="PHOTON" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q1" pad="3'"/>
</signal>
<signal name="RX">
<contactref element="PHOTON" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="Q1" pad="4"/>
<contactref element="Q1" pad="4'"/>
</signal>
<signal name="WKP">
<contactref element="PHOTON" pad="5"/>
<contactref element="JP1" pad="5"/>
<contactref element="Q1" pad="5"/>
<contactref element="Q1" pad="5'"/>
</signal>
<signal name="DAC">
<contactref element="PHOTON" pad="6"/>
<contactref element="JP1" pad="6"/>
<contactref element="Q1" pad="6"/>
<contactref element="Q1" pad="6'"/>
</signal>
<signal name="A5">
<contactref element="PHOTON" pad="7"/>
<contactref element="JP1" pad="7"/>
<contactref element="Q1" pad="7"/>
<contactref element="Q1" pad="7'"/>
</signal>
<signal name="A4">
<contactref element="PHOTON" pad="8"/>
<contactref element="JP1" pad="8"/>
<contactref element="Q1" pad="8"/>
<contactref element="Q1" pad="8'"/>
</signal>
<signal name="A3">
<contactref element="PHOTON" pad="9"/>
<contactref element="JP1" pad="9"/>
<contactref element="Q1" pad="9"/>
<contactref element="Q1" pad="9'"/>
</signal>
<signal name="A2">
<contactref element="PHOTON" pad="10"/>
<contactref element="JP1" pad="10"/>
<contactref element="Q1" pad="10"/>
<contactref element="Q1" pad="10'"/>
</signal>
<signal name="A1">
<contactref element="PHOTON" pad="11"/>
<contactref element="JP1" pad="11"/>
<contactref element="Q1" pad="11"/>
<contactref element="Q1" pad="11'"/>
</signal>
<signal name="A0">
<contactref element="PHOTON" pad="12"/>
<contactref element="JP1" pad="12"/>
<contactref element="Q1" pad="12"/>
<contactref element="Q1" pad="12'"/>
</signal>
<signal name="GND">
<contactref element="PHOTON" pad="2"/>
<contactref element="PHOTON" pad="21"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="Q2" pad="14"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="16"/>
<contactref element="Q1" pad="17"/>
<contactref element="Q1" pad="2"/>
<contactref element="DCJACK2" pad="GND"/>
<contactref element="DCJACK2" pad="GNDBREAK"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="Q1" pad="16'"/>
<contactref element="Q1" pad="17'"/>
<contactref element="Q1" pad="2'"/>
<contactref element="Q2" pad="1'"/>
<contactref element="Q2" pad="2'"/>
<contactref element="Q2" pad="14'"/>
<contactref element="CN2" pad="4"/>
<contactref element="CN1" pad="4"/>
<contactref element="JP12" pad="1"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="RST">
<contactref element="PHOTON" pad="23"/>
<contactref element="JP2" pad="2"/>
<contactref element="Q2" pad="16"/>
<contactref element="Q2" pad="16'"/>
</signal>
<signal name="D7">
<contactref element="PHOTON" pad="20"/>
<contactref element="JP2" pad="5"/>
<contactref element="Q2" pad="13"/>
<contactref element="Q2" pad="13'"/>
</signal>
<signal name="D6">
<contactref element="PHOTON" pad="19"/>
<contactref element="JP2" pad="6"/>
<contactref element="Q2" pad="12"/>
<contactref element="Q2" pad="12'"/>
</signal>
<signal name="D5">
<contactref element="PHOTON" pad="18"/>
<contactref element="JP2" pad="7"/>
<contactref element="Q2" pad="11"/>
<contactref element="Q2" pad="11'"/>
</signal>
<signal name="D4">
<contactref element="PHOTON" pad="17"/>
<contactref element="JP2" pad="8"/>
<contactref element="Q2" pad="10"/>
<contactref element="Q2" pad="10'"/>
</signal>
<signal name="D3">
<contactref element="PHOTON" pad="16"/>
<contactref element="JP2" pad="9"/>
<contactref element="Q2" pad="9"/>
<contactref element="Q2" pad="9'"/>
</signal>
<signal name="D2">
<contactref element="PHOTON" pad="15"/>
<contactref element="JP2" pad="10"/>
<contactref element="Q2" pad="8"/>
<contactref element="Q2" pad="8'"/>
</signal>
<signal name="D1">
<contactref element="PHOTON" pad="14"/>
<contactref element="JP2" pad="11"/>
<contactref element="Q2" pad="7"/>
<contactref element="Q2" pad="7'"/>
</signal>
<signal name="D0">
<contactref element="PHOTON" pad="13"/>
<contactref element="JP2" pad="12"/>
<contactref element="Q2" pad="6"/>
<contactref element="Q2" pad="6'"/>
</signal>
<signal name="VBAT">
<contactref element="PHOTON" pad="22"/>
<contactref element="JP2" pad="3"/>
<contactref element="Q2" pad="15"/>
<contactref element="Q2" pad="15'"/>
</signal>
<signal name="3V3">
<contactref element="PHOTON" pad="24"/>
<contactref element="JP2" pad="1"/>
<contactref element="Q2" pad="5"/>
<contactref element="Q2" pad="4"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q2" pad="17"/>
<contactref element="Q2" pad="5'"/>
<contactref element="Q2" pad="4'"/>
<contactref element="Q2" pad="3'"/>
<contactref element="Q2" pad="17'"/>
<contactref element="CN1" pad="1"/>
<contactref element="CN2" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="PHOTON" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="13"/>
<contactref element="Q1" pad="14"/>
<contactref element="Q1" pad="15"/>
<contactref element="C2" pad="+"/>
<contactref element="ON" pad="A"/>
<contactref element="IC1" pad="2"/>
<contactref element="Q1" pad="13'"/>
<contactref element="Q1" pad="14'"/>
<contactref element="Q1" pad="15'"/>
<contactref element="Q1" pad="1'"/>
<contactref element="CN1" pad="2"/>
<contactref element="CN2" pad="2"/>
</signal>
<signal name="9V2">
<contactref element="C1" pad="+"/>
<contactref element="OFF---ON" pad="3"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="OFF---ON" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="ON" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="D1" pad="A"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="9V">
<contactref element="F1" pad="1"/>
<contactref element="DCJACK2" pad="PWR"/>
<contactref element="CN1" pad="3"/>
<contactref element="CN2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
