<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="-1.75" y1="-0.75" x2="11.75" y2="-0.75" width="0" layer="20"/>
<wire x1="11.75" y1="-0.75" x2="11.75" y2="17.4" width="0" layer="20"/>
<wire x1="-1.75" y1="17.4" x2="-1.75" y2="-0.75" width="0" layer="20"/>
<text>Stepper Splitter</text>
<text>Stepper Splitter</text>
<text>Input</text>
<wire x1="-1.75" y1="17.4" x2="11.75" y2="17.4" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP6" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
</elements>
<signals>
<signal name="2B1M">
<contactref element="JP6" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="2A1M">
<contactref element="JP6" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="1A1M">
<contactref element="JP6" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="1B1M">
<contactref element="JP6" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
