<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="63.48" y2="0" width="0" layer="20"/>
<wire x1="63.48" y1="0" x2="63.48" y2="50.851" width="0" layer="20"/>
<wire x1="63.48" y1="50.851" x2="0" y2="50.851" width="0" layer="20"/>
<wire x1="0" y1="50.851" x2="0" y2="0" width="0" layer="20"/>
<text>SSTX+</text>
<text>SSTX-</text>
<text>DRAIN</text>
<text>SSRX-</text>
<text>SSRX+</text>
<text>VCC</text>
<text>D-</text>
<text>D+</text>
<text>GND</text>
<text>SHLD</text>
<text>+5VDC</text>
<text>GND</text>
<text>GND</text>
<text>SHLD</text>
<text>+12VDC</text>
<text>REV-A</text>
<text>Eric Martin</text>
<text>Tolerable
Endcap
Adapter</text>
</plain>
<libraries>
<library name="2355181-5">
<packages>
<package name="TE_2355181-5">
</package>
</packages>
</library>
<library name="mill-max">
<packages>
<package name="MILL_MAX_SERIES_858_5PIN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="2355181-5" package="TE_2355181-5" value="2355181-5">
<attribute name="COMMENT" value="2355181-5"/>
<attribute name="DESCRIPTION" value=" Pin 5P,2MM,BRK HDR,SRVT,2.8,0.38AU,BOX 5 POS "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="17-2355181-5-ND"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="2355181-5"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="J2" library="2355181-5" package="TE_2355181-5" value="2355181-5">
<attribute name="COMMENT" value="2355181-5"/>
<attribute name="DESCRIPTION" value=" Pin 5P,2MM,BRK HDR,SRVT,2.8,0.38AU,BOX 5 POS "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="17-2355181-5-ND"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="2355181-5"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="J3" library="2355181-5" package="TE_2355181-5" value="2355181-5">
<attribute name="COMMENT" value="2355181-5"/>
<attribute name="DESCRIPTION" value=" Pin 5P,2MM,BRK HDR,SRVT,2.8,0.38AU,BOX 5 POS "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="17-2355181-5-ND"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="2355181-5"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="J4" library="2355181-5" package="TE_2355181-5" value="2355181-5">
<attribute name="COMMENT" value="2355181-5"/>
<attribute name="DESCRIPTION" value=" Pin 5P,2MM,BRK HDR,SRVT,2.8,0.38AU,BOX 5 POS "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="17-2355181-5-ND"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="2355181-5"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="MILL-MAX1" library="mill-max" package="MILL_MAX_SERIES_858_5PIN" value="MILL_MAX_SERIES_858_5PIN"/>
<element name="MILL-MAX2" library="mill-max" package="MILL_MAX_SERIES_858_5PIN" value="MILL_MAX_SERIES_858_5PIN"/>
<element name="MILL-MAX3" library="mill-max" package="MILL_MAX_SERIES_858_5PIN" value="MILL_MAX_SERIES_858_5PIN"/>
</elements>
<signals>
<signal name="GND_DRN">
<contactref element="MILL-MAX2" pad="P$3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="MILL-MAX1" pad="P$5"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="MILL-MAX1" pad="P$4"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="3"/>
<contactref element="MILL-MAX1" pad="P$3"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="4"/>
<contactref element="MILL-MAX1" pad="P$2"/>
<contactref element="J3" pad="4"/>
<contactref element="MILL-MAX3" pad="P$2"/>
<contactref element="J4" pad="4"/>
<contactref element="J3" pad="2"/>
<contactref element="MILL-MAX3" pad="P$4"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="SHLD">
<contactref element="J1" pad="5"/>
<contactref element="MILL-MAX1" pad="P$1"/>
<contactref element="J3" pad="3"/>
<contactref element="MILL-MAX3" pad="P$3"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="1"/>
<contactref element="MILL-MAX2" pad="P$5"/>
</signal>
<signal name="N$7">
<contactref element="J2" pad="2"/>
<contactref element="MILL-MAX2" pad="P$4"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="4"/>
<contactref element="MILL-MAX2" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="5"/>
<contactref element="MILL-MAX2" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="J3" pad="1"/>
<contactref element="MILL-MAX3" pad="P$5"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="J3" pad="5"/>
<contactref element="MILL-MAX3" pad="P$1"/>
<contactref element="J4" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
