<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="7.62" y1="0" x2="47.93" y2="0" width="0" layer="20"/>
<wire x1="47.93" y1="0" x2="47.93" y2="27.93" width="0" layer="20"/>
<wire x1="47.93" y1="27.93" x2="7.62" y2="27.93" width="0" layer="20"/>
<wire x1="7.62" y1="27.93" x2="7.62" y2="0" width="0" layer="20"/>
<text>&lt;-USB</text>
<text>5v</text>
<text>3V3</text>
<text>FINGAZ</text>
<text>PWMer v1</text>
<text>WeMos D1 Mini v2</text>
</plain>
<libraries>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE08">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="TO229P990X238-4N">
<description>&lt;b&gt;DPAK-3&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV1" library="con-lsta" package="FE08" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV2" library="con-lsta" package="FE08" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SamacSys_Parts" package="TO229P990X238-4N" value="NCP1117DT50G">
<attribute name="DESCRIPTION" value="NCP1117DT50G, Low Dropout Voltage Regulator, 1A, 5 V 1%, 3-Pin DPAK"/>
<attribute name="HEIGHT" value="2.38mm"/>
<attribute name="MANUFACTURER_NAME" value="ON Semiconductor"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="NCP1117DT50G"/>
<attribute name="MOUSER_PART_NUMBER" value="863-NCP1117DT50G"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="eagle-ltspice" package="C1206" value="10uF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="eagle-ltspice" package="C1206" value="10uF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO220V" value="FQP30N06L">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="eagle-ltspice" package="0207/10" value="1k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle-ltspice" package="0207/10" value="1k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="LED-" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED+" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="12V" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$4">
<contactref element="SV2" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="SV2" pad="8"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="LED+" pad="1"/>
<contactref element="12V" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="2"/>
<contactref element="LED-" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="GND" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="SV2" pad="7"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
