<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="63.5" y1="0.9773" x2="63.5" y2="110.624990625" width="0.025" layer="20"/>
<wire x1="63.5" y1="110.624990625" x2="10.231490625" y2="110.624990625" width="0.025" layer="20"/>
<wire x1="10.231490625" y1="110.624990625" x2="10.231490625" y2="105.839140625" width="0.025" layer="20"/>
<wire x1="10.231490625" y1="105.839140625" x2="4.722340625" y2="100.33" width="0.025" layer="20" curve="-90"/>
<wire x1="4.722340625" y1="100.33" x2="0" y2="100.33" width="0.025" layer="20"/>
<wire x1="0" y1="100.33" x2="0" y2="11.272290625" width="0.025" layer="20"/>
<wire x1="0" y1="11.272290625" x2="4.722340625" y2="11.272290625" width="0.025" layer="20"/>
<wire x1="4.722340625" y1="11.272290625" x2="10.231490625" y2="5.763140625" width="0.025" layer="20" curve="-90"/>
<wire x1="10.231490625" y1="5.763140625" x2="10.231490625" y2="0.9773" width="0.025" layer="20"/>
<wire x1="10.231490625" y1="0.9773" x2="63.5" y2="0.9773" width="0.025" layer="20"/>
<circle x="55.245" y="9.2323" radius="1.5875" width="0.025" layer="20"/>
<circle x="55.245" y="102.369990625" radius="1.5875" width="0.025" layer="20"/>
<circle x="13.358340625" y="14.462640625" radius="1.5875" width="0.025" layer="20"/>
<circle x="13.358340625" y="97.139640625" radius="1.5875" width="0.025" layer="20"/>
<text>CH1</text>
<text>CH2</text>
<text>CH3</text>
<text>CH4</text>
<text>CH5</text>
<text>BOWNET MK7 RX
9/24/17
DESIGNED IN WASHINGTON STATE, USA</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MINI">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
</package>
</packages>
</library>
<library name="NCP1117">
<packages>
<package name="DPAK-3">
<description>&lt;b&gt;DPAK-3&lt;/b&gt; (acc. to. ON Semiconductor specs)</description>
</package>
</packages>
</library>
<library name="con-jst2">
<description>&lt;b&gt;J.S.T. Connectors&lt;/b&gt;&lt;p&gt;
J.S.T Mfg Co.,Ltd.&lt;p&gt;
http://www.jst-mfg.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM08B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, side entry type&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="IGBT">
<description>IGBT Transistor</description>
<packages>
<package name="TO252_STM">
<description>TO-252 (DPAK) by STMicroelectronics</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
<library name="LOCKNOSILK">
<packages>
<package name="1X05_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="1.2k"/>
<element name="U$1" library="SparkFun-Boards" package="ARDUINO_MINI" value="ARDUINO_MINI"/>
<element name="U$2" library="SparkFun-Connectors" package="2X4" value="M04X2"/>
<element name="U$3" library="NCP1117" package="DPAK-3" value="NCP1117"/>
<element name="X1" library="con-jst2" package="SM08B-SRSS-TB" value="SM08B-SRSS-TB"/>
<element name="Q1" library="IGBT" package="TO252_STM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="1206" value="10k"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value=""/>
<element name="D2" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value=""/>
<element name="CHANNEL" library="LOCKNOSILK" package="1X05_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SELECT" library="LOCKNOSILK" package="1X05_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="8"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="4"/>
<contactref element="X1" pad="1"/>
<contactref element="X1" pad="8"/>
<contactref element="U$3" pad="1"/>
<contactref element="C2" pad="C"/>
<contactref element="C1" pad="C"/>
<contactref element="Q1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="SELECT" pad="1"/>
<contactref element="SELECT" pad="2"/>
<contactref element="SELECT" pad="3"/>
<contactref element="SELECT" pad="4"/>
<contactref element="SELECT" pad="5"/>
</signal>
<signal name="INPUT">
<contactref element="U$1" pad="24"/>
<contactref element="U$3" pad="3"/>
<contactref element="C1" pad="A"/>
<contactref element="X1" pad="4"/>
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="IRQ">
<contactref element="U$2" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="CSN">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="CE">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="3V">
<contactref element="U$2" pad="7"/>
<contactref element="U$3" pad="4"/>
<contactref element="C2" pad="A"/>
</signal>
<signal name="LED">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="TRANIN">
<contactref element="X1" pad="3"/>
<contactref element="Q1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="21"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="6"/>
<contactref element="X1" pad="7"/>
</signal>
<signal name="SOL">
<contactref element="U$1" pad="5"/>
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="BAT">
<contactref element="D2" pad="A"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="CH1">
<contactref element="U$1" pad="6"/>
<contactref element="CHANNEL" pad="1"/>
</signal>
<signal name="CH2">
<contactref element="U$1" pad="7"/>
<contactref element="CHANNEL" pad="2"/>
</signal>
<signal name="CH3">
<contactref element="U$1" pad="8"/>
<contactref element="CHANNEL" pad="3"/>
</signal>
<signal name="CH4">
<contactref element="U$1" pad="9"/>
<contactref element="CHANNEL" pad="4"/>
</signal>
<signal name="CH5">
<contactref element="U$1" pad="10"/>
<contactref element="CHANNEL" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
