<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="11.1" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="26.65" y2="0" width="0" layer="20"/>
<wire x1="26.65" y1="0" x2="27.92" y2="1.27" width="0" layer="20"/>
<wire x1="27.92" y1="1.27" x2="27.92" y2="12.37" width="0" layer="20"/>
<wire x1="27.92" y1="12.37" x2="26.65" y2="13.64" width="0" layer="20"/>
<wire x1="26.65" y1="13.64" x2="2.54" y2="13.64" width="0" layer="20"/>
<wire x1="2.54" y1="13.64" x2="0" y2="11.1" width="0" layer="20"/>
<wire x1="2.54" y1="13.589" x2="26.67" y2="13.589" width="0.3048" layer="46"/>
<wire x1="26.67" y1="13.589" x2="27.94" y2="12.319" width="0.3048" layer="46"/>
<wire x1="27.94" y1="12.319" x2="27.94" y2="1.27" width="0.3048" layer="46"/>
<wire x1="27.94" y1="1.27" x2="26.67" y2="0" width="0.3048" layer="46"/>
<wire x1="26.67" y1="0" x2="2.54" y2="0" width="0.3048" layer="46"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0.3048" layer="46"/>
<wire x1="0" y1="2.54" x2="0" y2="11.049" width="0.3048" layer="46"/>
<wire x1="0" y1="11.049" x2="2.54" y2="13.589" width="0.3048" layer="46"/>
</plain>
<libraries>
<library name="MF_Connectors">
<packages>
<package name="TC2050-IDC-NL">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for Tag Connect TC2050-NL style&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="con-leotronics">
<description>&lt;b&gt;Connectors from Leotronics&lt;/b&gt;&lt;p&gt;
www.leotronics.co.uk&lt;br&gt;</description>
<packages>
<package name="1365-10">
<description>&lt;b&gt;DUAL ROW STRAIGHT HEADER&lt;/b&gt; 1364 SERIES. 1.27mm x 1.27mm. Without Fixing Post. SMT&lt;p&gt;
Source: http://www.leotronics.co.uk/Conexcon/Data%20Sheets/sec.%20A/1364ing.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="con-leotronics" package="1365-10" value="1365-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="TAG-CONNECT" library="MF_Connectors" package="TC2050-IDC-NL" value="TC2050-IDC-NL">
<attribute name="HOUSEPART" value="NO"/>
<attribute name="LABEL01" value=""/>
<attribute name="LABEL02" value=""/>
<attribute name="LABEL03" value=""/>
<attribute name="LABEL04" value=""/>
<attribute name="LABEL05" value=""/>
<attribute name="LABEL06" value=""/>
<attribute name="LABEL07" value=""/>
<attribute name="LABEL08" value=""/>
<attribute name="LABEL09" value=""/>
<attribute name="LABEL10" value=""/>
<attribute name="MPN" value="TC2050-IDC-NL"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
<attribute name="URL" value="http://www.tag-connect.com/Materials/TC2050-IDC-NL%20Datasheet.pdf"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="TAG-CONNECT" pad="P$5"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="9"/>
</signal>
<signal name="SWCLK">
<contactref element="TAG-CONNECT" pad="P$4"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="SWDIO">
<contactref element="TAG-CONNECT" pad="P$2"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="TAG-CONNECT" pad="P$1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="TAG-CONNECT" pad="P$10"/>
<contactref element="X1" pad="10"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
