<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="26.416" x2="53.518" y2="26.416" width="0" layer="20"/>
<wire x1="53.518" y1="26.416" x2="53.518" y2="80" width="0" layer="20"/>
<wire x1="53.518" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="26.416" width="0" layer="20"/>
<text>pout</text>
<text>gnd</text>
<text>gnd</text>
<text>gnd</text>
<text>5v</text>
<text>5v</text>
<text>5v</text>
<text>5v</text>
<text>gnd</text>
<text>Vin</text>
<text>EN</text>
<text>sig</text>
<text>sig</text>
<text>sig</text>
<text>&lt;3 -Swiss</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LONGPADS">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1X01_LONGPAD">
</package>
<package name="1X05_LONGPADS">
</package>
<package name="POWER_JACK_PTH_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DOWN" library="SparkFun-Connectors" package="1X03_LONGPADS" value=""/>
<element name="J1" library="SparkFun-Boards" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="POUT" library="SparkFun-Connectors" package="1X02_LONGPADS" value=""/>
<element name="SERVO" library="SparkFun-Connectors" package="1X03_LONGPADS" value=""/>
<element name="SIG" library="SparkFun-Connectors" package="1X01_LONGPAD" value=""/>
<element name="UP" library="SparkFun-Connectors" package="1X03_LONGPADS" value=""/>
<element name="VREG" library="SparkFun-Connectors" package="1X05_LONGPADS" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="POWER_JACK_PTH_LOCK" value="POWER_JACKPTH_LOCK">
<attribute name="PROD_ID" value="CONN-08197"/>
<attribute name="SF_ID" value="PRT-00119"/>
</element>
</elements>
<signals>
<signal name="A0">
<contactref element="SIG" pad="1"/>
<contactref element="J1" pad="A0"/>
</signal>
<signal name="5V">
<contactref element="VREG" pad="1"/>
<contactref element="UP" pad="1"/>
<contactref element="DOWN" pad="1"/>
<contactref element="SERVO" pad="2"/>
<contactref element="J1" pad="5V"/>
</signal>
<signal name="GND">
<contactref element="VREG" pad="2"/>
<contactref element="VREG" pad="3"/>
<contactref element="UP" pad="3"/>
<contactref element="DOWN" pad="3"/>
<contactref element="SERVO" pad="3"/>
<contactref element="POUT" pad="2"/>
<contactref element="J1" pad="GND@2"/>
<contactref element="J1" pad="GND@0"/>
<contactref element="J1" pad="GND@1"/>
<contactref element="JP1" pad="GNDBREAK"/>
<contactref element="JP1" pad="GND"/>
</signal>
<signal name="VIN">
<contactref element="VREG" pad="4"/>
<contactref element="POUT" pad="1"/>
<contactref element="JP1" pad="PWR"/>
</signal>
<signal name="NC">
<contactref element="VREG" pad="5"/>
</signal>
<signal name="A5">
<contactref element="UP" pad="2"/>
<contactref element="J1" pad="A5"/>
</signal>
<signal name="A4">
<contactref element="DOWN" pad="2"/>
<contactref element="J1" pad="A4"/>
</signal>
<signal name="A1">
<contactref element="SERVO" pad="1"/>
<contactref element="J1" pad="A1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
