<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="8.255" y1="0" x2="8.255" y2="8.8775" width="0" layer="20"/>
<wire x1="8.255" y1="8.8775" x2="0.01" y2="8.8775" width="0" layer="20"/>
<wire x1="0.01" y1="8.8775" x2="0.01" y2="0" width="0" layer="20"/>
<wire x1="0.01" y1="0" x2="8.255" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X03_LOCK_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="MIDDLE">
<contactref element="Q1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="LEFT">
<contactref element="J1" pad="3"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="RIGHT">
<contactref element="J1" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
