<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="7.62" x2="0" y2="55.88" width="0.4064" layer="20"/>
<wire x1="0" y1="55.88" x2="1.27" y2="57.15" width="0.4064" layer="20"/>
<wire x1="53.34" y1="57.15" x2="53.34" y2="7.62" width="0.4064" layer="20"/>
<wire x1="1.27" y1="57.15" x2="53.34" y2="57.15" width="0.4064" layer="20"/>
<wire x1="0" y1="7.62" x2="53.34" y2="7.62" width="0.4064" layer="20"/>
<text>In from
Presort</text>
<text>Out to
wireless</text>
<text>Oregon Beverage Recycling Coop
Presort serial-ethernet interface
Rev 1.0  May 2014</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="DB9_MALE">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Boards" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="COM1_IN" library="SparkFun-Connectors" package="DB9" value="COM1_IN"/>
<element name="COM2_OUT" library="SparkFun-Connectors" package="DB9_MALE" value="COM2_OUT"/>
<element name="LED1" library="SparkFun-LED" package="LED5MM" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED5MM" value="BLUE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="330"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="330"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND@2"/>
<contactref element="U$1" pad="GND@1"/>
<contactref element="U$1" pad="GND@0"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="COM2_OUT" pad="5"/>
<contactref element="COM1_IN" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="D13"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="K"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="D12"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="RX"/>
<contactref element="COM1_IN" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="COM1_IN" pad="3"/>
<contactref element="U$1" pad="TX"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="D2"/>
<contactref element="COM2_OUT" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="COM2_OUT" pad="3"/>
<contactref element="U$1" pad="D3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
